<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="53.01" y2="0" width="0" layer="20"/>
<wire x1="53.01" y1="0" x2="53.01" y2="59.68" width="0" layer="20"/>
<wire x1="53.01" y1="59.68" x2="0" y2="59.68" width="0" layer="20"/>
<wire x1="0" y1="59.68" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X04-3.5MM">
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="1X2-3.5MM">
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="G5LE">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 10 A/120 V AC, 8 A/30 V ADC, Omron</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CN2" library="adafruit" package="1X04-3.5MM" value="1X4-3.5MM"/>
<element name="D1" library="adafruit" package="DO41-10" value="1N4004"/>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="J2" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="K1" library="relay" package="G5LE" value="G5LE">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="T2" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="T3" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="T3" pad="C"/>
<contactref element="D1" pad="A"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="T2" pad="B"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="T1" pad="B"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="D11"/>
</signal>
<signal name="N$8">
<contactref element="D1" pad="C"/>
<contactref element="K1" pad="2"/>
<contactref element="J2" pad="5V"/>
</signal>
<signal name="N$7">
<contactref element="K1" pad="P"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="1"/>
<contactref element="K1" pad="S"/>
</signal>
<signal name="N$10">
<contactref element="CN2" pad="4"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="CN2" pad="3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="T3" pad="B"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="T2" pad="C"/>
<contactref element="J2" pad="D7"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="D4"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="P$2"/>
<contactref element="J2" pad="D9"/>
</signal>
<signal name="GND-ISO">
<contactref element="T3" pad="E"/>
<contactref element="CN2" pad="1"/>
<contactref element="CN2" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="T2" pad="E"/>
<contactref element="J2" pad="GND@2"/>
<contactref element="J2" pad="GND@1"/>
<contactref element="J2" pad="GND@0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
