<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>https://dcdark.net</text>
<text>Assembly No:
DN-IR-6B 7 3 3
Rev 1.12.35</text>
<text>ICSP</text>
<text>FTDI</text>
<wire x1="43.815" y1="68.58" x2="85.725" y2="68.58" width="0" layer="20" curve="-50"/>
<wire x1="43.815" y1="37.465" x2="43.815" y2="3.81" width="0" layer="20" curve="-30"/>
<wire x1="85.725" y1="3.81" x2="85.725" y2="37.465" width="0" layer="20" curve="-30"/>
<wire x1="43.815" y1="68.58" x2="45.085" y2="57.15" width="0" layer="20" curve="-25"/>
<wire x1="85.725" y1="68.58" x2="84.455" y2="57.15" width="0" layer="20" curve="25"/>
<wire x1="50.8" y1="-2.54" x2="50.8" y2="3.81" width="0" layer="20"/>
<wire x1="50.8" y1="3.81" x2="78.105" y2="3.81" width="0" layer="20"/>
<wire x1="78.105" y1="3.81" x2="78.105" y2="-2.54" width="0" layer="20"/>
<wire x1="50.8" y1="-2.54" x2="43.815" y2="3.81" width="0" layer="20" curve="-20"/>
<wire x1="85.725" y1="3.81" x2="78.105" y2="-2.54" width="0" layer="20" curve="-20"/>
<wire x1="43.18" y1="54.61" x2="45.085" y2="57.15" width="0" layer="20" curve="-10"/>
<wire x1="84.455" y1="57.15" x2="86.36" y2="54.61" width="0" layer="20" curve="-10"/>
<wire x1="43.18" y1="54.61" x2="43.815" y2="37.465" width="0" layer="20"/>
<wire x1="86.36" y1="54.61" x2="85.725" y2="37.465" width="0" layer="20"/>
<text>BLK</text>
<text>GRN</text>
<text>USB Tx</text>
<text>FFADGFFDGGXA
GXADGXFXGXGX
XGAADDFXDFAX
GGFAGGDGXDGA
XAFDGDFDGFFA
GAXAFGFFGGGD
GGXAGAAAGADN
</text>
<text>42888609513
62573257526
47187425975</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FTDI_BASIC">
</package>
<package name="DIODE-ZENER">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="LED-1206">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="CERM_OSC">
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="1X1-SMALL">
</package>
</packages>
</library>
<library name="SYNShop">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="TACTILE-2PIN">
</package>
<package name="AXIAL-0.3">
</package>
<package name="AVRISP">
</package>
<package name="3-AAA-CELL_NOBORDER">
</package>
<package name="IR-MODULE">
</package>
<package name="KRUX_LOGO">
</package>
<package name="DN_LOGO">
</package>
<package name="TO262-H">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SYNShop" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SYNShop" package="AXIAL-0.3" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SYNShop" package="AXIAL-0.3" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="FTDI_BASIC" value="FTDI_BASICPTH"/>
<element name="LED1" library="SYNShop" package="LED5MM" value="XMT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SYNShop" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SYNShop" package="TACTILE-2PIN" value="Reset">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SYNShop" package="AVRISP" value="JP1"/>
<element name="IC1" library="adafruit" package="DIL28-3" value="ATMEGA328P-PU">
<attribute name="VALUE"/>
</element>
<element name="XTAL" library="adafruit" package="CERM_OSC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SYNShop" package="AXIAL-0.3" value="68">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SYNShop" package="AXIAL-0.3" value="68">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SYNShop" package="AXIAL-0.3" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C025-030X050" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C025-030X050" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun" package="DIODE-ZENER" value="3.6V Zener">
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun" package="DIODE-ZENER" value="3.6V Zener">
<attribute name="NAME"/>
</element>
<element name="X2" library="SparkFun" package="USB-B-PTH" value="USB">
<attribute name="VALUE"/>
</element>
<element name="U$5" library="SYNShop" package="3-AAA-CELL_NOBORDER" value="12BH423-GR3-CELL_NOBORDER"/>
<element name="U1" library="SYNShop" package="IR-MODULE" value="RCV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="SYNShop" package="TACTILE-2PIN" value="">
<attribute name="NAME"/>
</element>
<element name="JP3" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP4" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP5" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP6" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP7" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP8" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP9" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP10" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP11" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP12" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP13" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP14" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP15" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP16" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP17" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP18" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP19" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP20" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP21" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP22" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP23" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP24" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP25" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP26" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP27" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP28" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP29" library="adafruit" package="1X1-SMALL" value=""/>
<element name="JP30" library="adafruit" package="1X1-SMALL" value=""/>
<element name="U$7" library="SYNShop" package="KRUX_LOGO" value="KRUX_LOGO"/>
<element name="C3" library="adafruit" package="C025-030X050" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="LED3" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SYNShop" package="DN_LOGO" value="DN_LOGO"/>
<element name="U2" library="SYNShop" package="TO262-H" value="VT1045CTO262-H">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="PIN17">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="17"/>
<contactref element="JP19" pad="P$1"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="PIN6">
<contactref element="IC1" pad="6"/>
<contactref element="JP8" pad="P$1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="PIN19">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="19"/>
<contactref element="JP21" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="JP2" pad="GND"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="XTAL" pad="P$2"/>
<contactref element="IC1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="D1" pad="P$2"/>
<contactref element="D2" pad="P$2"/>
<contactref element="X2" pad="GND"/>
<contactref element="U$5" pad="-V"/>
<contactref element="U1" pad="3"/>
<contactref element="SW1" pad="P$1"/>
<contactref element="JP10" pad="P$1"/>
<contactref element="R7" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="R2" pad="P$2"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="JP9" pad="P$1"/>
<contactref element="JP22" pad="P$1"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="PIN1">
<contactref element="R2" pad="P$1"/>
<contactref element="RESET" pad="P$1"/>
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="P$1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="P$1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="+5V">
<contactref element="JP2" pad="VCC"/>
<contactref element="X2" pad="VBUS"/>
<contactref element="JP1" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$5" pad="+V"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$16">
</signal>
<signal name="PIN18">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="18"/>
<contactref element="JP20" pad="P$1"/>
<contactref element="SW1" pad="P$2"/>
</signal>
<signal name="PIN9">
<contactref element="XTAL" pad="P$1"/>
<contactref element="IC1" pad="9"/>
<contactref element="JP11" pad="P$1"/>
</signal>
<signal name="PIN10">
<contactref element="IC1" pad="10"/>
<contactref element="XTAL" pad="P$3"/>
<contactref element="JP12" pad="P$1"/>
</signal>
<signal name="PIN5">
<contactref element="R1" pad="P$2"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP7" pad="P$1"/>
</signal>
<signal name="PIN12">
<contactref element="IC1" pad="12"/>
<contactref element="JP14" pad="P$1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="PIN13">
<contactref element="IC1" pad="13"/>
<contactref element="JP15" pad="P$1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="P$1"/>
<contactref element="D2" pad="P$1"/>
<contactref element="X2" pad="D+"/>
</signal>
<signal name="USB">
<contactref element="R5" pad="P$1"/>
<contactref element="D1" pad="P$1"/>
<contactref element="X2" pad="D-"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="PIN4">
<contactref element="IC1" pad="4"/>
<contactref element="JP6" pad="P$1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="PIN3">
<contactref element="IC1" pad="3"/>
<contactref element="JP2" pad="RXI"/>
<contactref element="JP5" pad="P$1"/>
</signal>
<signal name="PIN2">
<contactref element="JP2" pad="TXO"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP4" pad="P$1"/>
</signal>
<signal name="PIN11">
<contactref element="IC1" pad="11"/>
<contactref element="JP13" pad="P$1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="PIN16">
<contactref element="IC1" pad="16"/>
<contactref element="JP18" pad="P$1"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="PIN15">
<contactref element="IC1" pad="15"/>
<contactref element="JP17" pad="P$1"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="PIN22">
<contactref element="IC1" pad="22"/>
<contactref element="JP24" pad="P$1"/>
</signal>
<signal name="PIN21">
<contactref element="IC1" pad="21"/>
<contactref element="JP23" pad="P$1"/>
</signal>
<signal name="PIN23">
<contactref element="IC1" pad="23"/>
<contactref element="JP25" pad="P$1"/>
</signal>
<signal name="PIN24">
<contactref element="IC1" pad="24"/>
<contactref element="JP26" pad="P$1"/>
</signal>
<signal name="PIN25">
<contactref element="IC1" pad="25"/>
<contactref element="JP27" pad="P$1"/>
</signal>
<signal name="PIN26">
<contactref element="IC1" pad="26"/>
<contactref element="JP28" pad="P$1"/>
</signal>
<signal name="PIN27">
<contactref element="IC1" pad="27"/>
<contactref element="JP29" pad="P$1"/>
</signal>
<signal name="PIN28">
<contactref element="IC1" pad="28"/>
<contactref element="JP30" pad="P$1"/>
</signal>
<signal name="PIN14">
<contactref element="IC1" pad="14"/>
<contactref element="JP16" pad="P$1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="DTR"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$24">
</signal>
<signal name="N$6">
</signal>
<signal name="N$2">
<contactref element="R7" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="LED4" pad="C"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R9" pad="2"/>
<contactref element="LED5" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="LED6" pad="C"/>
<contactref element="R10" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
