<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="63.5" width="0.254" layer="20"/>
<wire x1="0" y1="63.5" x2="66.04" y2="63.5" width="0.254" layer="20"/>
<wire x1="66.04" y1="63.5" x2="66.04" y2="0" width="0.254" layer="20"/>
<wire x1="66.04" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>HACKHD1</text>
<text>HACKHD2</text>
<text>HACKHD3</text>
<text>HACKHD4</text>
<text>HACKHD5</text>
<text>HACKHD6</text>
<text>RX2</text>
<text>RX3</text>
<hole x="18.542" y="5.2578" drill="3.2"/>
<hole x="18.5293" y="58.2168" drill="3.2"/>
<hole x="47.5361" y="58.2676" drill="3.2"/>
<hole x="47.4853" y="5.2451" drill="3.2"/>
<text>STATUS</text>
<text>S:1</text>
<text>S:2</text>
<text>S:3</text>
<text>S:4</text>
<text>S:5</text>
<text>GND</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="RJ45-8">
</package>
<package name="1X02_2.54_SCREWTERM">
</package>
<package name="1X14_LOCK">
</package>
<package name="POWER_JACK_SMD">
</package>
</packages>
</library>
<library name="Teensy3.0">
<packages>
<package name="TEENSY_3.0_BASIC">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XTEND-DIGI-MODEM">
<description>Package for the Xtend Digi Modem 40 mile range</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="POWER" library="SparkFun-Connectors" package="JST-2-SMD" value="5V">
<attribute name="PROD_ID" value="CONN-08352"/>
</element>
<element name="HACKHD3" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="HACKHD2" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="HACKHD4" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="HACKHD5" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="HACKHD1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="TEENSY" library="Teensy3.0" package="TEENSY_3.0_BASIC" value="TEENSY_3.0_BASIC">
<attribute name="NAME"/>
</element>
<element name="900MHZ_TX" library="SparkFun-RF" package="XTEND-DIGI-MODEM" value="XTEND-DIGI-MODEM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HACKHD6" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="CAM_CONTROL" library="SparkFun-DigitalIC" package="DIL28-3" value="ATMEGA328P_PDIP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="RX3" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="L1" library="adafruit" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="adafruit" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="adafruit" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="adafruit" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_13" library="adafruit" package="CHIP-LED0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="adafruit" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X14_LOCK" value="M14LOCK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X14_LOCK" value="M14LOCK"/>
<element name="BATT_CHARGE" library="SparkFun-Connectors" package="POWER_JACK_SMD" value="5.5x2.1mm Barrel">
<attribute name="PROD_ID" value="CONN-08106"/>
</element>
</elements>
<signals>
<signal name="VBAT">
<contactref element="TEENSY" pad="VBAT"/>
</signal>
<signal name="GND">
<contactref element="HACKHD6" pad="8"/>
<contactref element="HACKHD1" pad="8"/>
<contactref element="CAM_CONTROL" pad="8"/>
<contactref element="CAM_CONTROL" pad="22"/>
<contactref element="HACKHD2" pad="8"/>
<contactref element="HACKHD3" pad="8"/>
<contactref element="HACKHD4" pad="8"/>
<contactref element="HACKHD5" pad="8"/>
<contactref element="900MHZ_TX" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="POWER" pad="1"/>
<contactref element="RX3" pad="P1"/>
<contactref element="RX2" pad="P1"/>
<contactref element="L1" pad="3-GND"/>
<contactref element="L2" pad="3-GND"/>
<contactref element="L3" pad="3-GND"/>
<contactref element="L4" pad="3-GND"/>
<contactref element="R2" pad="1"/>
<contactref element="L5" pad="3-GND"/>
<contactref element="TEENSY" pad="GND"/>
<contactref element="TEENSY" pad="GND1"/>
<contactref element="JP1" pad="1"/>
<contactref element="BATT_CHARGE" pad="P$4"/>
</signal>
<signal name="HD1_1">
<contactref element="HACKHD1" pad="1"/>
<contactref element="CAM_CONTROL" pad="4"/>
</signal>
<signal name="HD1_2">
<contactref element="HACKHD1" pad="2"/>
<contactref element="CAM_CONTROL" pad="5"/>
</signal>
<signal name="HD2_1">
<contactref element="HACKHD2" pad="1"/>
<contactref element="CAM_CONTROL" pad="6"/>
</signal>
<signal name="HD2_2">
<contactref element="HACKHD2" pad="2"/>
<contactref element="CAM_CONTROL" pad="11"/>
</signal>
<signal name="HD3_1">
<contactref element="HACKHD3" pad="1"/>
<contactref element="CAM_CONTROL" pad="12"/>
</signal>
<signal name="HD3_2">
<contactref element="CAM_CONTROL" pad="13"/>
<contactref element="HACKHD3" pad="2"/>
</signal>
<signal name="HD4_1">
<contactref element="HACKHD4" pad="1"/>
<contactref element="CAM_CONTROL" pad="14"/>
</signal>
<signal name="HD4_2">
<contactref element="CAM_CONTROL" pad="15"/>
<contactref element="HACKHD4" pad="2"/>
</signal>
<signal name="HD5_1">
<contactref element="HACKHD5" pad="1"/>
<contactref element="CAM_CONTROL" pad="16"/>
</signal>
<signal name="HD5_2">
<contactref element="CAM_CONTROL" pad="17"/>
<contactref element="HACKHD5" pad="2"/>
</signal>
<signal name="HD6_1">
<contactref element="CAM_CONTROL" pad="18"/>
<contactref element="HACKHD6" pad="1"/>
</signal>
<signal name="HD6_2">
<contactref element="HACKHD6" pad="2"/>
<contactref element="CAM_CONTROL" pad="19"/>
</signal>
<signal name="N$14">
<contactref element="CAM_CONTROL" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="CAM_CONTROL" pad="7"/>
<contactref element="CAM_CONTROL" pad="20"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="900MHZ_TX" pad="2"/>
<contactref element="TEENSY" pad="VIN"/>
<contactref element="900MHZ_TX" pad="7"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="TX1">
<contactref element="TEENSY" pad="1"/>
<contactref element="900MHZ_TX" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="RX1">
<contactref element="CAM_CONTROL" pad="3"/>
<contactref element="TEENSY" pad="0"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RX2">
<contactref element="TEENSY" pad="9"/>
<contactref element="RX2" pad="P2"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="TX2">
<contactref element="TEENSY" pad="10"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="RX3">
<contactref element="TEENSY" pad="7"/>
<contactref element="RX3" pad="P2"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="TX3">
<contactref element="TEENSY" pad="8"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$15">
<contactref element="L1" pad="1-VDD"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="L2" pad="1-VDD"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="L3" pad="1-VDD"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="L4" pad="1-VDD"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="L3" pad="4-DIN"/>
<contactref element="L2" pad="2-DOUT"/>
</signal>
<signal name="N$20">
<contactref element="L4" pad="4-DIN"/>
<contactref element="L3" pad="2-DOUT"/>
</signal>
<signal name="N$21">
<contactref element="L1" pad="2-DOUT"/>
<contactref element="L2" pad="4-DIN"/>
</signal>
<signal name="PIXEL_IN">
<contactref element="TEENSY" pad="6"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$22">
<contactref element="LED_13" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="T13">
<contactref element="TEENSY" pad="13"/>
<contactref element="LED_13" pad="A"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="N$24">
<contactref element="L5" pad="1-VDD"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="L4" pad="2-DOUT"/>
<contactref element="L5" pad="4-DIN"/>
</signal>
<signal name="N$26">
<contactref element="R3" pad="2"/>
<contactref element="L1" pad="4-DIN"/>
</signal>
<signal name="T2">
<contactref element="TEENSY" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="T3">
<contactref element="TEENSY" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="T4">
<contactref element="TEENSY" pad="4"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="T5">
<contactref element="TEENSY" pad="5"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="T11">
<contactref element="TEENSY" pad="11"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="T12">
<contactref element="TEENSY" pad="12"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="T23">
<contactref element="TEENSY" pad="23/A9"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="T22">
<contactref element="TEENSY" pad="22/A8"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="T21">
<contactref element="TEENSY" pad="21/A7"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="T20">
<contactref element="TEENSY" pad="20/A6"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="T19">
<contactref element="TEENSY" pad="19/A5"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="T18">
<contactref element="TEENSY" pad="18/A4"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="T17">
<contactref element="TEENSY" pad="17/A3"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="T16">
<contactref element="TEENSY" pad="16/A2"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="T15">
<contactref element="TEENSY" pad="15/A1"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="T14">
<contactref element="TEENSY" pad="14/A0"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="N$33">
<contactref element="JP2" pad="3"/>
<contactref element="TEENSY" pad="3.3V"/>
<contactref element="TEENSY" pad="3.3V1"/>
</signal>
<signal name="AGND">
<contactref element="TEENSY" pad="AGND"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="5V_CHARGE">
<contactref element="HACKHD1" pad="3"/>
<contactref element="HACKHD2" pad="3"/>
<contactref element="HACKHD3" pad="3"/>
<contactref element="HACKHD4" pad="3"/>
<contactref element="HACKHD5" pad="3"/>
<contactref element="HACKHD6" pad="3"/>
<contactref element="BATT_CHARGE" pad="VIN0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
