<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="59.36" y2="0" width="0" layer="20"/>
<wire x1="59.36" y1="0" x2="59.36" y2="39.36" width="0" layer="20"/>
<wire x1="59.36" y1="39.36" x2="0" y2="39.36" width="0" layer="20"/>
<wire x1="0" y1="39.36" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>H</text>
<text>H-HI</text>
<text>H-MI</text>
<text>H-LO</text>
<text>H-LO</text>
<text>H-MI</text>
<text>H-HI</text>
<text>DRV</text>
<text>PAS</text>
<text>H-OUT</text>
<text>L-OUT</text>
<text>L-HI</text>
<text>L-HI</text>
<text>L-MI</text>
<text>L-MI</text>
<text>L-LO</text>
<text>L-LO</text>
<hole x="1.905" y="37.465" drill="3.2"/>
<hole x="1.905" y="1.905" drill="3.2"/>
<hole x="57.15" y="1.905" drill="3.2"/>
<hole x="57.15" y="37.465" drill="3.2"/>
<text>Arduino Powered Heated Seat
Controller rev. 2</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X06">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="E14_Arduino">
<packages>
<package name="ARDUINO_NANO">
<description>Footprint for representing an Arduino Nano board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="DIP254P762X508-16">
</package>
</packages>
</library>
<library name="M54564P-FP">
<description>&lt;b&gt;M54564P&lt;/b&gt; and &lt;b&gt;M54564FP&lt;/b&gt; are eight-circuit output-sourcing Darlington transistor arrays.
The circuits are made of PNP and NPN transistors.
Both the semiconductor integrated circuits perform high-current driving with extremely low input current supply.
&lt;br&gt;
The M54564P and M54564FP each have eight circuits, which are made of input inverters and current-sourcing outputs.
The outputs are made of PNP transistors and NPN Darlington transistors.
The PNP transistor base current is constant.
Resistance of 50kW is connected between each output pin and GND, making these ICs suitable for fluorescent display tubes.
VS and GND are used commonly among the eight circuits.
Output current is 500mA maximum. Supply voltage VS is 50V maximum.</description>
<packages>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Logo">
<packages>
<package name="OSHW_6X70_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BTN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H-OUT" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L-OUT" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L-TEST" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PCB1" library="E14_Arduino" package="ARDUINO_NANO" value="ARDUINO_NANO"/>
<element name="PWR" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="15k"/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="15k"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10k"/>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="10k"/>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="DIP254P762X508-16" value="ULN2003AN">
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="OC_NEWARK" value="98K2130"/>
<attribute name="MPN" value="ULN2003ANE4"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1210973"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="M54564P-FP" package="DIL18" value="M54564P">
<attribute name="MPN" value="M54564P"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN-TEST" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="Logo" package="OSHW_6X70_NOTEXT" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="PCB1" pad="GND."/>
<contactref element="PCB1" pad="GND"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="10"/>
<contactref element="L-TEST" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="PWR" pad="2"/>
</signal>
<signal name="D2">
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="PCB1" pad="D2"/>
<contactref element="BTN-TEST" pad="1"/>
</signal>
<signal name="D3">
<contactref element="R4" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="PCB1" pad="D3"/>
<contactref element="BTN-TEST" pad="2"/>
</signal>
<signal name="D-BTN">
<contactref element="R1" pad="2"/>
<contactref element="BTN" pad="1"/>
</signal>
<signal name="P-BTN">
<contactref element="R2" pad="2"/>
<contactref element="BTN" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="PCB1" pad="VIN"/>
<contactref element="PWR" pad="1"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="D4">
<contactref element="PCB1" pad="D4"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="D5">
<contactref element="PCB1" pad="D5"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="D10">
<contactref element="PCB1" pad="D10"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="D7">
<contactref element="PCB1" pad="D7"/>
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="D8">
<contactref element="PCB1" pad="D8"/>
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D9">
<contactref element="PCB1" pad="D9"/>
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="DH-HIGH">
<contactref element="U2" pad="18"/>
<contactref element="H-OUT" pad="1"/>
</signal>
<signal name="DH-MID">
<contactref element="U2" pad="17"/>
<contactref element="H-OUT" pad="2"/>
</signal>
<signal name="DH-LOW">
<contactref element="U2" pad="16"/>
<contactref element="H-OUT" pad="3"/>
</signal>
<signal name="PH-HIGH">
<contactref element="H-OUT" pad="4"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="PH-MID">
<contactref element="H-OUT" pad="5"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="PH-LOW">
<contactref element="H-OUT" pad="6"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="DL-HIGH">
<contactref element="L-OUT" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="DL-MID">
<contactref element="L-OUT" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="DL-LOW">
<contactref element="L-OUT" pad="3"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="PL-HIGH">
<contactref element="L-OUT" pad="4"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="PL-MID">
<contactref element="L-OUT" pad="5"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="PL-LOW">
<contactref element="L-OUT" pad="6"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="L-TEST">
<contactref element="U1" pad="9"/>
<contactref element="L-TEST" pad="1"/>
</signal>
<signal name="D6">
<contactref element="U2" pad="3"/>
<contactref element="PCB1" pad="D6"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="H-ON">
<contactref element="U2" pad="11"/>
<contactref element="PWR" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
