<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="97.79" y1="1.27" x2="24.13" y2="1.27" width="0.4064" layer="20"/>
<wire x1="102.87" y1="46.99" x2="97.79" y2="52.07" width="0.4064" layer="20" curve="90"/>
<wire x1="97.79" y1="1.27" x2="102.87" y2="6.35" width="0.4064" layer="20" curve="90"/>
<wire x1="151.13" y1="1.27" x2="110.49" y2="1.27" width="0.4064" layer="20"/>
<wire x1="156.21" y1="6.35" x2="156.21" y2="46.99" width="0.4064" layer="20"/>
<wire x1="97.79" y1="52.07" x2="24.13" y2="52.07" width="0.4064" layer="20"/>
<wire x1="151.384" y1="52.07" x2="156.21" y2="46.99" width="0.4064" layer="20" curve="-90"/>
<wire x1="151.13" y1="1.27" x2="156.21" y2="6.35" width="0.4064" layer="20" curve="90"/>
<text>300</text>
<text>STATUS_LED</text>
<text>AVR_RESET</text>
<text>10K</text>
<text>ICP Header</text>
<text>VCC</text>
<text>MOSI</text>
<text>GND</text>
<text>SCK</text>
<text>MISO</text>
<text>RESET</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>VREF</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>VCC</text>
<text>DOUT</text>
<text>DIN</text>
<text>NC</text>
<text>NC</text>
<text>RSSI</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>GND</text>
<text>XBEE_S2</text>
<text>9V Battery</text>
<text>VCC(+)</text>
<text>GND(-)</text>
<text>GND</text>
<text>VOUT(V3.3)</text>
<text>VIN</text>
<text>300</text>
<text>DC Barrel</text>
<text>PWR SW</text>
<text>10uF</text>
<text>100nF</text>
<text>DC VIN: min:6V-max:13V</text>
<text>PWR_ON</text>
<text>PWR_OFF</text>
<text>100nF</text>
<text>65</text>
<text>5</text>
<text>5</text>
<text>RED</text>
<text>GREEN</text>
<text>BLUE</text>
<text>VCC</text>
<text>RGB LED
Comm Anode</text>
<text>RSSI LED</text>
<text>Bottom Conn</text>
<text>Bottom Conn</text>
<text>P1</text>
<text>P1</text>
<text>P12</text>
<text>P12</text>
<text>DIP_1</text>
<text>DIP_4</text>
<wire x1="24.13" y1="1.27" x2="19.05" y2="6.35" width="0.4064" layer="20" curve="-90"/>
<wire x1="19.05" y1="6.35" x2="19.05" y2="46.99" width="0.4064" layer="20"/>
<wire x1="19.05" y1="46.99" x2="24.13" y2="52.07" width="0.4064" layer="20" curve="-90"/>
<wire x1="102.87" y1="46.99" x2="102.87" y2="6.35" width="0.4064" layer="20"/>
<text>VCC</text>
<text>RGB LED
Comm Anode</text>
<text>BLUE</text>
<text>GREEN</text>
<text>RED</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>10K</text>
<text>10K</text>
<text>10K</text>
<text>10K</text>
<text>100nF</text>
<text> 9.216 Mhz</text>
<text>20pF</text>
<text>20pF</text>
<text>PB1</text>
<text>PB2</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>AVCC</text>
<text>AREF</text>
<text>GND</text>
<text>PC0</text>
<text>PC1</text>
<text>PC2</text>
<text>PC3</text>
<text>PC4</text>
<text>PC5</text>
<text>RESET</text>
<text>RXD</text>
<text>TXD</text>
<text>PD2</text>
<text>PD3</text>
<text>PD4</text>
<text>VCC</text>
<text>GND</text>
<text>XL1</text>
<text>XL2</text>
<text>PD5</text>
<text>PD6</text>
<text>PD7</text>
<text>PB0</text>
<text>LED Node V1.1</text>
<text>James Stokebrand</text>
<text>(C) 11 Nov 2014</text>
<text>Layer 2 (Bottom)</text>
<text>Layer 2 (Top)</text>
<text>Layer 1 (Bottom)</text>
<text>Layer 1 (Top)</text>
<text>LED Node V1.1</text>
<text>James Stokebrand</text>
<text>(C) 11 Nov 2014</text>
<text>LED Node V1.1</text>
<text>James Stokebrand</text>
<text>(C) 11 Nov 2014</text>
<text>LED Node V1.1</text>
<text>James Stokebrand</text>
<text>(C) 11 Nov 2014</text>
<wire x1="151.384" y1="52.07" x2="110.744" y2="52.07" width="0.4064" layer="20"/>
<wire x1="110.744" y1="52.07" x2="105.41" y2="46.99" width="0.4064" layer="20" curve="90"/>
<wire x1="105.41" y1="46.99" x2="105.41" y2="6.35" width="0.4064" layer="20"/>
<wire x1="105.41" y1="6.35" x2="110.49" y2="1.27" width="0.4064" layer="20" curve="90"/>
</plain>
<libraries>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220L1">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="XBEE">
</package>
<package name="EG1213">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.3 mm with drill center</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="OPL_Eagle_Library_Seeed_Sudio">
<packages>
<package name="DIP28">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-RGB-THRU">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Keystone_Electronics_Battery_Holders">
<packages>
<package name="KEYSTONE_CLIP_9V_LOW_PROFILE_PN_71">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="v-reg" package="TO220L1" value="LD117AV33">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C025-030X050" value="100nF"/>
<element name="C2" library="adafruit" package="C025-030X050" value="10uF"/>
<element name="C3" library="adafruit" package="C025-024X044" value="100nF"/>
<element name="D1" library="adafruit" package="DO41-10" value="1N4004"/>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value="DC Barrel Jack"/>
<element name="R1" library="adafruit" package="0204/5" value="68 Ohm"/>
<element name="R2" library="adafruit" package="0204/5" value="5 Ohm"/>
<element name="H1" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H4" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="S2" library="switch-omron" package="B3F-10XX" value="RESET">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="ICP_HEADER" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0204/5" value="5 Ohm"/>
<element name="R9" library="adafruit" package="0204/5" value="10K Ohm"/>
<element name="XBEE" library="adafruit" package="XBEE" value="XBEE"/>
<element name="LED7" library="adafruit" package="LED3MM" value="3mm RED"/>
<element name="R21" library="adafruit" package="0204/5" value="300 Ohm"/>
<element name="U1" library="OPL_Eagle_Library_Seeed_Sudio" package="DIP28" value="ATMEGA328P-PU-1030050P1">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49U-V" value=" 9.216 Mhz"/>
<element name="C4" library="adafruit" package="C025-024X044" value="20pF"/>
<element name="C9" library="adafruit" package="C025-024X044" value="20pf"/>
<element name="S6" library="adafruit" package="EG1213" value="EG1213"/>
<element name="LED8" library="adafruit" package="LED3MM" value="3mm RED"/>
<element name="R14" library="adafruit" package="0204/5" value="300 Ohm"/>
<element name="H5" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H6" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="JP5" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="C13" library="adafruit" package="C025-024X044" value="100nF"/>
<element name="D2" library="SparkFun-LED" package="LED-RGB-THRU" value="LED-RGB-CA-THRUDIFFUSE">
<attribute name="PROD_ID" value="DIO-10632"/>
</element>
<element name="SW1" library="special" package="EDG-04" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0204/5" value="10K"/>
<element name="R5" library="adafruit" package="0204/5" value="10K"/>
<element name="R6" library="adafruit" package="0204/5" value="10K"/>
<element name="R7" library="adafruit" package="0204/5" value="10K"/>
<element name="JP1" library="pinhead" package="2X06" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="2X06" value="">
<attribute name="VALUE"/>
</element>
<element name="9V_BATTERY_CLIP" library="Keystone_Electronics_Battery_Holders" package="KEYSTONE_CLIP_9V_LOW_PROFILE_PN_71" value="KEYSTONE_CLIP_9V_LOW_PROFILE_PN_71"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="CN1" pad="PWR"/>
<contactref element="D1" pad="A"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="S6" pad="1"/>
</signal>
<signal name="GND">
<contactref element="CN1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="ICP_HEADER" pad="6"/>
<contactref element="XBEE" pad="10"/>
<contactref element="R21" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="SW1" pad="8"/>
<contactref element="JP2" pad="2"/>
<contactref element="SW1" pad="7"/>
<contactref element="SW1" pad="6"/>
<contactref element="SW1" pad="5"/>
</signal>
<signal name="+3V3">
<contactref element="ICP_HEADER" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="XBEE" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="XBEE" pad="14"/>
<contactref element="C13" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="AVR_TXD_M">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="AVR_RXD_M">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="XBEE_RSSI">
<contactref element="LED7" pad="A"/>
<contactref element="XBEE" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="LED7" pad="K"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="LED_STATUS">
<contactref element="U1" pad="4"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="XTAL1">
<contactref element="U1" pad="9"/>
<contactref element="Y1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="U1" pad="10"/>
<contactref element="Y1" pad="2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="AVR_MOSI_B">
<contactref element="ICP_HEADER" pad="4"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="AVR_MISO_B">
<contactref element="ICP_HEADER" pad="1"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="AVR_SCK_B">
<contactref element="ICP_HEADER" pad="3"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="S6" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="LED8" pad="K"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="AVR_RXD_B">
<contactref element="XBEE" pad="2"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="AVR_TXD_B">
<contactref element="XBEE" pad="3"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="AVR_SCK_M">
<contactref element="U1" pad="19"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="AVR_MISO_M">
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="AVR_MOSI_M">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="AVR_RESET_B">
<contactref element="ICP_HEADER" pad="5"/>
<contactref element="R9" pad="2"/>
<contactref element="S2" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="AVR_RESET_M">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="V33_M">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="20"/>
<contactref element="C3" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="GND_M">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="22"/>
<contactref element="C4" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP5" pad="2"/>
<contactref element="CN1" pad="GNDBREAK"/>
</signal>
<signal name="N$7">
</signal>
<signal name="AVR_TXD_M1">
</signal>
<signal name="RE_OUT_A1">
</signal>
<signal name="AVR_MOSI_M1">
</signal>
<signal name="LED_6_M1">
</signal>
<signal name="RE_SW+_M1">
</signal>
<signal name="RE_A_M1">
</signal>
<signal name="V33_M1">
</signal>
<signal name="+3V1">
</signal>
<signal name="N$4">
<contactref element="D2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="D2" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D2" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="DIP_1_B">
<contactref element="SW1" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="DIP_2_B">
<contactref element="SW1" pad="2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="DIP_3_B">
<contactref element="SW1" pad="3"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="DIP_4_B">
<contactref element="SW1" pad="4"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="DIP_1_OUT">
<contactref element="U1" pad="11"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="DIP_2_OUT">
<contactref element="U1" pad="12"/>
<contactref element="R5" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="DIP_3_OUT">
<contactref element="U1" pad="13"/>
<contactref element="R6" pad="1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="DIP_4_OUT">
<contactref element="U1" pad="14"/>
<contactref element="R7" pad="1"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="RED_LED_M">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="GREEN_LED_M">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="BLUE_LED_M">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="28"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
