<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="28" y2="0" width="0" layer="20"/>
<wire x1="28" y1="0" x2="28" y2="21" width="0" layer="20"/>
<wire x1="28" y1="21" x2="21" y2="28" width="0" layer="20"/>
<wire x1="21" y1="28" x2="7" y2="28" width="0" layer="20"/>
<wire x1="7" y1="28" x2="0" y2="21" width="0" layer="20"/>
<wire x1="0" y1="21" x2="0" y2="0" width="0" layer="20"/>
<text>XBee Stacker
Arduino USB v2.1</text>
<text>+</text>
<text>Rob
Faludi
2014</text>
<text>VCC</text>
<text>D11/TX</text>
<text>D10/RX</text>
<text>MISO</text>
<text>RESET</text>
<text>D9</text>
<text>MOSI</text>
<text>D8</text>
<text>D7</text>
<text>GND</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>D6</text>
<text>D5</text>
<text>D4</text>
<text>D3/SCL</text>
<text>D2/SDA</text>
<text>SCK</text>
<text>+</text>
<text>RESET</text>
<text>+</text>
<text>+</text>
<text>XBee Reset</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X10-2MM-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="PAD.02X.02">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="OPL Eagle Library">
<packages>
<package name="4P-SMD-7.0X3.5X3.5H-90D">
</package>
<package name="2P-SMD-5.0X3.2">
<description>3.2mm*5mm dimension &lt;br&gt;
8MHz available</description>
</package>
<package name="B-SMD-5P">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X10-2MM-SMD" value="M102MMSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X10-2MM-SMD" value="M102MMSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0603-CAP" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X10-2MM-SMD" value="M102MMSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X10-2MM-SMD" value="M102MMSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="STATUS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0603-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-DigitalIC" package="SPARKFUN-DIGITALIC_TQFP44" value="ATMEGA32U4TQFP">
<attribute name="PROD_ID" value="IC-11161"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="ASSOC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="22ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="22ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0603-CAP" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SparkFun-PowerIC" package="SOT223" value="3.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0603-CAP" value="1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun-LED" package="LED-0603" value="RX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun-LED" package="LED-0603" value="TX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K2" library="OPL Eagle Library" package="4P-SMD-7.0X3.5X3.5H-90D" value="RESET">
<attribute name="NAME"/>
</element>
<element name="X1" library="OPL Eagle Library" package="2P-SMD-5.0X3.2" value="CRYSTAL 16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun-LED" package="LED-0603" value="RSSI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="SparkFun-Passives" package="PAD.02X.02" value="GND"/>
<element name="TP2" library="SparkFun-Passives" package="PAD.02X.02" value="XB_Reset"/>
<element name="J1" library="OPL Eagle Library" package="B-SMD-5P" value="MICRO-USB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="JP3" pad="10"/>
<contactref element="R25" pad="1"/>
<contactref element="U$1" pad="43"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="35"/>
<contactref element="R4" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="K2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="J1" pad="E1"/>
<contactref element="J1" pad="E2"/>
<contactref element="J1" pad="P2"/>
<contactref element="J1" pad="P1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="3.3V">
<contactref element="JP1" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="44"/>
<contactref element="U$1" pad="42"/>
<contactref element="JP2" pad="4"/>
<contactref element="IC1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="C1" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="U$1" pad="13"/>
<contactref element="JP3" pad="5"/>
<contactref element="K2" pad="1"/>
</signal>
<signal name="ASSOC">
<contactref element="JP2" pad="5"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="XTAL1">
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="17"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="16"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="11"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="9"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="10"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="RSSI">
<contactref element="JP1" pad="6"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="COMMISSIONING">
<contactref element="JP2" pad="10"/>
</signal>
<signal name="PRG_RSET">
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="R25" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="VBUS">
<contactref element="U$1" pad="7"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="U$1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="UCAP">
<contactref element="U$1" pad="6"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="RD+">
<contactref element="U$1" pad="4"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="RD-">
<contactref element="U$1" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="HWB">
<contactref element="U$1" pad="33"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="36"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="38"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="39"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="A4">
<contactref element="U$1" pad="40"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="D0/RX">
<contactref element="U$1" pad="20"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D1/TX">
<contactref element="U$1" pad="21"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="D2/SDA">
<contactref element="U$1" pad="19"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="D3/SCL">
<contactref element="U$1" pad="18"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="25"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="31"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="1"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="D8">
<contactref element="U$1" pad="28"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="D9">
<contactref element="U$1" pad="29"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="D10">
<contactref element="U$1" pad="30"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="D11">
<contactref element="U$1" pad="12"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="D12">
<contactref element="U$1" pad="26"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="D13">
<contactref element="U$1" pad="32"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="RXLED">
<contactref element="U$1" pad="8"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="TXLED">
<contactref element="U$1" pad="22"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="27"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="D+">
<contactref element="J1" pad="3"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D-">
<contactref element="J1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="37"/>
<contactref element="JP4" pad="9"/>
</signal>
<signal name="A5">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="41"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED5" pad="C"/>
</signal>
<signal name="XB_RESET">
<contactref element="JP1" pad="5"/>
<contactref element="TP2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
