<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<text>T.......................</text>
<text>T++....</text>
<text>T......</text>
<text>T++...................</text>
<wire x1="0" y1="1.3462" x2="1.27" y2="0.0762" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0.0762" x2="77.246975" y2="0.0762" width="0" layer="20"/>
<wire x1="77.246975" y1="0.0762" x2="78.669375" y2="1.3208" width="0" layer="20" curve="90"/>
<wire x1="78.669375" y1="1.3208" x2="78.669375" y2="49.5808" width="0" layer="20"/>
<wire x1="78.669375" y1="49.5808" x2="77.348575" y2="51.4604" width="0" layer="20" curve="90"/>
<wire x1="77.348575" y1="51.4604" x2="1.1176" y2="51.4096" width="0" layer="20"/>
<wire x1="1.1176" y1="51.4096" x2="0" y2="50.419" width="0" layer="20" curve="90"/>
<wire x1="0" y1="50.419" x2="0" y2="1.3462" width="0" layer="20"/>
<hole x="28.125715625" y="25.6942" drill="2.2606"/>
<text>ArtFAB Maxuino Master</text>
<hole x="61.221915625" y="48.4272" drill="2.2606"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="1X04">
</package>
<package name="1X02">
</package>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="teensy_ali">
<packages>
<package name="TEENSY-OR-++">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="VCC_SELECT" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="V_EXT" value="V_EXT"/>
<attribute name="TEENSY" value="Teensy"/>
</element>
<element name="I2C_TEENSY++" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D0[0]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B1[1]"/>
</element>
<element name="I2C_TEENSY" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1[1]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B2[2]"/>
</element>
<element name="D2[2]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B3[3]"/>
</element>
<element name="D3[3]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B7[4]"/>
</element>
<element name="D4[4]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="D0[5]"/>
</element>
<element name="D5[5]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="D1[6]"/>
</element>
<element name="D6[6]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="D2[7]"/>
</element>
<element name="D7[7]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="D3[8]"/>
</element>
<element name="C0[10]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1[11]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2[12]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3[13]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4[14]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5[15]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6[16]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7[17]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B0[20]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B6[15]"/>
</element>
<element name="B1[21]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="F7[16]"/>
</element>
<element name="B2[22]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="F6[17]"/>
</element>
<element name="B3[23]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="F5[18]"/>
</element>
<element name="B4[23]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="F4[18]"/>
</element>
<element name="B5[24]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="F1[19]"/>
</element>
<element name="B6[26]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="F0[21]"/>
</element>
<element name="B7[27]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="TEENSY" value="B0[0]"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1[39]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2[40]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F3[41]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F4[42]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F5[43]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F6[44]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F7[45]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E1[9]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="C7[10]"/>
</element>
<element name="E4[36]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="5V" value="VCC"/>
<attribute name="GND" value="GND"/>
<attribute name="PIN" value="Pin"/>
<attribute name="VEXT" value="VExt"/>
</element>
<element name="E5[37]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E6[18]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B4[13]"/>
</element>
<element name="E7[19]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="B5[14]"/>
</element>
<element name="E6[24]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="5V" value="VCC"/>
<attribute name="GND" value="GND"/>
<attribute name="PIN" value="Pin"/>
<attribute name="VEXT" value="VExt"/>
</element>
<element name="A0[28]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GND" value="GND"/>
<attribute name="PIN" value="pin"/>
<attribute name="VCC" value="VCC"/>
<attribute name="VEXT" value="vext"/>
<attribute name="TEENSY" value="Teensy++"/>
</element>
<element name="A1[29]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A2[30]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A3[31]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A4[32]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A5[33]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A6[34]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A7[35]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4[22]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5[23]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C_TEENSYPP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="I2C_TEENSY1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="I2C_TEENSYPP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="I2C_TEENSY2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
<attribute name="GND" value="GND"/>
<attribute name="SCL" value="SCL"/>
<attribute name="SDA" value="SDA"/>
<attribute name="VCC" value="VCC"/>
</element>
<element name="D7[12]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEENSY-POWER" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VEXT" value="vext"/>
</element>
<element name="TEENSY2/++" library="teensy_ali" package="TEENSY-OR-++" value="TEENSY-OR-++"/>
<element name="V_EXT" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="VALUE"/>
</element>
<element name="F0[38]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E0[8]" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TEENSY" value="C6[9]"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="I2C_TEENSY++" pad="1"/>
<contactref element="D0[0]" pad="2"/>
<contactref element="D1[1]" pad="2"/>
<contactref element="D2[2]" pad="2"/>
<contactref element="D3[3]" pad="2"/>
<contactref element="D4[4]" pad="2"/>
<contactref element="D5[5]" pad="2"/>
<contactref element="D6[6]" pad="2"/>
<contactref element="D7[7]" pad="2"/>
<contactref element="C0[10]" pad="2"/>
<contactref element="C1[11]" pad="2"/>
<contactref element="C2[12]" pad="2"/>
<contactref element="C3[13]" pad="2"/>
<contactref element="C4[14]" pad="2"/>
<contactref element="C5[15]" pad="2"/>
<contactref element="C6[16]" pad="2"/>
<contactref element="C7[17]" pad="2"/>
<contactref element="B0[20]" pad="2"/>
<contactref element="B1[21]" pad="2"/>
<contactref element="B2[22]" pad="2"/>
<contactref element="B3[23]" pad="2"/>
<contactref element="B4[23]" pad="2"/>
<contactref element="B5[24]" pad="2"/>
<contactref element="B6[26]" pad="2"/>
<contactref element="B7[27]" pad="2"/>
<contactref element="F1[39]" pad="2"/>
<contactref element="F2[40]" pad="2"/>
<contactref element="F3[41]" pad="2"/>
<contactref element="F4[42]" pad="2"/>
<contactref element="F5[43]" pad="2"/>
<contactref element="F6[44]" pad="2"/>
<contactref element="F7[45]" pad="2"/>
<contactref element="E1[9]" pad="2"/>
<contactref element="E4[36]" pad="2"/>
<contactref element="E5[37]" pad="2"/>
<contactref element="E6[18]" pad="2"/>
<contactref element="E7[19]" pad="2"/>
<contactref element="E6[24]" pad="2"/>
<contactref element="A0[28]" pad="2"/>
<contactref element="A1[29]" pad="2"/>
<contactref element="A2[30]" pad="2"/>
<contactref element="A3[31]" pad="2"/>
<contactref element="A4[32]" pad="2"/>
<contactref element="A5[33]" pad="2"/>
<contactref element="A6[34]" pad="2"/>
<contactref element="A7[35]" pad="2"/>
<contactref element="D4[22]" pad="2"/>
<contactref element="D5[23]" pad="2"/>
<contactref element="I2C_TEENSY" pad="1"/>
<contactref element="D7[12]" pad="2"/>
<contactref element="I2C_TEENSY1" pad="1"/>
<contactref element="I2C_TEENSY2" pad="1"/>
<contactref element="TEENSY2/++" pad="GND"/>
<contactref element="TEENSY2/++" pad="GND"/>
<contactref element="V_EXT" pad="GND"/>
<contactref element="V_EXT" pad="GNDBREAK"/>
<contactref element="I2C_TEENSYPP2" pad="1"/>
<contactref element="I2C_TEENSYPP1" pad="1"/>
<contactref element="F0[38]" pad="2"/>
<contactref element="E0[8]" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="VCC_SELECT" pad="2"/>
<contactref element="D0[0]" pad="3"/>
<contactref element="D1[1]" pad="3"/>
<contactref element="D2[2]" pad="3"/>
<contactref element="D3[3]" pad="3"/>
<contactref element="D4[4]" pad="3"/>
<contactref element="D5[5]" pad="3"/>
<contactref element="D6[6]" pad="3"/>
<contactref element="D7[7]" pad="3"/>
<contactref element="C0[10]" pad="3"/>
<contactref element="C1[11]" pad="3"/>
<contactref element="C2[12]" pad="3"/>
<contactref element="C3[13]" pad="3"/>
<contactref element="C4[14]" pad="3"/>
<contactref element="C5[15]" pad="3"/>
<contactref element="C6[16]" pad="3"/>
<contactref element="C7[17]" pad="3"/>
<contactref element="B0[20]" pad="3"/>
<contactref element="B1[21]" pad="3"/>
<contactref element="B2[22]" pad="3"/>
<contactref element="B3[23]" pad="3"/>
<contactref element="B4[23]" pad="3"/>
<contactref element="B5[24]" pad="3"/>
<contactref element="B6[26]" pad="3"/>
<contactref element="B7[27]" pad="3"/>
<contactref element="F2[40]" pad="3"/>
<contactref element="F3[41]" pad="3"/>
<contactref element="F4[42]" pad="3"/>
<contactref element="F5[43]" pad="3"/>
<contactref element="F6[44]" pad="3"/>
<contactref element="F7[45]" pad="3"/>
<contactref element="E1[9]" pad="3"/>
<contactref element="E4[36]" pad="3"/>
<contactref element="E5[37]" pad="3"/>
<contactref element="E6[18]" pad="3"/>
<contactref element="E7[19]" pad="3"/>
<contactref element="E6[24]" pad="3"/>
<contactref element="A0[28]" pad="3"/>
<contactref element="A1[29]" pad="3"/>
<contactref element="A2[30]" pad="3"/>
<contactref element="A3[31]" pad="3"/>
<contactref element="A4[32]" pad="3"/>
<contactref element="A5[33]" pad="3"/>
<contactref element="A6[34]" pad="3"/>
<contactref element="A7[35]" pad="3"/>
<contactref element="D4[22]" pad="3"/>
<contactref element="D5[23]" pad="3"/>
<contactref element="F1[39]" pad="3"/>
<contactref element="D7[12]" pad="3"/>
<contactref element="F0[38]" pad="3"/>
<contactref element="E0[8]" pad="3"/>
</signal>
<signal name="NFO">
<contactref element="VCC_SELECT" pad="3"/>
<contactref element="D0[0]" pad="1"/>
<contactref element="D1[1]" pad="1"/>
<contactref element="D2[2]" pad="1"/>
<contactref element="D3[3]" pad="1"/>
<contactref element="D4[4]" pad="1"/>
<contactref element="D5[5]" pad="1"/>
<contactref element="D6[6]" pad="1"/>
<contactref element="D7[7]" pad="1"/>
<contactref element="C0[10]" pad="1"/>
<contactref element="C1[11]" pad="1"/>
<contactref element="C2[12]" pad="1"/>
<contactref element="C3[13]" pad="1"/>
<contactref element="C4[14]" pad="1"/>
<contactref element="C5[15]" pad="1"/>
<contactref element="C6[16]" pad="1"/>
<contactref element="C7[17]" pad="1"/>
<contactref element="B0[20]" pad="1"/>
<contactref element="B1[21]" pad="1"/>
<contactref element="B2[22]" pad="1"/>
<contactref element="B3[23]" pad="1"/>
<contactref element="B4[23]" pad="1"/>
<contactref element="B5[24]" pad="1"/>
<contactref element="B6[26]" pad="1"/>
<contactref element="B7[27]" pad="1"/>
<contactref element="F1[39]" pad="1"/>
<contactref element="F2[40]" pad="1"/>
<contactref element="F3[41]" pad="1"/>
<contactref element="F4[42]" pad="1"/>
<contactref element="F5[43]" pad="1"/>
<contactref element="F6[44]" pad="1"/>
<contactref element="F7[45]" pad="1"/>
<contactref element="E1[9]" pad="1"/>
<contactref element="E4[36]" pad="1"/>
<contactref element="E5[37]" pad="1"/>
<contactref element="E6[18]" pad="1"/>
<contactref element="E7[19]" pad="1"/>
<contactref element="E6[24]" pad="1"/>
<contactref element="A0[28]" pad="1"/>
<contactref element="A1[29]" pad="1"/>
<contactref element="A2[30]" pad="1"/>
<contactref element="A3[31]" pad="1"/>
<contactref element="A4[32]" pad="1"/>
<contactref element="A5[33]" pad="1"/>
<contactref element="A6[34]" pad="1"/>
<contactref element="A7[35]" pad="1"/>
<contactref element="D4[22]" pad="1"/>
<contactref element="D5[23]" pad="1"/>
<contactref element="D7[12]" pad="1"/>
<contactref element="TEENSY-POWER" pad="2"/>
<contactref element="V_EXT" pad="PWR"/>
<contactref element="F0[38]" pad="1"/>
<contactref element="E0[8]" pad="1"/>
</signal>
<signal name="C0">
<contactref element="C0[10]" pad="4"/>
<contactref element="TEENSY2/++" pad="C0"/>
</signal>
<signal name="C1">
<contactref element="C1[11]" pad="4"/>
<contactref element="TEENSY2/++" pad="C1"/>
</signal>
<signal name="C2">
<contactref element="C2[12]" pad="4"/>
<contactref element="TEENSY2/++" pad="C2"/>
</signal>
<signal name="C3">
<contactref element="C3[13]" pad="4"/>
<contactref element="TEENSY2/++" pad="C3"/>
</signal>
<signal name="C4">
<contactref element="C4[14]" pad="4"/>
<contactref element="TEENSY2/++" pad="C4"/>
</signal>
<signal name="C5">
<contactref element="C5[15]" pad="4"/>
<contactref element="TEENSY2/++" pad="C5"/>
</signal>
<signal name="E4">
<contactref element="E4[36]" pad="4"/>
<contactref element="TEENSY2/++" pad="E4"/>
</signal>
<signal name="E5">
<contactref element="E5[37]" pad="4"/>
<contactref element="TEENSY2/++" pad="E5"/>
</signal>
<signal name="A7">
<contactref element="A7[35]" pad="4"/>
<contactref element="TEENSY2/++" pad="A7"/>
</signal>
<signal name="A6">
<contactref element="A6[34]" pad="4"/>
<contactref element="TEENSY2/++" pad="A6"/>
</signal>
<signal name="A5">
<contactref element="A5[33]" pad="4"/>
<contactref element="TEENSY2/++" pad="A5"/>
</signal>
<signal name="A3">
<contactref element="A3[31]" pad="4"/>
<contactref element="TEENSY2/++" pad="A3"/>
</signal>
<signal name="A4">
<contactref element="A4[32]" pad="4"/>
<contactref element="TEENSY2/++" pad="A4"/>
</signal>
<signal name="A2">
<contactref element="A2[30]" pad="4"/>
<contactref element="TEENSY2/++" pad="A2"/>
</signal>
<signal name="A0">
<contactref element="A0[28]" pad="4"/>
<contactref element="TEENSY2/++" pad="A0"/>
</signal>
<signal name="F4">
<contactref element="F4[42]" pad="4"/>
<contactref element="TEENSY2/++" pad="F4"/>
</signal>
<signal name="F1">
<contactref element="F1[39]" pad="4"/>
<contactref element="TEENSY2/++" pad="F1"/>
</signal>
<signal name="C6">
<contactref element="C6[16]" pad="4"/>
<contactref element="TEENSY2/++" pad="C6"/>
</signal>
<signal name="C7">
<contactref element="C7[17]" pad="4"/>
<contactref element="TEENSY2/++" pad="C7"/>
</signal>
<signal name="A1">
<contactref element="A1[29]" pad="4"/>
<contactref element="TEENSY2/++" pad="A1"/>
</signal>
<signal name="F7">
<contactref element="F7[45]" pad="4"/>
<contactref element="TEENSY2/++" pad="F7"/>
</signal>
<signal name="F6">
<contactref element="F6[44]" pad="4"/>
<contactref element="TEENSY2/++" pad="F6"/>
</signal>
<signal name="F5">
<contactref element="F5[43]" pad="4"/>
<contactref element="TEENSY2/++" pad="F5"/>
</signal>
<signal name="F3">
<contactref element="F3[41]" pad="4"/>
<contactref element="TEENSY2/++" pad="F3"/>
</signal>
<signal name="F2">
<contactref element="F2[40]" pad="4"/>
<contactref element="TEENSY2/++" pad="F2"/>
</signal>
<signal name="VCC">
<contactref element="VCC_SELECT" pad="1"/>
<contactref element="I2C_TEENSY++" pad="2"/>
<contactref element="I2C_TEENSY" pad="2"/>
<contactref element="I2C_TEENSYPP1" pad="2"/>
<contactref element="I2C_TEENSYPP2" pad="2"/>
<contactref element="I2C_TEENSY1" pad="2"/>
<contactref element="I2C_TEENSY2" pad="2"/>
<contactref element="TEENSY-POWER" pad="1"/>
<contactref element="TEENSY2/++" pad="VCC"/>
<contactref element="TEENSY2/++" pad="VCC"/>
</signal>
<signal name="B7_B0">
<contactref element="B7[27]" pad="4"/>
<contactref element="TEENSY2/++" pad="B7_B0"/>
</signal>
<signal name="D0_B1">
<contactref element="D0[0]" pad="4"/>
<contactref element="I2C_TEENSY++" pad="4"/>
<contactref element="I2C_TEENSYPP1" pad="4"/>
<contactref element="I2C_TEENSYPP2" pad="4"/>
<contactref element="TEENSY2/++" pad="D0_B1"/>
</signal>
<signal name="D1_B2">
<contactref element="D1[1]" pad="4"/>
<contactref element="I2C_TEENSY++" pad="3"/>
<contactref element="I2C_TEENSYPP1" pad="3"/>
<contactref element="I2C_TEENSYPP2" pad="3"/>
<contactref element="TEENSY2/++" pad="D1_B2"/>
</signal>
<signal name="D2_B3">
<contactref element="D2[2]" pad="4"/>
<contactref element="TEENSY2/++" pad="D2_B3"/>
</signal>
<signal name="D3_B7">
<contactref element="D3[3]" pad="4"/>
<contactref element="TEENSY2/++" pad="D3_B7"/>
</signal>
<signal name="D4_D0">
<contactref element="D4[4]" pad="4"/>
<contactref element="I2C_TEENSY" pad="4"/>
<contactref element="I2C_TEENSY1" pad="4"/>
<contactref element="I2C_TEENSY2" pad="4"/>
<contactref element="TEENSY2/++" pad="D4_D0"/>
</signal>
<signal name="D5_D1">
<contactref element="D5[5]" pad="4"/>
<contactref element="I2C_TEENSY" pad="3"/>
<contactref element="I2C_TEENSY1" pad="3"/>
<contactref element="I2C_TEENSY2" pad="3"/>
<contactref element="TEENSY2/++" pad="D5_D1"/>
</signal>
<signal name="D6_D2">
<contactref element="D6[6]" pad="4"/>
<contactref element="TEENSY2/++" pad="D6_D2"/>
</signal>
<signal name="D7_D3">
<contactref element="D7[7]" pad="4"/>
<contactref element="TEENSY2/++" pad="D7_D3"/>
</signal>
<signal name="E0_C6">
<contactref element="TEENSY2/++" pad="E0_C6"/>
<contactref element="E0[8]" pad="4"/>
</signal>
<signal name="E1_C7">
<contactref element="E1[9]" pad="4"/>
<contactref element="TEENSY2/++" pad="E1_C7"/>
</signal>
<signal name="B6_F0">
<contactref element="B6[26]" pad="4"/>
<contactref element="TEENSY2/++" pad="B6_F0"/>
</signal>
<signal name="B5_F1">
<contactref element="B5[24]" pad="4"/>
<contactref element="TEENSY2/++" pad="B5_F1"/>
</signal>
<signal name="B4_F4">
<contactref element="B4[23]" pad="4"/>
<contactref element="TEENSY2/++" pad="B4_F4"/>
</signal>
<signal name="B3_F5">
<contactref element="B3[23]" pad="4"/>
<contactref element="TEENSY2/++" pad="B3_F5"/>
</signal>
<signal name="B2_F6">
<contactref element="B2[22]" pad="4"/>
<contactref element="TEENSY2/++" pad="B2_F6"/>
</signal>
<signal name="B1_F7">
<contactref element="B1[21]" pad="4"/>
<contactref element="TEENSY2/++" pad="B1_F7"/>
</signal>
<signal name="B0_B6">
<contactref element="B0[20]" pad="4"/>
<contactref element="TEENSY2/++" pad="B0_B6"/>
</signal>
<signal name="E7_B5">
<contactref element="E7[19]" pad="4"/>
<contactref element="TEENSY2/++" pad="E7_B5"/>
</signal>
<signal name="E6_B4">
<contactref element="E6[18]" pad="4"/>
<contactref element="TEENSY2/++" pad="E6_B4"/>
</signal>
<signal name="GND1_D7">
<contactref element="D7[12]" pad="4"/>
<contactref element="TEENSY2/++" pad="GND1_D7"/>
</signal>
<signal name="F0">
<contactref element="TEENSY2/++" pad="F0"/>
<contactref element="F0[38]" pad="4"/>
</signal>
<signal name="_D5">
<contactref element="D5[23]" pad="4"/>
<contactref element="TEENSY2/++" pad="_D5"/>
</signal>
<signal name="_E6">
<contactref element="E6[24]" pad="4"/>
<contactref element="TEENSY2/++" pad="_E6"/>
</signal>
<signal name="AREF_D6">
<contactref element="TEENSY2/++" pad="AREF_D6"/>
</signal>
<signal name="_D4">
<contactref element="D4[22]" pad="4"/>
<contactref element="TEENSY2/++" pad="_D4"/>
</signal>
<signal name="RST">
<contactref element="TEENSY2/++" pad="RST_"/>
</signal>
<signal name="GND2">
<contactref element="TEENSY2/++" pad="GND2_"/>
</signal>
<signal name="VCC1">
<contactref element="TEENSY2/++" pad="VCC1_"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
