<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0.05" y1="0" x2="22.05" y2="0" width="0" layer="20"/>
<wire x1="22.05" y1="0" x2="22.05" y2="22.06" width="0" layer="20"/>
<wire x1="22.05" y1="22.06" x2="0.05" y2="22.06" width="0" layer="20"/>
<hole x="11.5125" y="8.0875" drill="6"/>
<text>BG DY 05.15 R 0.0.0 </text>
<wire x1="0.05" y1="0" x2="0.05" y2="22.06" width="0" layer="20"/>
<text>GND</text>
<text>VDD</text>
<text>SCL</text>
<text>MOSI</text>
<text>MISO</text>
<text>NCS</text>
<text>GND</text>
<text>RST</text>
</plain>
<libraries>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="avago_opt">
<packages>
<package name="DIP-8">
<description>Custom Dip-8 Package for the ADNS-5030. Pins on adjecent side of the package are offseted by 1 mm.</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE08">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="SparkFun-Retired" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="A5030" library="avago_opt" package="DIP-8" value=""/>
<element name="LED1" library="led" package="SML0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FH8" library="con-lsta" package="FE08" value="FE08-1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="SparkFun-Retired" package="0402-CAP" value="4.7uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="FH8" pad="2"/>
<contactref element="A5030" pad="P$6"/>
<contactref element="FH8" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="A5030" pad="P$4"/>
<contactref element="FH8" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="A5030" pad="P$3"/>
<contactref element="FH8" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="A5030" pad="P$5"/>
<contactref element="FH8" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="C"/>
<contactref element="A5030" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="A5030" pad="P$1"/>
<contactref element="FH8" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="FH8" pad="7"/>
<contactref element="A5030" pad="P$8"/>
</signal>
<signal name="N$7">
</signal>
<signal name="VDD">
<contactref element="LED1" pad="A"/>
<contactref element="C3" pad="1"/>
<contactref element="A5030" pad="P$7"/>
<contactref element="C1" pad="1"/>
<contactref element="FH8" pad="1"/>
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
