<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="86.03" y2="0" width="0" layer="20"/>
<wire x1="86.03" y1="0" x2="86.03" y2="33.01" width="0" layer="20"/>
<wire x1="86.03" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
<text>GND IN</text>
<text>GND OUT</text>
<text>5V IN</text>
<text>5V OUT</text>
<text>NO</text>
<text>NO</text>
<text>NC</text>
<text>NC</text>
<text>PS1 IN</text>
<text>PS1 OUT</text>
<text>PS2 IN</text>
<text>PS1 OUT</text>
<text>LED+</text>
<text>LED-</text>
<text>Pandora Products</text>
<text>PS Controller V 1.0</text>
<text>25 October 2014</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JS-M">
<description>&lt;b&gt;Automotive Ultra-Miniature Power Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61211_0000.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GOT" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="O_5" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="O_P1" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="O_P2" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="GIN" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="I_5" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="I_P1" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="I_P2" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="NO1" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="NO" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="NC" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="NC1" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="K1" library="relay" package="JS-M" value="JS-M1-9V-5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="K2" library="relay" package="JS-M" value="JS-M1-9V-5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="K3" library="relay" package="JS-M" value="JS-M1-9V-5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="470 ohm"/>
<element name="LED+" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
<element name="LED-" library="wirepad" package="3,81/1,4" value="WIREPAD3,81/1,4"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="GOT" pad="1"/>
<contactref element="GIN" pad="1"/>
<contactref element="K1" pad="2"/>
<contactref element="K2" pad="2"/>
<contactref element="K3" pad="2"/>
<contactref element="LED-" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="I_5" pad="1"/>
<contactref element="K1" pad="C"/>
<contactref element="NO1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="O_5" pad="1"/>
<contactref element="NC" pad="1"/>
<contactref element="K1" pad="NO"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="I_P2" pad="1"/>
<contactref element="K3" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="I_P1" pad="1"/>
<contactref element="K2" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="NC1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="C"/>
<contactref element="K2" pad="1"/>
<contactref element="K3" pad="1"/>
<contactref element="NO" pad="1"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="O_P1" pad="1"/>
<contactref element="K2" pad="NO"/>
</signal>
<signal name="N$10">
<contactref element="O_P2" pad="1"/>
<contactref element="K3" pad="NO"/>
</signal>
<signal name="N$11">
<contactref element="LED+" pad="1"/>
<contactref element="R1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
