<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="34.29" y2="0" width="0" layer="20"/>
<wire x1="34.29" y1="0" x2="34.29" y2="66.675" width="0" layer="20"/>
<wire x1="0" y1="66.675" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="66.675" x2="13.18386875" y2="66.675" width="0" layer="20"/>
<wire x1="13.18386875" y1="66.675" x2="13.18386875" y2="61.1886" width="0" layer="20"/>
<wire x1="13.18386875" y1="61.1886" x2="21.0947" y2="61.1886" width="0" layer="20"/>
<wire x1="21.0947" y1="61.1886" x2="21.0947" y2="66.675" width="0" layer="20"/>
<wire x1="21.0947" y1="66.675" x2="34.29" y2="66.675" width="0" layer="20"/>
</plain>
<libraries>
<library name="atmel-xmega">
<description>&lt;b&gt;&lt;font size=75 face=arial color="#007FFF"&gt;Atmel&lt;/font&gt;&lt;/b&gt;
&lt;p&gt;

&lt;b&gt;&lt;font size=4&gt;XMega Devices&lt;/font&gt;&lt;/b&gt;
&lt;p&gt;

&lt;table border=0 cellspacing=1 cellpadding=2&gt;
  &lt;tr&gt;
    &lt;td colspan=5 bgcolor="#cccccc"&gt;
      &lt;font color="#0000FF" size=3 face=arial&gt;&lt;b&gt;100-Pins Package&lt;/b&gt;&lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td align=center bgcolor="#eeeeee" width="20%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Devices Name&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd" width="10%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Flash (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee" width="10%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;SRAM (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd" width="10%"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;EEPROM (Bytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Packages&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      ATxmega64A1&lt;br&gt;
      ATxmega64A1U&lt;br&gt;
      ATxmega64B1&lt;br&gt;
      ATxmega128A1&lt;br&gt;
      ATxmega128A1U&lt;br&gt;
      ATxmega128B1&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center nowrap&gt;&lt;font face=arial size=3&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      TQFP 100A 100&lt;br&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      CBGA 100C1 100,TQFP 100A 100,VFBGA 100C2 100 (10x10)&lt;br&gt;
      TQFP 100A 100&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td colspan=5 bgcolor="#cccccc"&gt;
      &lt;font color="#0000FF" size=3 face=arial&gt;&lt;b&gt;64-Pins Package&lt;/b&gt;&lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Devices Name&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Flash (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;SRAM (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;EEPROM (Bytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Packages&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      ATxmega64A3&lt;br&gt;
      ATxmega64A3U&lt;br&gt;
      ATxmega64B3&lt;br&gt;
      ATxmega64C3&lt;br&gt;
      ATxmega64D3&lt;br&gt;
      ATxmega128A3&lt;br&gt;
      ATxmega128A3U&lt;br&gt;
      ATxmega128B3&lt;br&gt;
      ATxmega128C3&lt;br&gt;
      ATxmega128D3&lt;br&gt;
      ATxmega192A3&lt;br&gt;
      ATxmega192A3U&lt;br&gt;
      ATxmega192C3&lt;br&gt;
      ATxmega192D3&lt;br&gt;
      ATxmega256A3&lt;br&gt;
      ATxmega256A3B&lt;br&gt;
      ATxmega256A3BU&lt;br&gt;
      ATxmega256A3U&lt;br&gt;
      ATxmega256C3&lt;br&gt;
      ATxmega256D3&lt;br&gt;
      ATxmega384C3&lt;br&gt;
      ATxmega384D3&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      192&lt;br&gt;
      192&lt;br&gt;
      192&lt;br&gt;
      192&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      256&lt;br&gt;
      384&lt;br&gt;
      384&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center nowrap&gt;&lt;font face=arial size=3&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      4096&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64,TQFP 64A 64&lt;br&gt;
      TQFP MF 64,VQFN (Sawn) PJ 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      TQFP MF 64,VQFN (Sawn) PJ 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M1 64,MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      TQFP MF 64,VQFN (Sawn) PJ 64&lt;br&gt;
      MLF (VQFN) 64M2 64,TQFP 64A 64&lt;br&gt;
      TQFP 64A 64,VQFN (Sawn) PJ 64&lt;br&gt;
      TQFP 64A 64,VQFN (Sawn) PJ 64&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td colspan=5 bgcolor="#cccccc"&gt;
      &lt;font color="#0000FF" size=3 face=arial&gt;&lt;b&gt;44-Pins Package&lt;/b&gt;&lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Devices Name&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Flash (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;SRAM (Kbytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#dddddd"&gt;		
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;EEPROM (Bytes)&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
    &lt;td align=center bgcolor="#eeeeee"&gt;
      &lt;b&gt;
      &lt;font size=3 face=arial color="#007FFF"&gt;Packages&lt;/font&gt;
      &lt;/b&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

  &lt;tr&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      ATxmega16A4&lt;br&gt;
      ATxmega16A4U&lt;br&gt;
      ATxmega16C4&lt;br&gt;
      ATxmega16D4&lt;br&gt;
      ATxmega32A4&lt;br&gt;
      ATxmega32A4U&lt;br&gt;
      ATxmega32C4&lt;br&gt;
      ATxmega32D4&lt;br&gt;
      ATxmega64A4U&lt;br&gt;
      ATxmega64D4&lt;br&gt;
      ATxmega128A4U&lt;br&gt;
      ATxmega128D4&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center&gt;&lt;font face=arial size=3&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      16&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      32&lt;br&gt;
      64&lt;br&gt;
      64&lt;br&gt;
      128&lt;br&gt;
      128&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      3.3&lt;br&gt;
      3.3&lt;br&gt;
      4&lt;br&gt;
      2&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      4&lt;br&gt;
      8&lt;br&gt;
      8&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#dddddd" align=center nowrap&gt;&lt;font face=arial size=3&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      1024&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      2048&lt;br&gt;
      &lt;/font&gt;
    &lt;/td&gt;
    &lt;td bgcolor="#eeeeee" align=center&gt;&lt;font face=arial size=3&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44,VFBGA 49C2 49&lt;br&gt;
      MLF (VQFN) 44M1 44,TQFP 44A 44&lt;br&gt;
     &lt;/font&gt;
    &lt;/td&gt;
  &lt;/tr&gt;

&lt;/table&gt;</description>
<packages>
<package name="TQFP-64A-64">
<description>&lt;b&gt;64A&lt;/b&gt;, 64-lead, 14 x 14 mm Body Size, 1.0 mm Body Thickness, 0.8 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="0805">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="rocket">
<packages>
<package name="2X3">
</package>
<package name="USB_MICRO_B">
</package>
<package name="SOT233">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="atmel-xmega" package="TQFP-64A-64" value="ATXMEGA128A3-AU">
<attribute name="NAME"/>
</element>
<element name="PORTA" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTB" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTC" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTD" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTE" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTF" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="10k"/>
<element name="C1" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C2" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C3" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C4" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C5" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C6" library="SparkFun" package="0805" value="0.1uF"/>
<element name="U$1" library="rocket" package="2X3" value="PDI"/>
<element name="U$2" library="rocket" package="USB_MICRO_B" value="USB"/>
<element name="U$3" library="rocket" package="SOT233" value="MCP1825S"/>
<element name="C7" library="SparkFun" package="0805" value="10uF"/>
<element name="C8" library="SparkFun" package="0805" value="10uF"/>
<element name="JP1" library="SparkFun" package="1X02" value=""/>
<element name="JP2" library="SparkFun" package="1X02" value=""/>
<element name="LED1" library="led" package="CHIP-LED0805" value=""/>
<element name="R2" library="SparkFun" package="0805" value="10k"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="61"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="45"/>
<contactref element="U1" pad="53"/>
<contactref element="JP2" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="U$3" pad="3"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="44"/>
<contactref element="U1" pad="52"/>
<contactref element="U1" pad="60"/>
<contactref element="U$3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="U$2" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="5"/>
<contactref element="U1" pad="57"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="DATA">
<contactref element="U1" pad="56"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="PC7">
<contactref element="PORTC" pad="8"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="PC6">
<contactref element="PORTC" pad="7"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="PC5">
<contactref element="PORTC" pad="6"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="PC4">
<contactref element="PORTC" pad="5"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="PC3">
<contactref element="PORTC" pad="4"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="PC2">
<contactref element="PORTC" pad="3"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="PC1">
<contactref element="PORTC" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="PC0">
<contactref element="PORTC" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="PB7">
<contactref element="PORTB" pad="8"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="PB6">
<contactref element="PORTB" pad="7"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="PB5">
<contactref element="PORTB" pad="6"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="PB4">
<contactref element="PORTB" pad="5"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="PB1">
<contactref element="PORTB" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="PB3">
<contactref element="PORTB" pad="4"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="PB0">
<contactref element="PORTB" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="PA7">
<contactref element="PORTA" pad="8"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="PA6">
<contactref element="PORTA" pad="7"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="PA5">
<contactref element="PORTA" pad="6"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="PA4">
<contactref element="PORTA" pad="5"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="PA3">
<contactref element="PORTA" pad="4"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="PA2">
<contactref element="PORTA" pad="3"/>
<contactref element="U1" pad="64"/>
</signal>
<signal name="PA1">
<contactref element="PORTA" pad="2"/>
<contactref element="U1" pad="63"/>
</signal>
<signal name="PA0">
<contactref element="PORTA" pad="1"/>
<contactref element="U1" pad="62"/>
</signal>
<signal name="PF0">
<contactref element="PORTF" pad="1"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="PF1">
<contactref element="PORTF" pad="2"/>
<contactref element="U1" pad="47"/>
</signal>
<signal name="PF2">
<contactref element="PORTF" pad="3"/>
<contactref element="U1" pad="48"/>
</signal>
<signal name="PF3">
<contactref element="PORTF" pad="4"/>
<contactref element="U1" pad="49"/>
</signal>
<signal name="PF4">
<contactref element="PORTF" pad="5"/>
<contactref element="U1" pad="50"/>
</signal>
<signal name="PF5">
<contactref element="PORTF" pad="6"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="PF6">
<contactref element="PORTF" pad="7"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="PF7">
<contactref element="PORTF" pad="8"/>
<contactref element="U1" pad="55"/>
</signal>
<signal name="PE0">
<contactref element="PORTE" pad="1"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="PE1">
<contactref element="PORTE" pad="2"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="PE2">
<contactref element="PORTE" pad="3"/>
<contactref element="U1" pad="38"/>
</signal>
<signal name="PE3">
<contactref element="PORTE" pad="4"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="PE4">
<contactref element="PORTE" pad="5"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="PE5">
<contactref element="PORTE" pad="6"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="PE6">
<contactref element="PORTE" pad="7"/>
<contactref element="U1" pad="42"/>
</signal>
<signal name="PE7">
<contactref element="PORTE" pad="8"/>
<contactref element="U1" pad="43"/>
</signal>
<signal name="PB2">
<contactref element="PORTB" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="PD0">
<contactref element="U1" pad="26"/>
<contactref element="PORTD" pad="1"/>
</signal>
<signal name="PD1">
<contactref element="U1" pad="27"/>
<contactref element="PORTD" pad="2"/>
</signal>
<signal name="PD2">
<contactref element="U1" pad="28"/>
<contactref element="PORTD" pad="3"/>
</signal>
<signal name="PD3">
<contactref element="U1" pad="29"/>
<contactref element="PORTD" pad="4"/>
</signal>
<signal name="PD4">
<contactref element="U1" pad="30"/>
<contactref element="PORTD" pad="5"/>
</signal>
<signal name="PD5">
<contactref element="U1" pad="31"/>
<contactref element="PORTD" pad="6"/>
</signal>
<signal name="PD6">
<contactref element="U1" pad="32"/>
<contactref element="PORTD" pad="7"/>
</signal>
<signal name="PD7">
<contactref element="U1" pad="33"/>
<contactref element="PORTD" pad="8"/>
</signal>
<signal name="N$3">
</signal>
<signal name="RAW">
<contactref element="U$3" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
