<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="theairboard">
<description>&lt;h3&gt;The AirBoard®&lt;/h3&gt; is a thumb-size, Arduino-compatible, wireless,
ubiquitous computer designed to sketch Internet-of-Things, fast!
&lt;br&gt;&lt;br&gt;
Visit &lt;b&gt;http://www.theairboard.cc&lt;/b&gt;</description>
<packages>
<package name="SIL-1X10">
<description>&lt;b&gt;Single In Line 2.54mm header - 10 pins&lt;/b&gt;</description>
</package>
<package name="LAYOUT">
<description>25x25mm board template</description>
</package>
<package name="BRD_FRAME">
<description>&lt;b&gt;Board frame&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="DESIGNER" value="theairboard.cc"/>
<attribute name="REV" value="1.0"/>
<attribute name="SENSOR" value=""/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="theairboard" package="SIL-1X10" value="SIL">
<attribute name="OC_NEWARK" value="93K5133"/>
<attribute name="MANUFACTURER" value="FCI"/>
<attribute name="OC_FARNELL" value="1097958"/>
<attribute name="PART_NUMBER" value="77315-818-36LF "/>
</element>
<element name="FRAME1" library="theairboard" package="LAYOUT" value="SCH_FRAME"/>
<element name="U$1" library="theairboard" package="BRD_FRAME" value=""/>
</elements>
<signals>
<signal name="S$2">
<contactref element="JP1" pad="9"/>
</signal>
<signal name="S$3">
<contactref element="JP1" pad="8"/>
</signal>
<signal name="S$4">
<contactref element="JP1" pad="7"/>
</signal>
<signal name="S$5">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="S$6">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="S$7">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="S$8">
<contactref element="JP1" pad="3"/>
</signal>
<signal name="S$9">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="S$10">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="S$11">
</signal>
<signal name="S$12">
</signal>
<signal name="S$13">
</signal>
<signal name="S$14">
</signal>
<signal name="S$15">
</signal>
<signal name="S$16">
</signal>
<signal name="S$17">
</signal>
<signal name="S$18">
</signal>
<signal name="S$19">
</signal>
<signal name="S$20">
</signal>
<signal name="S$21">
</signal>
<signal name="S$22">
</signal>
<signal name="S$23">
</signal>
<signal name="S$24">
</signal>
<signal name="S$25">
</signal>
<signal name="S$26">
</signal>
<signal name="S$27">
</signal>
<signal name="S$28">
</signal>
<signal name="S$29">
</signal>
<signal name="S$30">
</signal>
<signal name="S$31">
</signal>
<signal name="S$32">
</signal>
<signal name="S$33">
</signal>
<signal name="S$34">
</signal>
<signal name="S$35">
</signal>
<signal name="S$36">
</signal>
<signal name="S$37">
</signal>
<signal name="S$38">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$41">
</signal>
<signal name="S$42">
</signal>
<signal name="S$43">
</signal>
<signal name="S$44">
</signal>
<signal name="S$45">
</signal>
<signal name="S$46">
</signal>
<signal name="S$56">
<contactref element="JP1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
