<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="15.494" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="38.354" y2="0" width="0.2032" layer="20"/>
<wire x1="38.354" y1="0" x2="38.354" y2="15.494" width="0.2032" layer="20"/>
<wire x1="38.354" y1="15.494" x2="0" y2="15.494" width="0.2032" layer="20"/>
<text>Close</text>
<text>BLK</text>
<text>DTR</text>
<text>David Merges</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>5V</text>
<text>3V3</text>
<text>hackerspace-ffm.de</text>
<text>v1.0</text>
<text>3V3</text>
<text>isolated versatile FTDI</text>
<text>VCC</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>DTR</text>
<text>CTS</text>
<text>5V</text>
<text>5Vsw</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED-0603">
</package>
<package name="1X06-SMD-FEMALE-V2">
<description>Package for 4UCONN part #19686 *UNPROVEN*</description>
</package>
<package name="1X01">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="1X06">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="MyEagleLibrary">
<packages>
<package name="SO-16W">
</package>
<package name="SRV05-SOT23">
</package>
<package name="USB_MICROAB">
</package>
<package name="PTC-1812">
</package>
<package name="SS_SSK-1202">
</package>
<package name="PWR_SWITCH_SOT23-5">
</package>
<package name="SOT23-3PIN">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
</packages>
</library>
<library name="hackffm_logo">
<packages>
<package name="LOGO_BSTOP">
</package>
<package name="LOGO_TPLACE_TSTOP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="MyEagleLibrary" package="USB_MICROAB" value="USB+SHIELD">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun" package="SSOP28DB" value="FT232RLSSOP"/>
<element name="R1" library="rcl" package="R0603" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_TX" library="SparkFun" package="LED-0603" value="red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_RX" library="SparkFun" package="LED-0603" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X06-SMD-FEMALE-V2" value=""/>
<element name="U$5" library="MyEagleLibrary" package="SO-16W" value="ADUM_1402"/>
<element name="C3" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="C4" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="JP2" library="SparkFun" package="1X06" value=""/>
<element name="C6" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="C7" library="rcl" package="C0805K" value="220nF X7R"/>
<element name="R3" library="rcl" package="R0805" value="330"/>
<element name="U$2" library="MyEagleLibrary" package="SRV05-SOT23" value="SRV05"/>
<element name="JP5" library="SparkFun" package="1X01" value="M01PTH"/>
<element name="JP6" library="SparkFun" package="1X01" value="M01PTH"/>
<element name="SJ_VBUS" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE"/>
<element name="F1" library="MyEagleLibrary" package="PTC-1812" value="PTC_FUSE"/>
<element name="SJ_VE1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="S1" library="MyEagleLibrary" package="SS_SSK-1202" value="SS_SMD402"/>
<element name="C10" library="rcl" package="C0603K" value="10uF"/>
<element name="C11" library="rcl" package="C0603K" value="10uF"/>
<element name="R4" library="rcl" package="R0603" value="2K2"/>
<element name="LED_5V" library="SparkFun" package="LED-0603" value="red"/>
<element name="R5" library="rcl" package="R0603" value="1K"/>
<element name="LED_3V3" library="SparkFun" package="LED-0603" value="orange"/>
<element name="U$9" library="MyEagleLibrary" package="PWR_SWITCH_SOT23-5" value="PWR_SWITCH_SOT23-5"/>
<element name="U$11" library="MyEagleLibrary" package="PWR_SWITCH_SOT23-5" value="PWR_SWITCH_SOT23-5"/>
<element name="SJ_V+" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE"/>
<element name="R6" library="rcl" package="R0603" value="10K"/>
<element name="R7" library="rcl" package="R0603" value="1K"/>
<element name="C1" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="C8" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="Q1" library="MyEagleLibrary" package="SOT23-3PIN" value="P-CHANNEL_MOSFETIRLML2244TRPBF"/>
<element name="JP3" library="SparkFun" package="1X01" value="M01PTH"/>
<element name="C9" library="rcl" package="C1206K" value="10uF"/>
<element name="SJ_5V_SW" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE"/>
<element name="U$10" library="hackffm_logo" package="LOGO_BSTOP" value="HACKFFM_LOGOLOGO_STOP"/>
<element name="SJ_V+_5V" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE"/>
<element name="SJ_V+_3V3" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="U$7" library="hackffm_logo" package="LOGO_TPLACE_TSTOP" value="HACKFFM_LOGOLOGO_TPLACE_TSTOP"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C12" library="rcl" package="C0603K" value="10uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="X2" pad="GND"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="21"/>
<contactref element="U$5" pad="8"/>
<contactref element="U$5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="U$9" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="D-">
<contactref element="X2" pad="D-"/>
<contactref element="U1" pad="16"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="D+">
<contactref element="X2" pad="D+"/>
<contactref element="U1" pad="15"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="CTS">
<contactref element="U1" pad="11"/>
<contactref element="U$5" pad="6"/>
</signal>
<signal name="DTR">
<contactref element="U1" pad="2"/>
<contactref element="U$5" pad="4"/>
</signal>
<signal name="TXLED">
<contactref element="U1" pad="23"/>
<contactref element="LED_TX" pad="C"/>
</signal>
<signal name="RXLED">
<contactref element="U1" pad="22"/>
<contactref element="LED_RX" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED_TX" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED_RX" pad="A"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="1"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="5"/>
<contactref element="U$5" pad="5"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="20"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="JP5" pad="1"/>
<contactref element="F1" pad="P$3"/>
<contactref element="SJ_VBUS" pad="2"/>
<contactref element="U$9" pad="5"/>
<contactref element="Q1" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="SJ_5V_SW" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="V+">
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="U$11" pad="5"/>
<contactref element="SJ_V+" pad="2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="TX2">
<contactref element="U$5" pad="14"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$10">
<contactref element="C7" pad="2"/>
<contactref element="X2" pad="MT2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="X2" pad="MT1"/>
</signal>
<signal name="I/O3">
<contactref element="U$2" pad="4"/>
</signal>
<signal name="VBUS">
<contactref element="SJ_VBUS" pad="1"/>
<contactref element="U$9" pad="1"/>
<contactref element="U$9" pad="3"/>
<contactref element="F1" pad="P$2"/>
<contactref element="U$2" pad="5"/>
<contactref element="X2" pad="VBUS"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$5" pad="7"/>
<contactref element="SJ_VE1" pad="2"/>
</signal>
<signal name="(FAULT/)">
<contactref element="U$9" pad="4"/>
</signal>
<signal name="VDD2">
<contactref element="C4" pad="1"/>
<contactref element="U$5" pad="16"/>
<contactref element="C10" pad="1"/>
<contactref element="SJ_V+" pad="1"/>
<contactref element="U$11" pad="1"/>
<contactref element="U$11" pad="3"/>
<contactref element="S1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="SJ_V+_5V" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="U$5" pad="9"/>
<contactref element="U$5" pad="15"/>
<contactref element="C4" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="U$11" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="SJ_V+_3V3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="DTR2">
<contactref element="U$5" pad="13"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="RX2">
<contactref element="U$5" pad="12"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="CTS2">
<contactref element="U$5" pad="11"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VSEL">
<contactref element="U$5" pad="10"/>
<contactref element="S1" pad="C"/>
<contactref element="SJ_V+_3V3" pad="2"/>
<contactref element="SJ_V+_5V" pad="2"/>
<contactref element="LED_3V3" pad="C"/>
<contactref element="LED_5V" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="U$11" pad="4"/>
</signal>
<signal name="PWREN">
<contactref element="U1" pad="14"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="5V_SWITCHED">
<contactref element="Q1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="SJ_VE1" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="SJ_5V_SW" pad="1"/>
</signal>
<signal name="I/O4">
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="1"/>
<contactref element="LED_3V3" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="LED_5V" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
