<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="26.7462" x2="32.48025" y2="26.7462" width="0.02031875" layer="20"/>
<wire x1="32.48025" y1="26.7462" x2="32.48025" y2="0" width="0.02031875" layer="20"/>
<wire x1="32.48025" y1="0" x2="0" y2="0" width="0.02031875" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="26.7462" width="0.02031875" layer="20"/>
<text>-   +</text>
<text>&lt;c&gt; Fahd Muhib</text>
<text>CellBoost</text>
<text>REV A</text>
<text>LT1302</text>
<text>3/2014</text>
<hole x="3.01625" y="23.65375" drill="3.6"/>
<hole x="29.36875" y="23.65375" drill="3.6"/>
<text>                                                          
                                                           
                                                       
                  ___                   
                 / () \\               
                _|_____|_            
                | | === | |             
                |_|  0  |_|              
                 ||  0  ||                
                 ||__*__||                 
                |~\\___/~|               
               /=\\/=\\/=\\                
            ___[_] [_] [_]___</text>
<text>              /~\\                                         
             ( 00|                                        
             _\\=/_                                      
            /  _  \\               
           //| /.\\ |\\\\            
           | |  \\/  | |          
           | | |   | | |          
           #  \\_/  #        
              | | |            
              | | |              
              []|[]             
              | | |             
        _____/]_[\\____</text>
<text>[ Did you hear that? ]
   /
  /
 
  </text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="R805">
</package>
<package name="CONN_USB_A_F">
<description>USB AF SMD &lt;br&gt;
Mfr no. AU-Y1006-2-R&lt;br&gt;
&lt;a href="http://www.digikey.com/product-detail/en/AU-Y1006-2-R/AE10332-ND/2077795"&gt; Digikey &lt;/a&gt;</description>
</package>
<package name="M1X2">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="SO08-SKINNYPADS">
</package>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MyPARTS">
<packages>
<package name="10UH_SMD_BOURNS">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="dp_devices" package="R805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="153CLV-0810" value="220uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="153CLV-0810" value="220uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="dp_devices" package="R805" value="75K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="dp_devices" package="R805" value="75K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="adafruit" package="SO08-SKINNYPADS" value="LT1302S8">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="dp_devices" package="R805" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="dp_devices" package="R805" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="dp_devices" package="R805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="dp_devices" package="R805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="dp_devices" package="CONN_USB_A_F" value="CON-USB-F-2PB"/>
<element name="L2" library="MyPARTS" package="10UH_SMD_BOURNS" value="10uH">
<attribute name="NAME"/>
</element>
<element name="D1" library="adafruit" package="SMADIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="dp_devices" package="R805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="dp_devices" package="R805" value="200pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2.5-7.0V" library="dp_devices" package="M1X2" value="CON_HEADER_1X02-PTH">
<attribute name="NAME"/>
</element>
<element name="DATA" library="testpad" package="B1,27" value="TPSB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW" library="testpad" package="B1,27" value="TPSB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BATT" library="testpad" package="B1,27" value="TPSB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VC" library="testpad" package="B1,27" value="TPSB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="testpad" package="B1,27" value="TPSB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C4" pad="-"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="USB1" pad="4"/>
<contactref element="IC1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="2.5-7.0V" pad="2"/>
<contactref element="GND" pad="TP"/>
</signal>
<signal name="D-">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="USB1" pad="2"/>
<contactref element="DATA" pad="TP"/>
</signal>
<signal name="D+">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="USB1" pad="3"/>
</signal>
<signal name="NODE1">
<contactref element="IC1" pad="7"/>
<contactref element="L2" pad="P$2"/>
<contactref element="D1" pad="A"/>
<contactref element="SW" pad="TP"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="+"/>
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="USB1" pad="1"/>
</signal>
<signal name="BATT+">
<contactref element="IC1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="+"/>
<contactref element="L2" pad="P$1"/>
<contactref element="2.5-7.0V" pad="1"/>
<contactref element="BATT" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="VC" pad="TP"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
