<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>+ side up</text>
<text>ATTinier84</text>
<text>ATTinier84</text>
<text>ATTinier84</text>
<text>ATTinier84</text>
<text>&gt;REVISION</text>
<text>&gt;REVISION</text>
<text>&gt;REVISION</text>
<text>&gt;REVISION</text>
</plain>
<libraries>
<library name="A_butts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="DIL14">
</package>
<package name="RESISTOR-AXIAL-PTH-7.62MM">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="TACTILE-PTH-SIDE">
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="ATTINIER84_SHIELD2">
</package>
<package name="SPDT-RA-2.54MM">
</package>
<package name="CC-BY-SA-4.0-NO-URL">
</package>
<package name="COW_SMALL">
</package>
<package name="BATTCON_20MM_PTH_TOPLOAD">
</package>
<package name="2X3">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REVISION" value="v1.0"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="A_butts" package="DUMMY" value="">
<attribute name="VERSION" value=""/>
<attribute name="DESIGNER" value="Nobody"/>
</element>
<element name="IC1" library="A_butts" package="DIL14" value="ATTiny84">
<attribute name="VALUE"/>
</element>
<element name="R1" library="A_butts" package="RESISTOR-AXIAL-PTH-7.62MM" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="A_butts" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="A_butts" package="TACTILE-PTH-SIDE" value="SPST-NO-TACT3MM-RA">
<attribute name="NAME"/>
</element>
<element name="U1" library="A_butts" package="ATTINIER84_SHIELD2" value="ATTINIER84_SHIELD1551G"/>
<element name="PWR" library="A_butts" package="SPDT-RA-2.54MM" value="SWITCH-SPDTPTH-RA-2.54MM">
<attribute name="NAME"/>
</element>
<element name="U$1" library="A_butts" package="CC-BY-SA-4.0-NO-URL" value=""/>
<element name="U$2" library="A_butts" package="COW_SMALL" value=""/>
<element name="BATT" library="A_butts" package="BATTCON_20MM_PTH_TOPLOAD" value="CR2032">
<attribute name="VALUE"/>
</element>
<element name="AVRISP" library="A_butts" package="2X3" value="AVR_SPI_PRG_6PTH">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="U1" pad="GND@2"/>
<contactref element="U1" pad="GND@1"/>
<contactref element="BATT" pad="-"/>
<contactref element="AVRISP" pad="6"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U1" pad="VCC"/>
<contactref element="PWR" pad="3"/>
<contactref element="AVRISP" pad="2"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="RST"/>
<contactref element="RST" pad="2"/>
<contactref element="AVRISP" pad="5"/>
</signal>
<signal name="PA7">
<contactref element="IC1" pad="6"/>
<contactref element="U1" pad="PA7"/>
</signal>
<signal name="PA6">
<contactref element="IC1" pad="7"/>
<contactref element="U1" pad="PA6"/>
<contactref element="AVRISP" pad="4"/>
</signal>
<signal name="PA5">
<contactref element="IC1" pad="8"/>
<contactref element="U1" pad="PA5"/>
<contactref element="AVRISP" pad="1"/>
</signal>
<signal name="PA4">
<contactref element="IC1" pad="9"/>
<contactref element="U1" pad="PA4"/>
<contactref element="AVRISP" pad="3"/>
</signal>
<signal name="PA3">
<contactref element="IC1" pad="10"/>
<contactref element="U1" pad="PA3"/>
</signal>
<signal name="PA2">
<contactref element="IC1" pad="11"/>
<contactref element="U1" pad="PA2"/>
</signal>
<signal name="PA1">
<contactref element="IC1" pad="12"/>
<contactref element="U1" pad="PA1"/>
</signal>
<signal name="PA0">
<contactref element="IC1" pad="13"/>
<contactref element="U1" pad="PA0"/>
</signal>
<signal name="PB0">
<contactref element="IC1" pad="2"/>
<contactref element="U1" pad="PB0"/>
</signal>
<signal name="PB1">
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="PB1"/>
</signal>
<signal name="PB2">
<contactref element="IC1" pad="5"/>
<contactref element="U1" pad="PB2"/>
</signal>
<signal name="N$1">
<contactref element="PWR" pad="2"/>
<contactref element="BATT" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
