<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="55.55" y2="0" width="0" layer="20"/>
<wire x1="55.88" y1="0" x2="55.88" y2="57.15" width="0" layer="20"/>
<wire x1="55.88" y1="57.15" x2="0" y2="57.15" width="0" layer="20"/>
<wire x1="0" y1="57.15" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="DIODE-1N4148">
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X04_LOCK">
</package>
<package name="DIL28-3-SIMON">
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="DIODE-1N4001">
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="AVRISP">
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F126Z12">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 3 mm, horizontal, grid 12.7 mm</description>
</package>
</packages>
</library>
<library name="Qxd">
<packages>
<package name="DCDC_SIP">
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="inductor-neosid">
<description>&lt;b&gt;Neosid Chokes and Transformers&lt;/b&gt;&lt;p&gt;

Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Electronic Component Book, Part 2 : Chokes, Fixed Value Inductors
&lt;li&gt;Part 3 : Filters, Coil Assemblies, Thermoplastic Parts
&lt;li&gt;Part 4 : SMD Filters, Coils, Fixed Value Inductors
&lt;li&gt;www.neosid.de
&lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BS11">
<description>NOMINAL &lt;b&gt;INDUCTANCE&lt;/b&gt;&lt;p&gt;
grid 5 mm, diameter 10.5 mm, height 13.5 mm</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<packages>
<package name="TO18">
<description>&lt;b&gt;TO 18&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C025-024X044" value="22pf"/>
<element name="C14" library="resistor" package="C025-025X050" value="0.1uf"/>
<element name="C15" library="resistor" package="C025-025X050" value="0.1uf"/>
<element name="C16" library="resistor" package="E2,5-7" value="33uf"/>
<element name="C17" library="resistor" package="E2,5-7" value="100uf"/>
<element name="C2" library="adafruit" package="C025-024X044" value="22pf"/>
<element name="C3" library="adafruit" package="C025-024X044" value="1uf"/>
<element name="C4" library="adafruit" package="C025-024X044" value=".1uf"/>
<element name="C5" library="adafruit" package="C025-024X044" value="1uf"/>
<element name="C6" library="adafruit" package="C025-024X044" value="2.2uf"/>
<element name="D1" library="SparkFun" package="DIODE-1N4148" value="1N4148"/>
<element name="D7" library="diode" package="F126Z12" value="B220/A"/>
<element name="DCDC" library="Qxd" package="DCDC_SIP" value="D107E"/>
<element name="FTDI" library="SparkFun" package="1X06_LOCK" value=""/>
<element name="I2C" library="SparkFun" package="1X04_LOCK" value=""/>
<element name="IC1" library="SparkFun" package="DIL28-3-SIMON" value="AVR-MEGA8-PSIM"/>
<element name="IC2" library="SparkFun" package="DIP08" value="LF353"/>
<element name="IC7" library="ic-package" package="DIL08" value="MAX5033-5"/>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="L3" library="inductor-neosid" package="BS11" value="220uh">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="Q2" library="transistor-npn" package="TO18" value="2N2222A"/>
<element name="R1" library="adafruit" package="0204/7" value="1k 1%"/>
<element name="R10" library="adafruit" package="0204/7" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="0204/7" value="330"/>
<element name="R2" library="adafruit" package="0204/7" value="2.5k"/>
<element name="R21" library="resistor" package="0204/7" value="1M"/>
<element name="R22" library="resistor" package="0204/7" value="274k"/>
<element name="R3" library="adafruit" package="0204/7" value="2.5k"/>
<element name="R5" library="adafruit" package="0204/7" value="56k"/>
<element name="R6" library="adafruit" package="0204/7" value="100k"/>
<element name="R7" library="adafruit" package="0204/7" value="200k"/>
<element name="R8" library="adafruit" package="0204/7" value="100k"/>
<element name="R9" library="adafruit" package="0204/7" value="100k"/>
<element name="RELAY" library="SparkFun" package="SCREWTERMINAL-3.5MM-2_LOCK" value="TE 1776275-2"/>
<element name="TVS" library="SparkFun" package="DIODE-1N4001" value="P6KE16CA"/>
<element name="Y1" library="SparkFun" package="HC49U-V" value="16000mhz"/>
<element name="DC_LINE-IN-12V" library="SparkFun" package="SCREWTERMINAL-5MM-2" value="gnd">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PILOT" library="SparkFun" package="SCREWTERMINAL-3.5MM-2_LOCK" value="TE 1776275-2"/>
</elements>
<signals>
<signal name="+5V">
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="7"/>
<contactref element="ISP1" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="FTDI" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="I2C" pad="2"/>
<contactref element="C16" pad="+"/>
<contactref element="L3" pad="1"/>
<contactref element="IC7" pad="4"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="22"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="ISP1" pad="6"/>
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="TVS" pad="A"/>
<contactref element="R8" pad="1"/>
<contactref element="FTDI" pad="1"/>
<contactref element="DCDC" pad="VIN-"/>
<contactref element="DCDC" pad="GND"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="I2C" pad="1"/>
<contactref element="C17" pad="-"/>
<contactref element="D7" pad="A"/>
<contactref element="C16" pad="-"/>
<contactref element="IC7" pad="6"/>
<contactref element="C15" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="IC7" pad="3"/>
<contactref element="DC_LINE-IN-12V" pad="1"/>
<contactref element="PILOT" pad="1"/>
</signal>
<signal name="RST">
<contactref element="ISP1" pad="5"/>
<contactref element="IC1" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C1" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="2"/>
<contactref element="Y1" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="PILOT">
<contactref element="TVS" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="PILOT" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="Q2" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="RELAY" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="ISP1" pad="4"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="N$15">
<contactref element="ISP1" pad="3"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$34">
<contactref element="IC1" pad="14"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="IC1" pad="24"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="D1" pad="C"/>
<contactref element="RELAY" pad="1"/>
<contactref element="DCDC" pad="VIN+"/>
<contactref element="C6" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="IC7" pad="7"/>
<contactref element="C17" pad="+"/>
<contactref element="DC_LINE-IN-12V" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="21"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="3"/>
<contactref element="FTDI" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="2"/>
<contactref element="FTDI" pad="4"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="ISP1" pad="1"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="S$2">
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="PD3">
<contactref element="IC1" pad="5"/>
</signal>
<signal name="PD4">
<contactref element="IC1" pad="6"/>
</signal>
<signal name="PLOW">
<contactref element="DCDC" pad="VOUT-"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="PHIGH">
<contactref element="DCDC" pad="VOUT+"/>
<contactref element="R2" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
<contactref element="I2C" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
<contactref element="I2C" pad="3"/>
</signal>
<signal name="PD6">
<contactref element="IC1" pad="12"/>
</signal>
<signal name="BST">
<contactref element="IC7" pad="1"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="LX">
<contactref element="C14" pad="2"/>
<contactref element="IC7" pad="8"/>
<contactref element="D7" pad="C"/>
<contactref element="L3" pad="2"/>
</signal>
<signal name="ON/OFF">
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="VD">
<contactref element="IC7" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
