<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="-0.3175" y1="0" x2="12.6875" y2="0" width="0" layer="20"/>
<wire x1="12.6875" y1="0" x2="12.6875" y2="22.5325" width="0" layer="20"/>
<wire x1="12.6875" y1="22.5325" x2="-0.3175" y2="22.5325" width="0" layer="20"/>
<wire x1="-0.3175" y1="22.5325" x2="-0.3175" y2="0" width="0" layer="20"/>
<wire x1="12.7" y1="0" x2="22.86" y2="0" width="0" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="22.5425" width="0" layer="20"/>
<wire x1="22.86" y1="22.5425" x2="12.7" y2="22.5425" width="0" layer="20"/>
<wire x1="12.7" y1="22.5425" x2="12.7" y2="12.7" width="0" layer="20"/>
<hole x="12.7" y="0.635" drill="0.5"/>
<hole x="12.7" y="1.5875" drill="0.5"/>
<hole x="12.7" y="2.54" drill="0.5"/>
<hole x="12.7" y="3.4925" drill="0.5"/>
<hole x="12.7" y="4.445" drill="0.5"/>
<hole x="12.7" y="5.3975" drill="0.5"/>
<hole x="12.7" y="6.35" drill="0.5"/>
<hole x="12.7" y="7.3025" drill="0.5"/>
<hole x="12.7" y="8.255" drill="0.5"/>
<hole x="12.7" y="9.2075" drill="0.5"/>
<hole x="12.7" y="10.16" drill="0.5"/>
<hole x="12.7" y="11.1125" drill="0.5"/>
<hole x="12.7" y="12.065" drill="0.5"/>
<hole x="12.7" y="13.0175" drill="0.5"/>
<hole x="12.7" y="13.97" drill="0.5"/>
<hole x="12.7" y="14.9225" drill="0.5"/>
<hole x="12.7" y="15.875" drill="0.5"/>
<hole x="12.7" y="16.8275" drill="0.5"/>
<hole x="12.7" y="17.78" drill="0.5"/>
<hole x="12.7" y="18.7325" drill="0.5"/>
<hole x="12.7" y="19.685" drill="0.5"/>
<hole x="12.7" y="20.6375" drill="0.5"/>
<hole x="12.7" y="21.59" drill="0.5"/>
</plain>
<libraries>
<library name="con-lstb">
<packages>
<package name="MA04-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="lex_etl">
<packages>
<package name="RF_BRD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SPI-1" library="con-lstb" package="MA04-2" value="MA04-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="lex_etl" package="RF_BRD" value="CC2500_BRD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value=""/>
<element name="U2" library="lex_etl" package="RF_BRD" value="CC2500_BRD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="SPI-1" pad="1"/>
<contactref element="U1" pad="VDD"/>
</signal>
<signal name="GND">
<contactref element="SPI-1" pad="6"/>
<contactref element="U1" pad="GND"/>
</signal>
<signal name="SI1">
<contactref element="SPI-1" pad="2"/>
<contactref element="U1" pad="SI"/>
</signal>
<signal name="SO1">
<contactref element="SPI-1" pad="4"/>
<contactref element="U1" pad="SO"/>
</signal>
<signal name="SCKL1">
<contactref element="SPI-1" pad="3"/>
<contactref element="U1" pad="SCLK"/>
</signal>
<signal name="GDO21">
<contactref element="SPI-1" pad="5"/>
<contactref element="U1" pad="GDIO2"/>
</signal>
<signal name="CS1">
<contactref element="SPI-1" pad="8"/>
<contactref element="U1" pad="CSN"/>
</signal>
<signal name="GDO01">
<contactref element="SPI-1" pad="7"/>
<contactref element="U1" pad="GDIO0"/>
</signal>
<signal name="GND1">
<contactref element="U2" pad="GND"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="U2" pad="VDD"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="3"/>
<contactref element="U2" pad="SI"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="4"/>
<contactref element="U2" pad="SCLK"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="5"/>
<contactref element="U2" pad="SO"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="6"/>
<contactref element="U2" pad="GDIO2"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="7"/>
<contactref element="U2" pad="GDIO0"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="CSN"/>
<contactref element="JP1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
