<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="38.735" x2="48" y2="38.735" width="0" layer="20"/>
<wire x1="48" y1="38.735" x2="48" y2="80" width="0" layer="20"/>
<wire x1="48" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="38.735" width="0" layer="20"/>
<text>Gigahearts_FX
LD-2  v2.1c</text>
<text>Layout by AP
(c)2014 
</text>
</plain>
<libraries>
<library name="mb_supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="mb_resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="mb_caps-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
<package name="072X045">
<description>&lt;b&gt;7.2mm x 4.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKP2, MKS2</description>
</package>
</packages>
</library>
<library name="mb_ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mb_9mm Pot">
<packages>
<package name="POT_9MM_PACK">
</package>
</packages>
</library>
<library name="mb_switches">
<description>&lt;b&gt;Switches&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;SPST, SPDT, DPDT, 3PDT
&lt;/ul&gt;</description>
<packages>
<package name="M9040P">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
</package>
</packages>
</library>
<library name="mb_caps-electro">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="080_035_2">
<description>&lt;b&gt;8mm diameter, 3.5mm lead spacing, 0.2" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mb_diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="DO35-2">
<description>&lt;b&gt;DO-35 0.2" pad spacing&lt;/b&gt;</description>
</package>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN1" library="mb_supply" package="SQUARE" value="IN(T)"/>
<element name="R1" library="mb_resistors" package="R0207/3" value="1M"/>
<element name="C1" library="mb_caps-box" package="072X025" value="22n"/>
<element name="R2" library="mb_resistors" package="R0207/3" value="1k"/>
<element name="C2" library="mb_caps-box" package="072X025" value="1n"/>
<element name="R3" library="mb_resistors" package="R0207/3" value="1m"/>
<element name="IC1" library="mb_ics" package="DIL08" value="TL072P"/>
<element name="C3" library="mb_caps-box" package="072X025" value="100p"/>
<element name="R4" library="mb_resistors" package="R0207/3" value="3.3k"/>
<element name="C4" library="mb_caps-box" package="072X025" value="220n"/>
<element name="GAIN" library="mb_9mm Pot" package="POT_9MM_PACK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="mb_resistors" package="R0207/3" value="10k"/>
<element name="C5" library="mb_caps-box" package="072X025" value="100n"/>
<element name="C6" library="mb_caps-box" package="072X025" value="100p"/>
<element name="R6" library="mb_resistors" package="R0207/3" value="470k"/>
<element name="C7" library="mb_caps-box" package="072X045" value="1uF"/>
<element name="R7" library="mb_resistors" package="R0207/3" value="470r"/>
<element name="SW1" library="mb_switches" package="M9040P" value=""/>
<element name="C8" library="mb_caps-box" package="072X045" value="1uF"/>
<element name="C9" library="mb_caps-box" package="072X025" value="47n"/>
<element name="R8" library="mb_resistors" package="R0207/3" value="10k"/>
<element name="R9" library="mb_resistors" package="R0207/3" value="2.2k"/>
<element name="TONE" library="mb_9mm Pot" package="POT_9MM_PACK" value=""/>
<element name="R10" library="mb_resistors" package="R0207/3" value="2.2k"/>
<element name="C10" library="mb_caps-box" package="072X025" value="47n"/>
<element name="R11" library="mb_resistors" package="R0207/3" value="10k"/>
<element name="IC2" library="mb_ics" package="DIL08" value="TL072P"/>
<element name="C11" library="mb_caps-box" package="072X045" value="1uF"/>
<element name="R12" library="mb_resistors" package="R0207/3" value="0k"/>
<element name="VOLUME" library="mb_9mm Pot" package="POT_9MM_PACK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="mb_supply" package="SQUARE" value="OUT(T)"/>
<element name="+9V1" library="mb_supply" package="SQUARE" value="+9V(T)"/>
<element name="C12" library="mb_caps-electro" package="080_035_2" value="100uF"/>
<element name="R13" library="mb_resistors" package="R0207/3" value="22k"/>
<element name="R14" library="mb_resistors" package="R0207/3" value="22k"/>
<element name="GND6" library="mb_supply" package="SQUARE" value="GND(T)"/>
<element name="GND7" library="mb_supply" package="SQUARE" value="GND(T)"/>
<element name="D1" library="mb_diodes" package="LED3MM" value="LED3MM"/>
<element name="D2" library="mb_diodes" package="LED3MM" value="LED3MM"/>
<element name="D3" library="mb_diodes" package="DO35-2" value="1N4148-2"/>
<element name="D4" library="mb_diodes" package="DO35-2" value="1N4148-2"/>
<element name="D5" library="mb_diodes" package="DO41-3" value="1n4001"/>
</elements>
<signals>
<signal name="IN">
<contactref element="IN1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="VOLUME" pad="P$1"/>
<contactref element="R14" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="C12" pad="-"/>
<contactref element="GND6" pad="1"/>
<contactref element="GND7" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="VB">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="GAIN" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="GAIN" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="GAIN" pad="P$3"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="6"/>
<contactref element="R5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="C6" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="R6" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C7" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="2"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="2"/>
<contactref element="SW1" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R9" pad="1"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R9" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R10" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="C10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="TONE" pad="P$2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="C11" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R12" pad="2"/>
<contactref element="VOLUME" pad="P$3"/>
</signal>
<signal name="OUT">
<contactref element="VOLUME" pad="P$2"/>
<contactref element="OUT1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="S$2">
<contactref element="IC2" pad="8"/>
<contactref element="R13" pad="2"/>
<contactref element="+9V1" pad="1"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="+9V">
<contactref element="IC1" pad="8"/>
<contactref element="C12" pad="+"/>
</signal>
<signal name="N$23">
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="A"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="S$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
