<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="0" y2="15.24" width="0.254" layer="20"/>
<wire x1="0" y1="15.24" x2="1.27" y2="16.51" width="0.254" layer="20" curve="-90"/>
<wire x1="1.27" y1="16.51" x2="39.37" y2="16.51" width="0.254" layer="20"/>
<wire x1="39.37" y1="16.51" x2="40.64" y2="15.24" width="0.254" layer="20" curve="-90"/>
<wire x1="1.27" y1="0" x2="39.37" y2="0" width="0.254" layer="20"/>
<wire x1="39.37" y1="0" x2="40.64" y2="1.27" width="0.254" layer="20" curve="90"/>
<wire x1="40.64" y1="1.27" x2="40.64" y2="15.24" width="0.254" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0.254" layer="20" curve="90"/>
<text>COLOUR PALETTE</text>
<text>LED PCB</text>
</plain>
<libraries>
<library name="DIYRE">
<packages>
<package name="LED-RGB">
</package>
<package name="CON-.100-12">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="DIYRE" package="LED-RGB" value="LED-RGB">
<attribute name="NAME"/>
</element>
<element name="LED2" library="DIYRE" package="LED-RGB" value="LED-RGB">
<attribute name="NAME"/>
</element>
<element name="LED3" library="DIYRE" package="LED-RGB" value="LED-RGB">
<attribute name="NAME"/>
</element>
<element name="CON1" library="DIYRE" package="CON-.100-12" value="CON-.100-12PIN">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$35">
<contactref element="LED1" pad="AR1"/>
<contactref element="CON1" pad="P$1"/>
</signal>
<signal name="N$36">
<contactref element="LED1" pad="AG1"/>
<contactref element="CON1" pad="P$2"/>
</signal>
<signal name="N$37">
<contactref element="LED1" pad="AB1"/>
<contactref element="CON1" pad="P$3"/>
</signal>
<signal name="N$38">
<contactref element="LED1" pad="K1"/>
<contactref element="CON1" pad="P$4"/>
</signal>
<signal name="N$39">
<contactref element="LED2" pad="AR1"/>
<contactref element="CON1" pad="P$5"/>
</signal>
<signal name="N$40">
<contactref element="LED2" pad="AG1"/>
<contactref element="CON1" pad="P$6"/>
</signal>
<signal name="N$41">
<contactref element="LED2" pad="AB1"/>
<contactref element="CON1" pad="P$7"/>
</signal>
<signal name="N$42">
<contactref element="LED2" pad="K1"/>
<contactref element="CON1" pad="P$8"/>
</signal>
<signal name="N$43">
<contactref element="LED3" pad="AR1"/>
<contactref element="CON1" pad="P$9"/>
</signal>
<signal name="N$44">
<contactref element="LED3" pad="AG1"/>
<contactref element="CON1" pad="P$10"/>
</signal>
<signal name="N$45">
<contactref element="LED3" pad="AB1"/>
<contactref element="CON1" pad="P$11"/>
</signal>
<signal name="N$46">
<contactref element="LED3" pad="K1"/>
<contactref element="CON1" pad="P$12"/>
</signal>
<signal name="N$18">
</signal>
</signals>
</board>
</drawing>
</eagle>
