<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="1" y1="0" x2="98.9" y2="0" width="0" layer="20"/>
<wire x1="98.9" y1="0" x2="99.9" y2="1" width="0" layer="20" curve="90"/>
<wire x1="99.9" y1="1" x2="99.9" y2="13" width="0" layer="20"/>
<wire x1="99.9" y1="13" x2="98.9" y2="14" width="0" layer="20" curve="90"/>
<wire x1="98.9" y1="14" x2="1" y2="14" width="0" layer="20"/>
<wire x1="1" y1="14" x2="0" y2="13" width="0" layer="20" curve="90"/>
<wire x1="0" y1="13" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<text>2013</text>
<text>pfriedel</text>
<text>\\O_o/</text>
<text>v2</text>
<text>3-4.5v</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<hole x="5" y="5" drill="2"/>
<hole x="5" y="9" drill="2"/>
<hole x="2.5" y="2.5" drill="2.8"/>
<hole x="2.5" y="11.5" drill="2.8"/>
</plain>
<libraries>
<library name="00_PERSONAL">
<packages>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOCKET-08">
<description>&lt;b&gt;Dual In Line Socket&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_OFFSET">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
</packages>
</library>
<library name="00_rgbled">
<packages>
<package name="10MM-RGB-LED-PER-SPEC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED3" library="00_rgbled" package="10MM-RGB-LED-PER-SPEC" value="10MM-RGB-LEDPERSPEC"/>
<element name="LED4" library="00_rgbled" package="10MM-RGB-LED-PER-SPEC" value="10MM-RGB-LEDPERSPEC"/>
<element name="LED5" library="00_rgbled" package="10MM-RGB-LED-PER-SPEC" value="10MM-RGB-LEDPERSPEC"/>
<element name="LED1" library="00_rgbled" package="10MM-RGB-LED-PER-SPEC" value="10MM-RGB-LEDPERSPEC"/>
<element name="LED2" library="00_rgbled" package="10MM-RGB-LED-PER-SPEC" value="10MM-RGB-LEDPERSPEC"/>
<element name="R3" library="00_PERSONAL" package="0207/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="00_PERSONAL" package="0207/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="00_PERSONAL" package="0207/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="00_PERSONAL" package="0207/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="00_PERSONAL" package="0207/7" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MODE" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ATTINY" library="ic-package" package="SOCKET-08" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="+" library="SparkFun" package="1X01_OFFSET" value="M01OFFSET">
<attribute name="NAME"/>
</element>
<element name="-" library="SparkFun" package="1X01_OFFSET" value="M01OFFSET">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="C025-025X050" value="100nF"/>
<element name="R6" library="00_PERSONAL" package="0207/2V" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK"/>
</elements>
<signals>
<signal name="2">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="1"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED5" pad="3"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="7">
<contactref element="R4" pad="2"/>
<contactref element="LED4" pad="1"/>
<contactref element="LED5" pad="2"/>
<contactref element="LED1" pad="3"/>
<contactref element="LED2" pad="4"/>
</signal>
<signal name="6">
<contactref element="R5" pad="1"/>
<contactref element="LED5" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="3"/>
<contactref element="LED3" pad="4"/>
</signal>
<signal name="5">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED3" pad="3"/>
<contactref element="LED4" pad="4"/>
</signal>
<signal name="3">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="1"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="3"/>
<contactref element="LED5" pad="4"/>
</signal>
<signal name="RST">
<contactref element="ATTINY" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="MODE" pad="1"/>
</signal>
<signal name="2R">
<contactref element="ATTINY" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="3R">
<contactref element="ATTINY" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="ATTINY" pad="4"/>
<contactref element="-" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="MODE" pad="3"/>
<contactref element="MODE" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="ATTINY" pad="8"/>
<contactref element="+" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="7R">
<contactref element="ATTINY" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="6R">
<contactref element="ATTINY" pad="6"/>
<contactref element="R5" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5R">
<contactref element="ATTINY" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
