<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="6.731" y1="0" x2="39.497" y2="0" width="0" layer="20"/>
<wire x1="39.497" y1="0" x2="46.228" y2="5.588" width="0" layer="20"/>
<wire x1="46.228" y1="5.588" x2="46.228" y2="30.48" width="0" layer="20"/>
<wire x1="46.228" y1="30.48" x2="39.497" y2="36.068" width="0" layer="20"/>
<wire x1="39.497" y1="36.068" x2="6.731" y2="36.068" width="0" layer="20"/>
<wire x1="6.731" y1="36.068" x2="0" y2="30.48" width="0" layer="20"/>
<wire x1="0" y1="30.48" x2="0" y2="5.588" width="0" layer="20"/>
<wire x1="0" y1="5.588" x2="6.731" y2="0" width="0" layer="20"/>
<text>BLK</text>
<text>X1</text>
<text>Antenna</text>
<text>C3</text>
<text>C1</text>
<text>C4</text>
<text>U2</text>
<text>R1</text>
<text>RFM12B</text>
<text>RXD</text>
<text>TXD</text>
<text>+5V</text>
<text>GND</text>
<text>GRN</text>
<text>RST</text>
<text>C2</text>
<text>3.3</text>
<text>GND</text>
<text>+5V</text>
<text>GND</text>
<text>LED</text>
<text>ColorNode V1.1</text>
<text>DigitalMisery.com</text>
<text>open</text>
<text>hardware</text>
<hole x="9.144" y="29.1465" drill="2.2"/>
<hole x="9.144" y="6.9215" drill="2.2"/>
<hole x="42.799" y="6.9215" drill="2.2"/>
<hole x="42.799" y="29.1465" drill="2.2"/>
<text>D1</text>
<text>R2</text>
<text>3.3V</text>
<text>GND</text>
<text>GND</text>
<text>3.3</text>
<text>SDA</text>
<text>SCL</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>D9</text>
<text>GND</text>
<text>U1</text>
<text>I2C</text>
</plain>
<libraries>
<library name="resistor">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="RESONATOR-PTH">
</package>
<package name="FTDI_BASIC">
</package>
<package name="1X01_2MM">
</package>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="JeeLabs">
<packages>
<package name="RFM12B">
<description>RFM12B radio module by HopeRF</description>
</package>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO92-INLINE">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jlpcb-105">
<packages>
<package name="ATMEGA8_DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="OSHW">
<packages>
<package name="OSHW_FILLX200_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
<package name="1X04_NO_SILK">
</package>
<package name="1X06">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="resistor" package="0204/7" value="10k"/>
<element name="C1" library="resistor" package="C025-024X044" value="0.1µ"/>
<element name="C2" library="resistor" package="C025-024X044" value="0.1µ"/>
<element name="C4" library="resistor" package="C025-024X044" value="0.1µ"/>
<element name="U3" library="JeeLabs" package="RFM12B" value="RFM12B">
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun" package="RESONATOR-PTH" value="16 MHz"/>
<element name="ANT" library="JeeLabs" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="FTDI_BASIC" value="FTDI">
<attribute name="VALUE"/>
</element>
<element name="U2" library="adafruit" package="TO92-INLINE" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="jlpcb-105" package="ATMEGA8_DIL28-3" value="ATMEGA8_ATMEGA48/88/168-PU">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="OSHW" package="OSHW_FILLX200_NOTEXT" value=""/>
<element name="C3" library="resistor" package="E1,8-4" value="10µ">
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="0204/7" value="1k">
<attribute name="ABBREV" value="jn5"/>
<attribute name="PROJECT" value="JeeNode v5"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="ABBREV" value="jn5"/>
<attribute name="PROJECT" value="JeeNode v5"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U3" pad="GND"/>
<contactref element="X1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="JP4" pad="CTS"/>
<contactref element="JP4" pad="GND"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="22"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="3"/>
<contactref element="C3" pad="-"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP8" pad="6"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$21">
<contactref element="X1" pad="3"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$13">
<contactref element="U3" pad="ANT"/>
<contactref element="ANT" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="IRQ"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="SDI"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$11">
<contactref element="U3" pad="SDO"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$12">
<contactref element="U3" pad="SCK"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="SEL"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="1"/>
<contactref element="JP4" pad="DTR"/>
</signal>
<signal name="N$6">
<contactref element="JP4" pad="TXO"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="JP4" pad="RXI"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="VDD"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="7"/>
<contactref element="JP4" pad="VCC"/>
<contactref element="C3" pad="+"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="LEDS">
<contactref element="U1" pad="26"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="JP7" pad="3"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="N$16">
<contactref element="JP7" pad="4"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="12"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="15"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="14"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="13"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="11"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="D1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
