<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="79.045" y2="0" width="0" layer="20"/>
<wire x1="79.045" y1="0" x2="79.045" y2="46.98" width="0" layer="20"/>
<wire x1="79.045" y1="46.98" x2="0" y2="46.98" width="0" layer="20"/>
<wire x1="0" y1="46.98" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="bodger">
<packages>
<package name="IN-8-2-GRID">
</package>
<package name="2X5-RA">
</package>
<package name="2X5-RAF">
</package>
<package name="1X02">
</package>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.5" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.5" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.5" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.5" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.5" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.5" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.5" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.5" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V0" library="bodger" package="IN-8-2-GRID" value="IN-8-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V1" library="bodger" package="IN-8-2-GRID" value="IN-8-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V2" library="bodger" package="IN-8-2-GRID" value="IN-8-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V3" library="bodger" package="IN-8-2-GRID" value="IN-8-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P0" library="bodger" package="2X5-RA" value="EVEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="bodger" package="2X5-RA" value="ODD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J0" library="bodger" package="2X5-RAF" value="EVEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="bodger" package="2X5-RAF" value="ODD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="bodger" package="1X02" value="ANODES">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P3" library="bodger" package="1X04" value="DECIMALS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$11">
<contactref element="R1" pad="P$1"/>
<contactref element="V0" pad="12"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="P$1"/>
<contactref element="V1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="P$1"/>
<contactref element="V2" pad="12"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="P$1"/>
<contactref element="V3" pad="12"/>
</signal>
<signal name="N$15">
<contactref element="V0" pad="8"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$16">
<contactref element="V1" pad="8"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$17">
<contactref element="V2" pad="8"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="V3" pad="8"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$22">
<contactref element="V3" pad="10"/>
<contactref element="V1" pad="10"/>
<contactref element="P1" pad="9"/>
<contactref element="J1" pad="9F"/>
</signal>
<signal name="N$30">
<contactref element="V3" pad="9"/>
<contactref element="V1" pad="9"/>
<contactref element="P1" pad="8"/>
<contactref element="J1" pad="8F"/>
</signal>
<signal name="N$28">
<contactref element="V3" pad="7"/>
<contactref element="V1" pad="7"/>
<contactref element="P1" pad="7"/>
<contactref element="J1" pad="7F"/>
</signal>
<signal name="N$31">
<contactref element="V1" pad="6"/>
<contactref element="V3" pad="6"/>
<contactref element="P1" pad="6"/>
<contactref element="J1" pad="6F"/>
</signal>
<signal name="N$27">
<contactref element="V1" pad="5"/>
<contactref element="V3" pad="5"/>
<contactref element="P1" pad="5"/>
<contactref element="J1" pad="5F"/>
</signal>
<signal name="N$26">
<contactref element="V3" pad="4"/>
<contactref element="V1" pad="4"/>
<contactref element="P1" pad="4"/>
<contactref element="J1" pad="4F"/>
</signal>
<signal name="N$25">
<contactref element="V1" pad="3"/>
<contactref element="V3" pad="3"/>
<contactref element="P1" pad="3"/>
<contactref element="J1" pad="3F"/>
</signal>
<signal name="N$24">
<contactref element="V1" pad="2"/>
<contactref element="V3" pad="2"/>
<contactref element="P1" pad="2"/>
<contactref element="J1" pad="2F"/>
</signal>
<signal name="N$23">
<contactref element="V1" pad="1"/>
<contactref element="V3" pad="1"/>
<contactref element="P1" pad="1"/>
<contactref element="J1" pad="1F"/>
</signal>
<signal name="N$21">
<contactref element="V1" pad="11"/>
<contactref element="V3" pad="11"/>
<contactref element="P1" pad="10"/>
<contactref element="J1" pad="10F"/>
</signal>
<signal name="N$33">
<contactref element="V2" pad="2"/>
<contactref element="V0" pad="2"/>
<contactref element="J0" pad="2F"/>
<contactref element="P0" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="P$1"/>
<contactref element="P3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R7" pad="P$1"/>
<contactref element="P3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="P$1"/>
<contactref element="P3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="P$1"/>
<contactref element="P3" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="V2" pad="11"/>
<contactref element="V0" pad="11"/>
<contactref element="P0" pad="10"/>
<contactref element="J0" pad="10F"/>
</signal>
<signal name="N$9">
<contactref element="V0" pad="5"/>
<contactref element="V2" pad="5"/>
<contactref element="P0" pad="5"/>
<contactref element="J0" pad="5F"/>
</signal>
<signal name="N$10">
<contactref element="V0" pad="3"/>
<contactref element="V2" pad="3"/>
<contactref element="P0" pad="3"/>
<contactref element="J0" pad="3F"/>
</signal>
<signal name="N$19">
<contactref element="V0" pad="1"/>
<contactref element="V2" pad="1"/>
<contactref element="P0" pad="1"/>
<contactref element="J0" pad="1F"/>
</signal>
<signal name="N$20">
<contactref element="V0" pad="4"/>
<contactref element="P0" pad="4"/>
<contactref element="V2" pad="4"/>
<contactref element="J0" pad="4F"/>
</signal>
<signal name="N$29">
<contactref element="V0" pad="6"/>
<contactref element="P0" pad="6"/>
<contactref element="V2" pad="6"/>
<contactref element="J0" pad="6F"/>
</signal>
<signal name="N$8">
<contactref element="V0" pad="7"/>
<contactref element="P0" pad="7"/>
<contactref element="J0" pad="7F"/>
<contactref element="V2" pad="7"/>
</signal>
<signal name="N$39">
<contactref element="V0" pad="9"/>
<contactref element="P0" pad="8"/>
<contactref element="J0" pad="8F"/>
<contactref element="V2" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="P0" pad="9"/>
<contactref element="V0" pad="10"/>
<contactref element="J0" pad="9F"/>
<contactref element="V2" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$2"/>
<contactref element="P2" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$32">
<contactref element="P2" pad="2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
