<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<text>1</text>
<text>0</text>
<text>Red-</text>
<text>Yellow+</text>
<text>MAX31850K</text>
<text>&gt;CVERSION</text>
<wire x1="0" y1="2.54" x2="0" y2="19.05" width="0.0254" layer="20"/>
<wire x1="0" y1="19.05" x2="2.54" y2="21.59" width="0.0254" layer="20" curve="-90"/>
<wire x1="2.54" y1="21.59" x2="19.05" y2="21.59" width="0.0254" layer="20"/>
<wire x1="19.05" y1="21.59" x2="21.59" y2="19.05" width="0.0254" layer="20" curve="-90"/>
<wire x1="21.59" y1="19.05" x2="21.59" y2="2.54" width="0.0254" layer="20"/>
<wire x1="21.59" y1="2.54" x2="19.05" y2="0" width="0.0254" layer="20" curve="-90"/>
<wire x1="19.05" y1="0" x2="2.54" y2="0" width="0.0254" layer="20"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0.0254" layer="20" curve="-90"/>
<text>3V3</text>
<text>GND</text>
<text>VIN</text>
<text>DATA</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>VIN: 3.6-16V
DATA: 3.3V</text>
</plain>
<libraries>
<library name="LoganSmith-Capacitors">
<packages>
<package name="0603-CAP">
<description>&lt;b&gt;0603 Chip Capacitor&lt;/b&gt;
&lt;p&gt;Follows standard set in &lt;a href="http://www.tortai-tech.com/upload/download/2011102023233369053.pdf"&gt;IPC-SM-782&lt;/a&gt;, section 8.2 "Chip Capacitors", sub-section 5.0 "Land Pattern Dimensions", Figure 3, RLP 132A.&lt;/p&gt;</description>
</package>
<package name="1206-CAP">
<description>&lt;b&gt;1206 Chip Capacitor&lt;/b&gt;
&lt;p&gt;Follows standard set in &lt;a href="http://www.tortai-tech.com/upload/download/2011102023233369053.pdf"&gt;IPC-SM-782&lt;/a&gt;, section 8.2 "Chip Capacitors", sub-section 5.0 "Land Pattern Dimensions", Figure 3, RLP 134A.&lt;/p&gt;</description>
</package>
<package name="0805-CAP">
<description>&lt;b&gt;0805 Chip Capacitor&lt;/b&gt;
&lt;p&gt;Follows standard set in &lt;a href="http://www.tortai-tech.com/upload/download/2011102023233369053.pdf"&gt;IPC-SM-782&lt;/a&gt;, section 8.2 "Chip Capacitors", sub-section 5.0 "Land Pattern Dimensions", Figure 3, RLP 133A.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LoganSmith-Inductors">
<packages>
<package name="0603-RES">
<description>&lt;b&gt;0603 Chip Resistor&lt;/b&gt;
&lt;p&gt;Follows standard set in &lt;a href="http://www.tortai-tech.com/upload/download/2011102023233369053.pdf"&gt;IPC-SM-782&lt;/a&gt;, section 8.1 "Chip Resistors", sub-section 5.0 "Land Pattern Dimensions", Figure 3, RLP 101A.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LoganSmith-Power_IC">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="LoganSmith-Connectors">
<packages>
<package name="1X08_SQ1">
<description>&lt;p&gt;0.1" spaced header with silkscreen and square pin #1&lt;/p&gt;</description>
</package>
<package name="SJ_3">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="LoganSmith-Electromechanical">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
<description>&lt;p&gt;#2 Mounting Hole&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LoganSmith-Analog_IC">
<packages>
<package name="10-TDFN-EP">
<description>&lt;p&gt;Plastic Very Very Thin Dual Flatpack, No Leads&lt;/p&gt;
&lt;p&gt;Based on Maxim land pattern 90-0247:&lt;br/&gt;
&lt;a href="http://pdfserv.maximintegrated.com/land_patterns/90-0247.PDF"&gt;Land Pattern&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://pdfserv.maximintegrated.com/package_dwgs/21-0268.PDF"&gt;Package Outline&lt;/a&gt;
&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="CVERSION" value="v1.01"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="LoganSmith-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="MFR" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="TEMP_COEFF" value="X7R"/>
<attribute name="TEMP_RANGE" value="-55C to 125C"/>
<attribute name="MPN" value="CL10B104KO8NNNC"/>
<attribute name="THICK" value="0.90mm"/>
<attribute name="DIGIKEY_OC" value="1276-1005-1-ND"/>
<attribute name="TOL" value="+/-10%"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="NAME"/>
</element>
<element name="FB1" library="LoganSmith-Inductors" package="0603-RES" value="">
<attribute name="DC_RES" value="600mOhm(max)"/>
<attribute name="CURRENT_RATING" value="250mA"/>
<attribute name="MFR" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="MPN" value="CIM10J102NC"/>
<attribute name="DIGIKEY_OC" value="1276-6378-1-ND"/>
<attribute name="VALUE" value="1kOhm@100MHz"/>
<attribute name="THICK" value="0.95mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="LoganSmith-Inductors" package="0603-RES" value="">
<attribute name="DC_RES" value="600mOhm(max)"/>
<attribute name="CURRENT_RATING" value="250mA"/>
<attribute name="MFR" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="MPN" value="CIM10J102NC"/>
<attribute name="DIGIKEY_OC" value="1276-6378-1-ND"/>
<attribute name="VALUE" value="1kOhm@100MHz"/>
<attribute name="THICK" value="0.95mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="LoganSmith-Power_IC" package="SOT23-5" value="3.3V">
<attribute name="MFR" value="Texas Instruments"/>
<attribute name="TEMP_RANGE" value="-40C to 125C"/>
<attribute name="MPN" value="LP2985-33DBVR"/>
<attribute name="DIGIKEY_OC" value="296-18476-1-ND"/>
<attribute name="VALUE" value="3.3V"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="LoganSmith-Capacitors" package="1206-CAP" value="10uF">
<attribute name="MFR" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="TEMP_COEFF" value="X7R"/>
<attribute name="TEMP_RANGE" value="-55C to 125C"/>
<attribute name="MPN" value="CL31B106KLHNNNE"/>
<attribute name="THICK" value="1.80mm"/>
<attribute name="DIGIKEY_OC" value="1276-3103-1-ND"/>
<attribute name="TOL" value="+/-10%"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="LoganSmith-Capacitors" package="0805-CAP" value="10uF">
<attribute name="MFR" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="TEMP_COEFF" value="X7R"/>
<attribute name="TEMP_RANGE" value="-55C to 125C"/>
<attribute name="MPN" value="CL21B106KQQNNNE"/>
<attribute name="THICK" value="1.40mm"/>
<attribute name="DIGIKEY_OC" value="1276-1113-1-ND"/>
<attribute name="TOL" value="+/-10%"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="LoganSmith-Analog_IC" package="10-TDFN-EP" value="Type K">
<attribute name="NAME"/>
<attribute name="VALUE" value="Type K"/>
<attribute name="DESC" value=""/>
<attribute name="MFR" value="Maxim Integrated"/>
<attribute name="MPN" value="MAX31850KATB+"/>
<attribute name="DIGIKEY_OC" value="MAX31850KATB+-ND"/>
</element>
<element name="J1" library="LoganSmith-Connectors" package="1X08_SQ1" value="M08SQ1">
<attribute name="MFR" value=""/>
<attribute name="MPN" value=""/>
<attribute name="DIGIKEY_OC" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="AD0" library="LoganSmith-Connectors" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AD1" library="LoganSmith-Connectors" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AD2" library="LoganSmith-Connectors" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AD3" library="LoganSmith-Connectors" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="LoganSmith-Electromechanical" package="MOUNTINGHOLE_2.0_PLATED" value="MNTHOLE-2.0"/>
<element name="U$2" library="LoganSmith-Electromechanical" package="MOUNTINGHOLE_2.0_PLATED" value="MNTHOLE-2.0"/>
<element name="J2" library="LoganSmith-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M02ST-3.5MM">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="TP_FILT">
<contactref element="C1" pad="P$1"/>
<contactref element="U2" pad="3"/>
<contactref element="FB1" pad="P$2"/>
</signal>
<signal name="TM_FILT">
<contactref element="C1" pad="P$2"/>
<contactref element="U2" pad="2"/>
<contactref element="FB2" pad="P$2"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="5"/>
<contactref element="C3" pad="P$1"/>
<contactref element="U2" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="P$4"/>
<contactref element="C3" pad="P$2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="PAD"/>
<contactref element="J1" pad="1"/>
<contactref element="AD0" pad="3"/>
<contactref element="AD1" pad="3"/>
<contactref element="AD2" pad="3"/>
<contactref element="AD3" pad="3"/>
</signal>
<signal name="DATA">
<contactref element="J1" pad="8"/>
<contactref element="U2" pad="5"/>
<contactref element="AD1" pad="1"/>
<contactref element="AD2" pad="1"/>
<contactref element="AD3" pad="1"/>
<contactref element="AD0" pad="1"/>
</signal>
<signal name="AD3">
<contactref element="J1" pad="7"/>
<contactref element="U2" pad="9"/>
<contactref element="AD3" pad="2"/>
</signal>
<signal name="AD2">
<contactref element="J1" pad="6"/>
<contactref element="U2" pad="8"/>
<contactref element="AD2" pad="2"/>
</signal>
<signal name="AD1">
<contactref element="J1" pad="5"/>
<contactref element="U2" pad="7"/>
<contactref element="AD1" pad="2"/>
</signal>
<signal name="AD0">
<contactref element="J1" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="AD0" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="P$3"/>
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="TP_RAW">
<contactref element="FB1" pad="P$1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="TM_RAW">
<contactref element="FB2" pad="P$1"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
