<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="33.8699625" x2="0" y2="1.79605" width="0" layer="20"/>
<wire x1="0" y1="1.79605" x2="1.79605" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.79605" y1="0" x2="33.8699625" y2="0" width="0" layer="20"/>
<wire x1="33.8699625" y1="0" x2="35.999928125" y2="2.129965625" width="0" layer="20" curve="90"/>
<wire x1="35.999928125" y1="2.129965625" x2="35.999928125" y2="33.581725" width="0" layer="20"/>
<wire x1="35.999928125" y1="33.581725" x2="33.581725" y2="35.999928125" width="0" layer="20" curve="90"/>
<wire x1="33.581725" y1="35.999928125" x2="2.129965625" y2="35.999928125" width="0" layer="20"/>
<wire x1="2.129965625" y1="35.999928125" x2="0" y2="33.8699625" width="0" layer="20" curve="90"/>
<hole x="2.75000625" y="2.75000625" drill="3"/>
<hole x="33.250125" y="2.75000625" drill="3"/>
<hole x="33.250125" y="33.250125" drill="3"/>
<hole x="2.75000625" y="33.250125" drill="3"/>
<text>5v
gnd
scl
sda
drdy
3v3</text>
<text>5v
gnd
scl
sda
sda
scl
gnd
3v3</text>
<text>gnd
5v
rx
  tx</text>
<text>rx
  tx
  pwr
  gnd</text>
<text>rx
  tx
  pwr
  gnd</text>
<text>www.spikey.si
may the fourth, 2015</text>
<text>&lt;-</text>
<text>sda
scl
gnd
3v3</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="53261-04">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
right angle</description>
</package>
</packages>
</library>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BMP180" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HMC5883L" library="pinhead-1" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C3V3" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3V3" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="PROD_ID" value="RES-09883"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="PROD_ID" value="RES-09883"/>
</element>
<element name="MAINPORT_SMD" library="con-molex" package="53261-04" value="53261-04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FLEXIPORT_SMD" library="con-molex" package="53261-04" value="53261-04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPS_SMD" library="con-molex" package="53261-04" value="53261-04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C3V3_SMD" library="con-molex" package="53261-04" value="53261-04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MAINPORT" library="pinhead-1" package="1X04SMD/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FLEXIPORT" library="pinhead-1" package="1X04SMD/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPS" library="pinhead-1" package="1X04SMD/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="HMC5883L" pad="1"/>
<contactref element="BMP180" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="MAINPORT_SMD" pad="2"/>
<contactref element="FLEXIPORT_SMD" pad="2"/>
<contactref element="GPS_SMD" pad="2"/>
<contactref element="MAINPORT" pad="2"/>
<contactref element="FLEXIPORT" pad="2"/>
<contactref element="GPS" pad="2"/>
</signal>
<signal name="GND">
<contactref element="I2C3V3" pad="2"/>
<contactref element="BMP180" pad="2"/>
<contactref element="HMC5883L" pad="2"/>
<contactref element="3V3" pad="C"/>
<contactref element="5V" pad="C"/>
<contactref element="MAINPORT_SMD" pad="1"/>
<contactref element="FLEXIPORT_SMD" pad="1"/>
<contactref element="GPS_SMD" pad="1"/>
<contactref element="I2C3V3_SMD" pad="3"/>
<contactref element="MAINPORT" pad="1"/>
<contactref element="FLEXIPORT" pad="1"/>
<contactref element="GPS" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="HMC5883L" pad="6"/>
<contactref element="I2C3V3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="I2C3V3_SMD" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="BMP180" pad="4"/>
<contactref element="I2C3V3" pad="4"/>
<contactref element="HMC5883L" pad="4"/>
<contactref element="FLEXIPORT_SMD" pad="4"/>
<contactref element="I2C3V3_SMD" pad="1"/>
<contactref element="FLEXIPORT" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="BMP180" pad="3"/>
<contactref element="I2C3V3" pad="3"/>
<contactref element="HMC5883L" pad="3"/>
<contactref element="FLEXIPORT_SMD" pad="3"/>
<contactref element="I2C3V3_SMD" pad="2"/>
<contactref element="FLEXIPORT" pad="3"/>
</signal>
<signal name="GPS_TX">
<contactref element="MAINPORT_SMD" pad="4"/>
<contactref element="GPS_SMD" pad="4"/>
<contactref element="MAINPORT" pad="4"/>
<contactref element="GPS" pad="4"/>
</signal>
<signal name="GPS_RX">
<contactref element="MAINPORT_SMD" pad="3"/>
<contactref element="GPS_SMD" pad="3"/>
<contactref element="MAINPORT" pad="3"/>
<contactref element="GPS" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="3V3" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="5V" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
