<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="42.41" y1="38.24" x2="43.68" y2="36.97" width="0" layer="20" curve="-90"/>
<wire x1="43.68" y1="36.97" x2="42.41" y2="35.7" width="0" layer="20" curve="-90"/>
<wire x1="26.84" y1="35.7" x2="25.57" y2="36.97" width="0" layer="20" curve="-90"/>
<wire x1="25.57" y1="36.97" x2="26.84" y2="38.24" width="0" layer="20" curve="-90"/>
<wire x1="42.41" y1="35.7" x2="26.84" y2="35.7" width="0" layer="20"/>
<wire x1="42.41" y1="13.24" x2="43.68" y2="11.97" width="0" layer="20" curve="-90"/>
<wire x1="43.68" y1="11.97" x2="42.41" y2="10.7" width="0" layer="20" curve="-90"/>
<wire x1="26.84" y1="10.7" x2="25.57" y2="11.97" width="0" layer="20" curve="-90"/>
<wire x1="25.57" y1="11.97" x2="26.84" y2="13.24" width="0" layer="20" curve="-90"/>
<wire x1="26.84" y1="13.24" x2="42.41" y2="13.24" width="0" layer="20"/>
<wire x1="42.41" y1="10.7" x2="26.84" y2="10.7" width="0" layer="20"/>
<circle x="34.75" y="24.5" radius="17.78" width="0.002540625" layer="20"/>
<wire x1="26.84" y1="38.24" x2="42.41" y2="38.24" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CR2032-THRU">
</package>
</packages>
</library>
<library name="zak">
<description>Zaks library</description>
<packages>
<package name="USB-MICROB">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$5" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$2" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$3" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$7" library="adafruit" package="CR2032-THRU" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="USB1" library="zak" package="USB-MICROB" value="USB-MICROBNORMAL"/>
<element name="TP15" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP1" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$7" pad="-"/>
<contactref element="USB1" pad="GND"/>
<contactref element="TP1" pad="TP"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="VBAT">
<contactref element="U$7" pad="+1"/>
<contactref element="U$7" pad="+2"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="VBUS">
<contactref element="USB1" pad="VBUS"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
</signals>
</board>
</drawing>
</eagle>
