<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.86" y2="0" width="0" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="21.6535" width="0" layer="20"/>
<wire x1="22.86" y1="21.6535" x2="0" y2="21.6535" width="0" layer="20"/>
<wire x1="0" y1="21.6535" x2="0" y2="0" width="0" layer="20"/>
<hole x="21.209" y="1.5875" drill="2.54"/>
<text>BATT</text>
<text>DC</text>
<text>T</text>
<text>R</text>
<text>S</text>
<text>S</text>
<text>T</text>
<text>OUT</text>
<text>IN</text>
<text>O</text>
<text>V</text>
<text>G</text>
<text>I</text>
<text>A</text>
<text>Boilerplate</text>
<text>ver2</text>
</plain>
<libraries>
<library name="switches">
<packages>
<package name="3PDT">
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0204/2">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 3mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 2 holes

&lt;p&gt;This length resistor applies to 1/8 watt metal film.</description>
</package>
</packages>
</library>
<library name="gm-trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="SOT54ES">
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.9 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="OCTOGON-L">
</package>
<package name="OCTOGON">
<description>&lt;b&gt;Octogonal Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.9 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="gm-caps-electro-pol" package="050_020" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gm-caps-film-box" package="072X025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="gm-resistors" package="R0204/2" value="3MM.2">
<attribute name="NAME"/>
</element>
<element name="Q1" library="gm-trans" package="SOT54ES" value="BS250S">
<attribute name="NAME"/>
</element>
<element name="R1" library="gm-resistors" package="R0204/2" value="3MM.2">
<attribute name="NAME"/>
</element>
<element name="SW1" library="switches" package="3PDT" value="3PDT"/>
<element name="D1" library="gm-diodes" package="LED3MM" value="LED3MM"/>
<element name="R2" library="gm-resistors" package="R0204/2" value="3MM.2">
<attribute name="NAME"/>
</element>
<element name="C" library="gm-supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
<element name="P" library="gm-supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
<element name="S" library="gm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="A" library="gm-supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
<element name="I" library="gm-supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
<element name="O" library="gm-supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
<element name="V" library="gm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="G" library="gm-supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
<element name="_" library="gm-supply" package="OCTOGON-L" value="">
<attribute name="NAME"/>
</element>
<element name="+" library="gm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="OT" library="gm-supply" package="SQUARE" value=""/>
<element name="OS" library="gm-supply" package="OCTOGON" value=""/>
<element name="IT" library="gm-supply" package="SQUARE" value=""/>
<element name="IS" library="gm-supply" package="OCTOGON" value=""/>
<element name="IR" library="gm-supply" package="OCTOGON" value=""/>
<element name="V1" library="gm-supply" package="SQUARE" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="L1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="V" pad="1"/>
<contactref element="V1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="SW1" pad="B2"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="P" pad="1"/>
<contactref element="G" pad="1"/>
<contactref element="OS" pad="1"/>
<contactref element="IS" pad="1"/>
<contactref element="SW1" pad="A3"/>
</signal>
<signal name="N$5">
<contactref element="I" pad="1"/>
<contactref element="SW1" pad="A2"/>
</signal>
<signal name="N$6">
<contactref element="O" pad="1"/>
<contactref element="SW1" pad="C1"/>
</signal>
<signal name="N$7">
<contactref element="OT" pad="1"/>
<contactref element="SW1" pad="C2"/>
</signal>
<signal name="N$8">
<contactref element="IT" pad="1"/>
<contactref element="SW1" pad="A1"/>
<contactref element="SW1" pad="C3"/>
</signal>
<signal name="N$4">
<contactref element="SW1" pad="B3"/>
<contactref element="A" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="SW1" pad="B1"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="D1" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="N$14">
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="Q1" pad="S"/>
</signal>
<signal name="N$15">
<contactref element="Q1" pad="D"/>
<contactref element="R2" pad="1"/>
<contactref element="S" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C" pad="1"/>
<contactref element="+" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="_" pad="P$1"/>
<contactref element="IR" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
