<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="6.35" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="3.175" y2="0" width="0" layer="20"/>
<wire x1="3.175" y1="0" x2="4.445" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.715" y1="0" x2="7.62" y2="0" width="0" layer="20"/>
<wire x1="7.62" y1="0" x2="8.89" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="8.89" y1="1.27" x2="10.16" y2="0" width="0" layer="20" curve="90"/>
<wire x1="10.16" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="7.62" width="0" layer="20"/>
<wire x1="25.4" y1="7.62" x2="10.16" y2="7.62" width="0" layer="20"/>
<wire x1="10.16" y1="7.62" x2="8.89" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="8.89" y1="6.35" x2="7.62" y2="7.62" width="0" layer="20" curve="90"/>
<wire x1="7.62" y1="7.62" x2="5.715" y2="7.62" width="0" layer="20"/>
<wire x1="5.715" y1="7.62" x2="4.445" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="4.445" y1="6.35" x2="3.175" y2="7.62" width="0" layer="20" curve="90"/>
<wire x1="3.175" y1="7.62" x2="1.27" y2="7.62" width="0" layer="20"/>
<wire x1="1.27" y1="7.62" x2="0" y2="6.35" width="0" layer="20" curve="90"/>
<hole x="4.445" y="5.715" drill="0.3302"/>
<hole x="4.445" y="1.905" drill="0.3302"/>
<hole x="4.445" y="3.81" drill="0.3302"/>
<hole x="4.445" y="4.7625" drill="0.3302"/>
<hole x="4.445" y="2.8575" drill="0.3302"/>
<wire x1="7.62" y1="0" x2="8.89" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="8.89" y1="1.27" x2="10.16" y2="0" width="0" layer="20" curve="90"/>
<wire x1="10.16" y1="7.62" x2="8.89" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="8.89" y1="6.35" x2="7.62" y2="7.62" width="0" layer="20" curve="90"/>
<hole x="8.89" y="5.715" drill="0.3302"/>
<hole x="8.89" y="1.905" drill="0.3302"/>
<hole x="8.89" y="3.81" drill="0.3302"/>
<hole x="8.89" y="4.7625" drill="0.3302"/>
<hole x="8.89" y="2.8575" drill="0.3302"/>
<text>Pic ICSP Pogo adapter</text>
<text>Copyright 2015 N3M0</text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="CON_POGO_ICSP_PROG">
<description>&lt;B&gt;Pogo pin ICSP programmer side footprint &lt;/B&gt;
&lt;BR/&gt; pogo pin diameter 0.65mm
&lt;BR/&gt; total pogo diameter 1.70mm
&lt;BR/&gt; pinout from top left: MCLR, GND, VCC
&lt;BR/&gt; pinout from bottom left: PGD, PGC, KEY(NC)</description>
</package>
</packages>
</library>
<library name="special-drill">
<description>&lt;b&gt;Special drills&lt;/b&gt;&lt;p&gt;
For drills bigger as 0.51602 Inch you must draw a circle in Layer 20 Dimension.&lt;br&gt;
See also HELP HOLE,</description>
<packages>
<package name="PAD_0.1250">
<description>&lt;b&gt;0.1250 Inch&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad2">
<packages>
<package name="1,2/0,6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="dp_devices" package="CON_POGO_ICSP_PROG" value="CON_HEADER_PRG_PIC_ICSP-POGO-PROG">
<attribute name="NAME"/>
</element>
<element name="J2" library="dp_devices" package="CON_POGO_ICSP_PROG" value="CON_HEADER_PRG_PIC_ICSP-POGO-PROG">
<attribute name="NAME"/>
</element>
<element name="H1" library="special-drill" package="PAD_0.1250" value="SPECIAL_DRILL_0.1250">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="PAD2" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="PAD3" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="PAD4" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="PAD5" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="PAD6" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="NC" library="wirepad2" package="1,2/0,6" value="WIREPAD1,2/0,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PGC" library="wirepad2" package="1,2/0,6" value="WIREPAD1,2/0,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PGD" library="wirepad2" package="1,2/0,6" value="WIREPAD1,2/0,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MCLR" library="wirepad2" package="1,2/0,6" value="WIREPAD1,2/0,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad2" package="1,2/0,6" value="WIREPAD1,2/0,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+V" library="wirepad2" package="1,2/0,6" value="WIREPAD1,2/0,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="PAD1" pad="1"/>
<contactref element="NC" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="PAD2" pad="1"/>
<contactref element="PGC" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="PAD3" pad="1"/>
<contactref element="PGD" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="PAD4" pad="1"/>
<contactref element="MCLR" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="PAD5" pad="1"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="PAD6" pad="1"/>
<contactref element="+V" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
