<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="47.9425" y1="7.9375" x2="47.9425" y2="44.755" width="0" layer="20"/>
<wire x1="47.9425" y1="44.755" x2="14.2975" y2="44.755" width="0" layer="20"/>
<wire x1="14.2975" y1="44.755" x2="14.2975" y2="7.9375" width="0" layer="20"/>
<wire x1="14.2975" y1="7.9375" x2="47.9425" y2="7.9375" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="1X02_XTRA_BIG">
</package>
<package name="VNH2SP30">
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Passives" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="1206" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="1206" value="33nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="PANASONIC_G" value="560uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X02_XTRA_BIG" value="M1"/>
<element name="U1" library="SparkFun" package="VNH2SP30" value="VNH2SP30">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P" library="SparkFun" package="1X08" value="M1"/>
<element name="JP3" library="SparkFun" package="1X02_XTRA_BIG" value="VCC"/>
<element name="C3" library="SparkFun" package="PANASONIC_G" value="560uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="OUTA1">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="SLUG3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="OUTB1">
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="SLUG2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="P" pad="8"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="18"/>
<contactref element="JP3" pad="2"/>
<contactref element="C3" pad="-"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="SLUG1"/>
<contactref element="C2" pad="+"/>
<contactref element="JP3" pad="1"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="INA1">
<contactref element="R1" pad="1"/>
<contactref element="P" pad="1"/>
</signal>
<signal name="INB1">
<contactref element="R2" pad="1"/>
<contactref element="P" pad="6"/>
</signal>
<signal name="PWM1">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="P" pad="3"/>
</signal>
<signal name="CS1">
<contactref element="C1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="P" pad="4"/>
</signal>
<signal name="5V">
<contactref element="P" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
