<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="32.0449375" y1="20.6375" x2="1.5875" y2="20.6375" width="0.2032" layer="20"/>
<wire x1="1.5875" y1="20.6375" x2="0" y2="19.05" width="0.2032" layer="20" curve="90"/>
<wire x1="0" y1="19.05" x2="0" y2="2.289525" width="0.2032" layer="20"/>
<wire x1="32.0449375" y1="20.6375" x2="34.29" y2="18.3924375" width="0.2032" layer="20" curve="-90"/>
<wire x1="2.289525" y1="0" x2="33.1452375" y2="0" width="0.2032" layer="20"/>
<wire x1="33.1452375" y1="0" x2="34.29" y2="1.1447625" width="0.2032" layer="20" curve="90"/>
<wire x1="34.29" y1="1.1447625" x2="34.29" y2="18.3924375" width="0.2032" layer="20"/>
<wire x1="0" y1="2.289525" x2="2.289525" y2="0" width="0.2032" layer="20" curve="90"/>
<text>TD1207/8 Breakout board</text>
<text>TXO</text>
<text>RXI</text>
<text>3V3</text>
<text>GND</text>
<text>DTR</text>
<text>CTS</text>
<text>http://hidnseek.fr</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="FIDUCIAL-1X2">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="EIA3216">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="droneRescueAkeru_Beta_3.2">
<description>Generated from &lt;b&gt;Akeru_Beta_3.2.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="TD1202">
<description>Telecom Design - SIGFOX Gateway TD1202</description>
</package>
<package name="SMA_EDGE">
</package>
</packages>
</library>
<library name="PP_Passives">
<packages>
<package name="SOD-923">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="logo">
<description>&lt;b&gt;Electronic logos&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="ESD_10.00">
<description>&lt;b&gt;Logo ESD 10 mm&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$7" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$16" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$11" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="C1" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERIAL" library="SparkFun" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TD1208" library="droneRescueAkeru_Beta_3.2" package="TD1202" value="SIGFOX_TD1202"/>
<element name="J$1" library="droneRescueAkeru_Beta_3.2" package="SMA_EDGE" value="SMA_EDGE"/>
<element name="C4" library="SparkFun" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TVS1" library="PP_Passives" package="SOD-923" value="">
<attribute name="NAME"/>
</element>
<element name="D1" library="adafruit" package="CHIP-LED0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0402-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="CHIP-LED0603" value="GRN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0402-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="logo" package="ESD_10.00" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="C"/>
<contactref element="C2" pad="2"/>
<contactref element="SERIAL" pad="6"/>
<contactref element="TD1208" pad="1"/>
<contactref element="TD1208" pad="2"/>
<contactref element="TD1208" pad="11"/>
<contactref element="TD1208" pad="11"/>
<contactref element="TD1208" pad="1"/>
<contactref element="TD1208" pad="2"/>
<contactref element="TD1208" pad="25"/>
<contactref element="TD1208" pad="23"/>
<contactref element="TD1208" pad="12"/>
<contactref element="TD1208" pad="22"/>
<contactref element="D1" pad="C"/>
<contactref element="J$1" pad="GND@0"/>
<contactref element="J$1" pad="GND@1"/>
<contactref element="J$1" pad="GND@2"/>
<contactref element="J$1" pad="GND@3"/>
<contactref element="TVS1" pad="P$1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="RESET">
<contactref element="TD1208" pad="14"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="A"/>
<contactref element="C2" pad="1"/>
<contactref element="TD1208" pad="9"/>
<contactref element="R3" pad="2"/>
<contactref element="SERIAL" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="TX3V3">
<contactref element="TD1208" pad="18"/>
<contactref element="SERIAL" pad="2"/>
</signal>
<signal name="RX3V3">
<contactref element="TD1208" pad="19"/>
<contactref element="SERIAL" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="J$1" pad="SIG"/>
<contactref element="TD1208" pad="24"/>
<contactref element="TVS1" pad="P$2"/>
</signal>
<signal name="DTR3V3">
<contactref element="SERIAL" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="TD1208" pad="21"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
