<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="36.068" y1="29.972" x2="63.932" y2="29.972" width="0" layer="20"/>
<wire x1="63.932" y1="29.972" x2="63.932" y2="51.298" width="0" layer="20"/>
<wire x1="63.932" y1="51.298" x2="36.068" y2="51.298" width="0" layer="20"/>
<wire x1="36.068" y1="51.298" x2="36.068" y2="29.972" width="0" layer="20"/>
<text>VCC</text>
<text>NC3</text>
<text>RST</text>
<text>GND</text>
<text>HM-11 Breakout</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>See boxbeacon.com/hm-11-breakout.php 
for full information.</text>
</plain>
<libraries>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="08P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="HM-11">
<packages>
<package name="HM-11">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="0" library="con-amp-quick" package="08P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="1" library="con-amp-quick" package="08P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$2" library="HM-11" package="HM-11" value="HM-11"/>
</elements>
<signals>
<signal name="S$7">
</signal>
<signal name="GND">
<contactref element="1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="UART_RTS"/>
<contactref element="0" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="UART_TX"/>
<contactref element="0" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="UART_CTS"/>
<contactref element="0" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="UART_RX"/>
<contactref element="0" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="NC1"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="NV1"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="NV2"/>
<contactref element="0" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="1" pad="8"/>
<contactref element="U$2" pad="PIO0"/>
</signal>
<signal name="N$10">
<contactref element="1" pad="7"/>
<contactref element="U$2" pad="PIO1"/>
</signal>
<signal name="N$11">
<contactref element="1" pad="6"/>
<contactref element="U$2" pad="PIO2"/>
</signal>
<signal name="N$12">
<contactref element="1" pad="5"/>
<contactref element="U$2" pad="PIO3"/>
</signal>
<signal name="N$16">
<contactref element="1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="1" pad="1"/>
<contactref element="U$2" pad="VCC"/>
</signal>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$3">
<contactref element="0" pad="6"/>
</signal>
<signal name="S$4">
<contactref element="0" pad="5"/>
</signal>
<signal name="S$5">
</signal>
<signal name="S$6">
</signal>
<signal name="S$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
