<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0.762" y1="0" x2="25.8572" y2="0" width="0" layer="20"/>
<wire x1="26.6192" y1="0.762" x2="26.6192" y2="33.274" width="0" layer="20"/>
<text>mBLE STM32F042K6T6</text>
<text>Debugger
Prototype V1</text>
<text>February 2015
Colin Szechy</text>
<wire x1="25.6032" y1="34.036" x2="0.762" y2="34.036" width="0" layer="20"/>
<wire x1="0" y1="33.274" x2="0" y2="0.762" width="0" layer="20"/>
<wire x1="0.762" y1="0" x2="0" y2="0.762" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="33.274" x2="0.762" y2="34.036" width="0" layer="20" curve="-90"/>
<wire x1="25.8572" y1="0" x2="26.6192" y2="0.762" width="0" layer="20" curve="90"/>
<wire x1="25.6032" y1="34.036" x2="26.6192" y2="33.274" width="0" layer="20" curve="-90"/>
<text>RESET</text>
<text>BOOT</text>
</plain>
<libraries>
<library name="mBLE">
<packages>
<package name="LQFP32-7X7">
<description>&lt;b&gt;LQFP-32 package&lt;/b&gt; 7x7 mm case, 0.8 mm lead pitch&lt;/b&gt;&lt;p&gt;
Sourced: &lt;a href="http://www.st.com/stonline/products/literature/ds/14771/stm8s105c4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="USB_MICRO_B-JST-MC5BR3-M404-4S-TB">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED-0603">
</package>
<package name="0805">
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="mBLE" package="LQFP32-7X7" value="STM32F042K6T6"/>
<element name="J1" library="mBLE" package="USB_MICRO_B-JST-MC5BR3-M404-4S-TB" value="MICRO_USB_B_JST_MC5BR3-M404-4S">
<attribute name="MOUSER" value="53X3655"/>
<attribute name="DIGIKEY" value="455-2567-2-ND"/>
</element>
<element name="U$6" library="mBLE" package="SOT23-5" value="LDO">
<attribute name="DIGIKEY" value="296-27893-1-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="4.7uF">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0805" value="4.7uF">
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0805" value="10nF">
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="27">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="27">
<attribute name="VALUE"/>
</element>
<element name="S1" library="mBLE" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="mBLE" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="mBLE" package="0805" value="56">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="mBLE" package="2X10" value="M10X2"/>
<element name="J2" library="mBLE" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="mBLE" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="mBLE" package="0805" value="56">
<attribute name="VALUE"/>
</element>
<element name="S2" library="mBLE" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="U$6" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="32"/>
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="10"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="U$6" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U$6" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U$6" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="17"/>
<contactref element="R4" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="J2" pad="6"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="21"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SWCLK">
<contactref element="U1" pad="24"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="SWDIO">
<contactref element="U$1" pad="7"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="NRST">
<contactref element="U1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="26"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="SWDIO_TAR">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="SWDCLK_TAR">
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="SWO_TAR">
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="RESET_TAR">
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="NRST1">
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="31"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
