<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>Bendulum Clock
Shield - Rev H</text>
<text>B</text>
<text>B</text>
<text>A</text>
<text>A</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>Vcc</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4001-KIT">
</package>
</packages>
</library>
<library name="dehne">
<description>David Ehnebuske's parts library</description>
<packages>
<package name="LED-RGB-THRU">
<description>RGB LED PTH Spaced for easy soldering</description>
</package>
<package name="DUEMILANOVE_SHIELD">
<description>&lt;p&gt;&lt;b&gt;Arduino Shield&lt;/b&gt;&lt;/p&gt;</description>
</package>
<package name="HMF-LOGO">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="SOCKET-08">
<description>8-Pin DIP socket</description>
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CAP-PTH-5MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P5" library="dehne" package="1X02" value="Pwr"/>
<element name="P4" library="dehne" package="1X02" value="Batt"/>
<element name="J1" library="dehne" package="1X02" value="Cold Start"/>
<element name="P3" library="dehne" package="1X02" value="Coil"/>
<element name="P1" library="dehne" package="1X02" value="Clock"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001-KIT" value="1N4002"/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="0.1uF"/>
<element name="P2" library="dehne" package="1X03" value="IR Recv"/>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="47uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="D2" library="dehne" package="LED-RGB-THRU" value="RGB-LED">
<attribute name="PROD_ID" value="DIO-09434"/>
</element>
<element name="U$1" library="dehne" package="DUEMILANOVE_SHIELD" value="ARDUINO-SHIELD"/>
<element name="S1" library="dehne" package="TACTILE-PTH" value="Reset"/>
<element name="U$2" library="dehne" package="HMF-LOGO" value=""/>
<element name="R1" library="dehne" package="AXIAL-0.4" value="18R"/>
<element name="R3" library="dehne" package="AXIAL-0.4" value="1.2k"/>
<element name="R4" library="dehne" package="AXIAL-0.4" value="47k"/>
<element name="R5" library="dehne" package="AXIAL-0.4" value="47k"/>
<element name="R6" library="dehne" package="AXIAL-0.4" value="330R"/>
<element name="R7" library="dehne" package="AXIAL-0.4" value="330R"/>
<element name="R8" library="dehne" package="AXIAL-0.4" value="330R"/>
<element name="R9" library="dehne" package="AXIAL-0.4" value="680R"/>
<element name="U1" library="dehne" package="SOCKET-08" value="LP2951-N"/>
<element name="TMP102" library="dehne" package="1X06" value="P6"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="P4" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="N$3">
<contactref element="P5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="U1">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="P5" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="P3" pad="1"/>
<contactref element="U$1" pad="A2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="D12"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="3.3V"/>
<contactref element="R4" pad="P$2"/>
<contactref element="TMP102" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="AREF"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="D2"/>
</signal>
<signal name="N$14">
<contactref element="P2" pad="1"/>
<contactref element="U$1" pad="D3"/>
</signal>
<signal name="N$15">
<contactref element="P2" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="5V"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="P3" pad="2"/>
<contactref element="P4" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="P2" pad="2"/>
<contactref element="U$1" pad="GND@0"/>
<contactref element="R5" pad="P$1"/>
<contactref element="U1" pad="8"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="TMP102" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="D9"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="D6"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="D5"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$17">
<contactref element="D2" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="D2" pad="3"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="D2" pad="4"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="D10"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="P1" pad="1"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="D11"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="S1" pad="2"/>
<contactref element="U$1" pad="RES"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="TMP102" pad="4"/>
<contactref element="U$1" pad="A4"/>
</signal>
<signal name="N$16">
<contactref element="TMP102" pad="3"/>
<contactref element="U$1" pad="A5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
