<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.02" y2="0" width="0" layer="20"/>
<wire x1="33.02" y1="0" x2="33.02" y2="22.86" width="0" layer="20"/>
<wire x1="33.02" y1="22.86" x2="0" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="22.86" x2="0" y2="0" width="0" layer="20"/>
<text>(C) 2013</text>
<text>ae</text>
</plain>
<libraries>
<library name="mm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="mm-ics" package="DIL08" value="LT1054"/>
<element name="C1" library="mm-caps-electro-pol" package="063_025" value="100µ"/>
<element name="C2" library="mm-caps-electro-pol" package="063_025" value="100µ"/>
<element name="C3" library="mm-caps-electro-pol" package="050_020_1" value="10µ"/>
<element name="C4" library="mm-caps-electro-pol" package="050_020_1" value="10µ"/>
<element name="C5" library="mm-caps-electro-pol" package="050_020_1" value="10µ"/>
<element name="Z1" library="mm-diodes" package="DO41-3" value=""/>
<element name="D1" library="mm-diodes" package="DO41-3" value=""/>
<element name="D2" library="mm-diodes" package="DO41-3" value=""/>
<element name="D3" library="mm-diodes" package="DO41-3" value=""/>
<element name="D4" library="mm-diodes" package="DO41-3" value=""/>
<element name="D5" library="mm-diodes" package="DO41-3" value=""/>
<element name="Z2" library="mm-diodes" package="DO41-3" value=""/>
<element name="Z3" library="mm-diodes" package="DO41-3" value=""/>
<element name="V+" library="mm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="+12" library="mm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="-12" library="mm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="G3" library="mm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="G2" library="mm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="G1" library="mm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="8"/>
<contactref element="D1" pad="A"/>
<contactref element="Z1" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="V+" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="+"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="+"/>
</signal>
<signal name="N$5">
<contactref element="C5" pad="-"/>
<contactref element="D4" pad="A"/>
<contactref element="D5" pad="C"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="D2" pad="C"/>
<contactref element="Z2" pad="C"/>
<contactref element="+12" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="D3" pad="C"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="N$9">
<contactref element="D5" pad="A"/>
<contactref element="Z3" pad="A"/>
<contactref element="-12" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="D4" pad="C"/>
<contactref element="Z3" pad="C"/>
<contactref element="C2" pad="+"/>
<contactref element="Z2" pad="A"/>
<contactref element="C1" pad="-"/>
<contactref element="Z1" pad="A"/>
<contactref element="G3" pad="1"/>
<contactref element="G2" pad="1"/>
<contactref element="G1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
