<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="5.23634375" y1="0" x2="48.7016375" y2="0" width="0" layer="20"/>
<wire x1="48.7016375" y1="0" x2="53.01" y2="4.3083625" width="0" layer="20" curve="90"/>
<wire x1="53.01" y1="4.3083625" x2="53.01" y2="55.284084375" width="0" layer="20"/>
<wire x1="53.01" y1="55.284084375" x2="48.614084375" y2="59.68" width="0" layer="20" curve="90"/>
<wire x1="48.614084375" y1="59.68" x2="4.573509375" y2="59.68" width="0" layer="20"/>
<wire x1="4.573509375" y1="59.68" x2="0" y2="55.106490625" width="0" layer="20" curve="90"/>
<wire x1="0" y1="55.106490625" x2="0" y2="5.23634375" width="0" layer="20"/>
<wire x1="0" y1="5.23634375" x2="5.23634375" y2="0" width="0" layer="20" curve="90"/>
<text>PT2399</text>
<text>TL072</text>
<text>78L05</text>
<text>Rebote 2.5 Delay Clone Rev 1.0</text>
<text>Visit lemonlimefx.wordpress.com</text>
</plain>
<libraries>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-regulators">
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-pots">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;chassis-mount (e.g., Alpha 16mm) pots&lt;/li&gt;
&lt;li&gt;board-mount trim pots (1/4" and 3/8")&lt;/li&gt;
&lt;li&gt; all pot values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="POT">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;3 terminals for circuit board for wires connecting to 3 lugs of pot off-board</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="logos">
<packages>
<package name="LOGO-4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="gm-resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="gm-resistors" package="R0207/3" value="510K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="gm-resistors" package="R0207/3" value="240K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="gm-resistors" package="R0207/3" value="510K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="gm-resistors" package="R0207/3" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="gm-resistors" package="R0207/3" value="24K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="gm-resistors" package="R0207/3" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="gm-resistors" package="R0207/3" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="gm-resistors" package="R0207/3" value="24K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="gm-resistors" package="R0207/3" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="gm-resistors" package="R0207/3" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="gm-resistors" package="R0207/3" value="15K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="gm-resistors" package="R0207/3" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="gm-resistors" package="R0207/3" value="24K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="gm-resistors" package="R0207/3" value="2.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="gm-caps-film-box" package="072X025" value=".082uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gm-caps-film-box" package="072X025" value="5pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="gm-caps-film-box" package="072X025" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gm-caps-film-box" package="072X025" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="gm-caps-film-box" package="072X025" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="gm-caps-film-box" package="072X025" value="51pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="gm-caps-film-box" package="072X025" value="560pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="gm-caps-film-box" package="072X025" value=".027uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="gm-caps-film-box" package="072X025" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="gm-caps-film-box" package="072X025" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="gm-caps-film-box" package="072X025" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="gm-caps-film-box" package="072X025" value="0.001uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="gm-caps-film-box" package="072X025" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="gm-caps-electro-pol" package="050_020_1" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="gm-caps-electro-pol" package="050_020_1" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="gm-caps-electro-pol" package="050_020_1" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="gm-caps-electro-pol" package="050_020_1" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="gm-caps-electro-pol" package="050_020_1" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="gm-caps-electro-pol" package="050_020_1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="gm-caps-electro-pol" package="050_020_1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="gm-caps-electro-pol" package="050_020_1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="gm-caps-film-box" package="072X025" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="gm-caps-film-box" package="072X025" value=".082uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="gm-caps-film-box" package="072X025" value=".082uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="gm-ics" package="DIL08" value="TL072P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="gm-ics" package="DIL16" value="PT2399">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="gm-caps-electro-pol" package="050_020_1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="gm-regulators" package="TO92-" value="78L05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+9V" library="gm-supply" package="SQUARE" value="+9V(T)">
<attribute name="NAME"/>
</element>
<element name="GND" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="IN" library="gm-supply" package="SQUARE" value="IN(T)">
<attribute name="NAME"/>
</element>
<element name="OUT" library="gm-supply" package="SQUARE" value="OUT(T)">
<attribute name="NAME"/>
</element>
<element name="REPEATS" library="gm-pots" package="POT" value="25K-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LEVEL" library="gm-pots" package="POT" value="100K-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DELAY" library="gm-pots" package="POT" value="50K-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="U$1" library="logos" package="LOGO-4" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="C20" pad="+"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="C17" pad="+"/>
<contactref element="C16" pad="+"/>
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C18" pad="+"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC2" pad="7"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC2" pad="8"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="9"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C23" pad="2"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="11"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C20" pad="-"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="R22" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C21" pad="+"/>
</signal>
<signal name="N$28">
<contactref element="C22" pad="2"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R17" pad="1"/>
<contactref element="REPEATS" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R8" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="IC1" pad="3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R11" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C19" pad="+"/>
</signal>
<signal name="VA">
<contactref element="IC2" pad="16"/>
<contactref element="C7" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="VB">
<contactref element="IC2" pad="15"/>
<contactref element="R16" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="VC">
<contactref element="IC2" pad="14"/>
<contactref element="R22" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="VD">
<contactref element="IC2" pad="13"/>
<contactref element="C12" pad="2"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="+9V">
<contactref element="C14" pad="+"/>
<contactref element="R5" pad="2"/>
<contactref element="+9V" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C14" pad="-"/>
<contactref element="GND" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C15" pad="-"/>
<contactref element="IC3" pad="2"/>
<contactref element="C17" pad="-"/>
<contactref element="C16" pad="-"/>
<contactref element="C5" pad="1"/>
<contactref element="C18" pad="-"/>
<contactref element="IC2" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="REPEATS" pad="1"/>
<contactref element="LEVEL" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="IN">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="IN" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="C19" pad="-"/>
<contactref element="R12" pad="2"/>
<contactref element="OUT" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C21" pad="-"/>
<contactref element="REPEATS" pad="3"/>
<contactref element="LEVEL" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="LEVEL" pad="2"/>
<contactref element="C25" pad="-"/>
</signal>
<signal name="N$16">
<contactref element="C25" pad="+"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="C24" pad="2"/>
<contactref element="IC2" pad="12"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="DELAY" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="DELAY" pad="2"/>
</signal>
<signal name="VR">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="C15" pad="+"/>
<contactref element="R3" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="DELAY" pad="1"/>
<contactref element="IC2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
