<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="36.5" y1="25.96676875" x2="36.5" y2="45.97379375" width="0" layer="20"/>
<wire x1="36.5" y1="45.97379375" x2="33.58879375" y2="48.885" width="0" layer="20" curve="90"/>
<wire x1="33.58879375" y1="48.885" x2="2.6870125" y2="48.885" width="0" layer="20"/>
<wire x1="2.6870125" y1="48.885" x2="0" y2="46.1979875" width="0" layer="20" curve="90"/>
<wire x1="0" y1="46.1979875" x2="0" y2="26.189075" width="0" layer="20"/>
<wire x1="0" y1="26.189075" x2="2.694075" y2="23.495" width="0" layer="20" curve="90"/>
<wire x1="2.694075" y1="23.495" x2="34.02823125" y2="23.495" width="0" layer="20"/>
<wire x1="34.02823125" y1="23.495" x2="36.5" y2="25.96676875" width="0" layer="20" curve="90"/>
<text>Raspberry Pi
Hub75-Dual v1.1</text>
<text>by CaptainMurdoch
http://FalconChristmas.com
Falcon Player</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="raspberrypi_bastelstube_v12">
<description>&lt;b&gt;Raspberry Pi&lt;/b&gt; by &lt;b&gt;Martin's Bastelstube&lt;/b&gt;
&lt;p&gt;
Different shapes of piggyback boards for the famous &amp;amp; fabulous
&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt; computer.
&lt;p&gt;
The outline of the Raspberry Pi board is drawn on layer 52 bDocu, so you can make it invisible if necessary.&lt;br/&gt;
Recommendation: Start your design with RASPI_BOARD_*_FULL, so you are aware of all the big components and
connectors when you're drawing the dimensions of your board and placing your own components.&lt;br/&gt;
Later, you can simply change the package of your Raspberry Pi connector to the RASPI_BOARD_*_EDGES type,
so you can concentrate on your own design.
&lt;p&gt;
My board packages don't have the outline drawn in layer 20 Dimension. This allows you to deviate from the original Raspberry Pi board shape, e.g. when you need more space behind the GPIO connector for the routing of the power supply lines. If you want to stick exactly to the Raspberry Pi board shape, then just draw the Dimension layer exactly on the lines in layer bDocu.

&lt;hr&gt;&lt;br/&gt;

Version 1.2
&lt;ul&gt;
&lt;li&gt;Added a 26-pin GPIO connector with board dimensions of model B+&lt;br/&gt;
       for backwards compatibility with models A and B, named &amp;quot;B-&amp;quot;&lt;/li&gt;
&lt;/ul&gt;

Version 1.1
&lt;ul&gt;
&lt;li&gt;New GPIO connector and board dimensions of model B+&lt;/li&gt;
&lt;li&gt;Old connector and board (for models A and B) renamed to AB&lt;/li&gt;
&lt;li&gt;GPIO pin numbers on connector changed to match Rev2 board design&lt;/li&gt;
&lt;/ul&gt;

Version 1.0
&lt;ul&gt;
&lt;li&gt;More detailed descriptions for all components&lt;/li&gt;
&lt;li&gt;Published on Cadsoft webpage&lt;/li&gt;
&lt;/ul&gt;

&lt;hr&gt;&lt;br/&gt;

Designed by &lt;a href="http://bastelstube.rocci.net/"&gt;Martin's Bastelstube&lt;/a&gt;&lt;br&gt;
Comments / complaints / bug reports / suggestions to &lt;author&gt;eightbit@web.de&lt;/author&gt;</description>
<packages>
<package name="RASPI_BOARD_AB_THIN">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P0" library="pinhead" package="2X08" value=""/>
<element name="X1" library="raspberrypi_bastelstube_v12" package="RASPI_BOARD_AB_THIN" value="RASPI_BOARD_AB_T"/>
<element name="P1" library="pinhead" package="2X08" value=""/>
</elements>
<signals>
<signal name="5V0">
<contactref element="X1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="P0" pad="4"/>
<contactref element="X1" pad="6"/>
<contactref element="P1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="P0" pad="2"/>
<contactref element="X1" pad="12"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="11"/>
<contactref element="P0" pad="1"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="15"/>
<contactref element="P0" pad="3"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="16"/>
<contactref element="P0" pad="5"/>
<contactref element="P1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="22"/>
<contactref element="P0" pad="7"/>
<contactref element="P1" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="X1" pad="18"/>
<contactref element="P0" pad="6"/>
<contactref element="P1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="26"/>
<contactref element="P0" pad="9"/>
<contactref element="P1" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="X1" pad="21"/>
<contactref element="P0" pad="11"/>
<contactref element="P1" pad="11"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="24"/>
<contactref element="P0" pad="10"/>
<contactref element="P1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="X1" pad="19"/>
<contactref element="P0" pad="12"/>
<contactref element="P1" pad="12"/>
</signal>
<signal name="N$12">
<contactref element="X1" pad="3"/>
<contactref element="P0" pad="15"/>
<contactref element="P1" pad="15"/>
</signal>
<signal name="N$13">
<contactref element="X1" pad="5"/>
<contactref element="P0" pad="13"/>
<contactref element="P1" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="X1" pad="7"/>
<contactref element="P0" pad="14"/>
<contactref element="P1" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
