<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.17" y2="-0.0762" width="0" layer="20"/>
<wire x1="63.17" y1="-0.0762" x2="63.17" y2="14.3283" width="0" layer="20"/>
<wire x1="63.17" y1="14.3283" x2="6.35" y2="14.3383" width="0" layer="20"/>
<wire x1="6.35" y1="14.3383" x2="6.35" y2="14.3283" width="0" layer="20"/>
<wire x1="6.35" y1="14.3283" x2="0" y2="14.3283" width="0" layer="20"/>
<wire x1="0" y1="14.3283" x2="0" y2="0" width="0" layer="20"/>
<text>VEX UART-AM Converter v1.0</text>
<text>TX</text>
<text>RX</text>
<text>VCC</text>
<text>GND</text>
<text>DATA</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>DATA</text>
<text>GND</text>
<text>BTN1</text>
<text>MISO</text>
<text>SCK</text>
<text>RST</text>
<text>VCC</text>
<text>MOSI</text>
<text>GND</text>
<text>Designed by Nicholas Junker</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="SOIC127P798X216-8N">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="adafruit" package="1X03" value="TX">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP2" library="adafruit" package="1X03" value="RX">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP3" library="adafruit" package="1X01" value="RX">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP4" library="adafruit" package="2X04" value="UART">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="SOIC127P798X216-8N" value="ATTINY85-20SU">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="68T3810"/>
<attribute name="MPN" value="ATTINY85-20SU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1455164"/>
<attribute name="NAME"/>
<attribute name="MF" value=""/>
</element>
<element name="JP5" library="adafruit" package="1X03" value="BTN">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="01N6987"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCHP05W4F1000T5E"/>
</element>
<element name="JP6" library="adafruit" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP4" pad="7"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP3" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="7"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="2"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="3"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP7" pad="3"/>
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
