<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35" y2="0" width="0" layer="20"/>
<wire x1="35" y1="0" x2="35" y2="35" width="0" layer="20"/>
<wire x1="35" y1="35" x2="0" y2="35" width="0" layer="20"/>
<wire x1="0" y1="35" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="TI_MSP430_v16">
<packages>
<package name="RGZ48">
<description>*** TI: RGZ *** JEDEC: S-PQFP-N48 *** 48 PINS *** 
---&gt; PIN TP (exposed thermal die pad) should be connected with GND</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="16LPCC">
</package>
<package name="QFN-24">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="1X02">
</package>
<package name="0603">
</package>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SpriteAntenna">
<packages>
<package name="ANTENNA">
</package>
</packages>
</library>
<library name="TASC">
<packages>
<package name="TASC">
</package>
</packages>
</library>
<library name="ABM11">
<packages>
<package name="ABM11_CERAMIC-SMD-CRYSTAL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="TI_MSP430_v16" package="RGZ48" value="CC430F5137"/>
<element name="C1" library="SparkFun" package="0603-CAP" value="27pF"/>
<element name="C2" library="SparkFun" package="0603-CAP" value="27pF"/>
<element name="R1" library="rcl" package="R0603" value="56K"/>
<element name="C3" library="rcl" package="C0603" value="470nF"/>
<element name="C4" library="rcl" package="C0603" value="470nF"/>
<element name="U2" library="SparkFun" package="16LPCC" value="HMC5883LSMD"/>
<element name="C11" library="SparkFun" package="0603-CAP" value="100nF"/>
<element name="C12" library="SparkFun" package="0603-CAP" value="220nF"/>
<element name="C13" library="SparkFun" package="0603-CAP" value="4.7uF"/>
<element name="U3" library="SparkFun" package="QFN-24" value="ITG-3200"/>
<element name="C8" library="SparkFun" package="0603-CAP" value="2.2nF"/>
<element name="C9" library="SparkFun" package="0603-CAP" value="100nF"/>
<element name="C10" library="SparkFun" package="0603-CAP" value="10nF"/>
<element name="R3" library="SparkFun" package="0603-RES" value="4.7K"/>
<element name="R4" library="SparkFun" package="0603-RES" value="4.7K"/>
<element name="JP2" library="SparkFun" package="1X02" value=""/>
<element name="JP1" library="SparkFun" package="1X02" value=""/>
<element name="ANT-N" library="SpriteAntenna" package="ANTENNA" value="ANTENNA"/>
<element name="ANT-P" library="SpriteAntenna" package="ANTENNA" value="ANTENNA"/>
<element name="R2" library="SparkFun" package="0603-RES" value="47K"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="2.2nF"/>
<element name="L1" library="SparkFun" package="0603" value="12 nH"/>
<element name="C7" library="SparkFun" package="0603-CAP" value="10nF"/>
<element name="C6" library="SparkFun" package="0603-CAP" value="100nF"/>
<element name="S1" library="TASC" package="TASC" value="TASC"/>
<element name="LED1" library="SparkFun" package="LED-0603" value=""/>
<element name="R5" library="SparkFun" package="0603-RES" value="270R"/>
<element name="X1" library="ABM11" package="ABM11_CERAMIC-SMD-CRYSTAL" value="26 MHz"/>
<element name="JP4" library="SparkFun" package="1X02" value=""/>
<element name="JP3" library="SparkFun" package="1X02" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="U3" pad="13"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="C10" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="45"/>
<contactref element="U1" pad="41"/>
<contactref element="U1" pad="34"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="8"/>
<contactref element="L1" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="TP"/>
<contactref element="U1" pad="42"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U2" pad="9"/>
<contactref element="U2" pad="11"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="11"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="9"/>
<contactref element="U3" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="S1" pad="MINUS1"/>
<contactref element="S1" pad="MINUS2"/>
<contactref element="LED1" pad="C"/>
<contactref element="X1" pad="P$4"/>
<contactref element="X1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="26"/>
<contactref element="C2" pad="1"/>
<contactref element="X1" pad="P$3"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="25"/>
<contactref element="C1" pad="1"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="33"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="7"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="RFN">
<contactref element="U1" pad="30"/>
<contactref element="ANT-N" pad="IN1"/>
<contactref element="ANT-N" pad="IN3"/>
<contactref element="ANT-N" pad="IN2"/>
</signal>
<signal name="RFP">
<contactref element="U1" pad="29"/>
<contactref element="ANT-P" pad="IN1"/>
<contactref element="ANT-P" pad="IN3"/>
<contactref element="ANT-P" pad="IN2"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="40"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="TEST">
<contactref element="U1" pad="39"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="23"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U2" pad="16"/>
<contactref element="U3" pad="24"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="8"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="12"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="10"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U3" pad="20"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="10"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="VCCRF">
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="31"/>
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="28"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="VSOLAR">
<contactref element="JP4" pad="1"/>
<contactref element="S1" pad="PLUS"/>
</signal>
<signal name="TXD">
<contactref element="JP3" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="RXD">
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
