<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="10" y1="0" x2="0" y2="10" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="10" x2="10" y2="20" width="0" layer="20" curve="-90"/>
<wire x1="10" y1="20" x2="20" y2="10" width="0" layer="20" curve="-90"/>
<wire x1="20" y1="10" x2="10" y2="0" width="0" layer="20" curve="-90"/>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
</plain>
<libraries>
<library name="A_butts">
<packages>
<package name="LED5MM_SHORTPADS">
</package>
<package name="1X01NSATALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R3" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="W2" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="R1" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="W3" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="R2" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="W4" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="W1" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="W5" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="R4" library="A_butts" package="LED5MM_SHORTPADS" value="LED5MM_SHORTPADS"/>
<element name="WHITE" library="A_butts" package="1X01NSATALL" value="M01PTH-NS-NOTSUCK"/>
<element name="VCC" library="A_butts" package="1X01NSATALL" value="M01PTH-NS-NOTSUCK"/>
<element name="RED" library="A_butts" package="1X01NSATALL" value="M01PTH-NS-NOTSUCK"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="W1" pad="K"/>
<contactref element="W2" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="W2" pad="K"/>
<contactref element="W3" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="W3" pad="K"/>
<contactref element="W4" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="W4" pad="K"/>
<contactref element="W5" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="A"/>
<contactref element="R1" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="K"/>
<contactref element="R3" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="K"/>
<contactref element="R4" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="W5" pad="K"/>
<contactref element="WHITE" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="K"/>
<contactref element="RED" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="W1" pad="A"/>
<contactref element="VCC" pad="1"/>
<contactref element="R1" pad="A"/>
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
</signals>
</board>
</drawing>
</eagle>
