<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0.127" y1="1.397" x2="0.127" y2="29.62275" width="0.0508" layer="20"/>
<wire x1="19.304" y1="29.62275" x2="19.304" y2="1.397" width="0.0508" layer="20"/>
<text>Ant</text>
<text>SD</text>
<text>C2</text>
<text>GND</text>
<text>IRQ</text>
<text>CSN</text>
<text>SDI</text>
<text>SDO</text>
<text>SCK</text>
<text>RFM</text>
<text>IRQ</text>
<text>RFM69W/SD/Flash</text>
<text>3V3</text>
<text>VCC</text>
<text>GND</text>
<text>CE</text>
<text>433 MHz 165 mm
868 MHz  82 mm</text>
<text>V1.0</text>
<text>R4</text>
<text>http://hallard.me
V1.0</text>
<wire x1="18.034" y1="0.127" x2="1.397" y2="0.127" width="0.0508" layer="20"/>
<wire x1="18.034" y1="30.89275" x2="19.304" y2="29.62275" width="0.0508" layer="20" curve="-90"/>
<wire x1="1.397" y1="30.89275" x2="0.127" y2="29.62275" width="0.0508" layer="20" curve="90"/>
<wire x1="18.034" y1="0.127" x2="19.304" y2="1.397" width="0.0508" layer="20" curve="90"/>
<wire x1="1.397" y1="0.127" x2="0.127" y2="1.397" width="0.0508" layer="20" curve="-90"/>
<wire x1="1.36525" y1="30.89275" x2="18.034" y2="30.89275" width="0.0508" layer="20"/>
<text>IRQ</text>
<text>CSN</text>
<text>SDI</text>
<text>3V3</text>
<text>GND</text>
<text>SDO</text>
<text>SCK</text>
<text>CE</text>
<text>RFM69(H)W</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
</plain>
<libraries>
<library name="JeeLabs">
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-Connector">
<packages>
<package name="2X4P-2.54">
</package>
</packages>
</library>
<library name="Connector">
<packages>
<package name="9P-SMD-W/-RING">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="RFM69W">
<description>Generated from &lt;b&gt;untitled.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs-replace.ulp</description>
<packages>
<package name="RFM69W-MINPADS">
</package>
</packages>
</library>
<library name="_c2h">
<packages>
<package name="0805-RES">
</package>
<package name="0805-CAP">
</package>
<package name="0805-LED-LARGEPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANT." library="JeeLabs" package="1,6/0,8" value="433 Mhz">
<attribute name="VALUE"/>
</element>
<element name="J1" library="Seeed-Connector" package="2X4P-2.54" value="NRF connector"/>
<element name="J2" library="Connector" package="9P-SMD-W/-RING" value="SD card">
<attribute name="VALUE"/>
</element>
<element name="C2" library="_c2h" package="0805-CAP" value="100nF"/>
<element name="R1" library="_c2h" package="0805-RES" value="1K"/>
<element name="R2" library="_c2h" package="0805-RES" value="1K"/>
<element name="R3" library="_c2h" package="0805-RES" value="1K"/>
<element name="AT25512" library="Atmel_By_element14_Batch_1" package="SOIC127P600X175-8N" value="Flash">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="12T1360"/>
<attribute name="MPN" value="AT25512N-SH-B"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1841581"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="_c2h" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
</element>
<element name="U$1" library="RFM69W" package="RFM69W-MINPADS" value="RFM69"/>
<element name="R4" library="_c2h" package="0805-RES" value="100"/>
<element name="U$2" library="_c2h" package="0805-LED-LARGEPADS" value="LED0805-LARGE"/>
<element name="U$3" library="_c2h" package="0805-LED-LARGEPADS" value="LED0805-LARGE"/>
<element name="U$4" library="_c2h" package="0805-LED-LARGEPADS" value="LED0805-LARGE"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="G2"/>
<contactref element="J2" pad="G1"/>
<contactref element="J2" pad="G3"/>
<contactref element="J2" pad="G4"/>
<contactref element="AT25512" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="AT25512" pad="8"/>
<contactref element="AT25512" pad="8"/>
<contactref element="AT25512" pad="3"/>
<contactref element="AT25512" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="VDD"/>
<contactref element="U$1" pad="VDD"/>
</signal>
<signal name="N$1">
<contactref element="ANT." pad="1"/>
<contactref element="U$1" pad="ANT"/>
</signal>
<signal name="N$4">
</signal>
<signal name="CE">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="AT25512" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U$2" pad="MINUS"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="5"/>
<contactref element="AT25512" pad="6"/>
<contactref element="U$1" pad="SCK"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="7"/>
<contactref element="AT25512" pad="2"/>
<contactref element="U$1" pad="MISO"/>
</signal>
<signal name="CSN">
<contactref element="J1" pad="7"/>
<contactref element="U$1" pad="NSS"/>
<contactref element="U$3" pad="MINUS"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="3"/>
<contactref element="AT25512" pad="5"/>
<contactref element="U$1" pad="MOSI"/>
</signal>
<signal name="IRQ">
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="DIO0"/>
<contactref element="U$4" pad="MINUS"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="PLUS"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="U$3" pad="PLUS"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="U$4" pad="PLUS"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="U$1" pad="DIO2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
