<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="31.42" y1="5.160084375" x2="31.42" y2="35.47729375" width="0" layer="20"/>
<wire x1="31.42" y1="35.47729375" x2="26.26729375" y2="40.63" width="0" layer="20" curve="90"/>
<wire x1="26.26729375" y1="40.63" x2="4.573509375" y2="40.63" width="0" layer="20"/>
<wire x1="4.573509375" y1="40.63" x2="0" y2="36.056490625" width="0" layer="20" curve="90"/>
<wire x1="0" y1="36.056490625" x2="0" y2="5.23634375" width="0" layer="20"/>
<wire x1="0" y1="5.23634375" x2="5.23634375" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.23634375" y1="0" x2="26.259915625" y2="0" width="0" layer="20"/>
<wire x1="26.259915625" y1="0" x2="31.42" y2="5.160084375" width="0" layer="20" curve="90"/>
<text>Red Llama Clone Rev 1.0</text>
<text>Visit lemonlimefx.wordpress.com</text>
</plain>
<libraries>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-pots">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;chassis-mount (e.g., Alpha 16mm) pots&lt;/li&gt;
&lt;li&gt;board-mount trim pots (1/4" and 3/8")&lt;/li&gt;
&lt;li&gt; all pot values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="POT">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;3 terminals for circuit board for wires connecting to 3 lugs of pot off-board</description>
</package>
</packages>
</library>
<library name="gm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="logos">
<packages>
<package name="LOGO-3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+9V1" library="gm-supply" package="SQUARE" value="+9V(T)">
<attribute name="NAME"/>
</element>
<element name="C1" library="gm-caps-film-box" package="072X025" value="0.068uF"/>
<element name="C2" library="gm-caps-film-box" package="072X025" value="51pF"/>
<element name="C3" library="gm-caps-film-box" package="072X025" value="100pF"/>
<element name="C4" library="gm-caps-film-box" package="072X025" value="0.033uF"/>
<element name="C5" library="gm-caps-electro-pol" package="050_020" value="10uF Tantalum"/>
<element name="C6" library="gm-caps-electro-pol" package="050_020" value="330uF"/>
<element name="D1" library="gm-diodes" package="DO41-3" value="1N4004"/>
<element name="GAIN" library="gm-pots" package="POT" value="1M-B"/>
<element name="GND1" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="IC1" library="gm-ics" package="DIL16" value="CD4049UBE"/>
<element name="IN1" library="gm-supply" package="SQUARE" value="IN(T)">
<attribute name="NAME"/>
</element>
<element name="OUT1" library="gm-supply" package="SQUARE" value="OUT(T)">
<attribute name="NAME"/>
</element>
<element name="R1" library="gm-resistors" package="R0207/3" value="100K"/>
<element name="R2" library="gm-resistors" package="R0207/3" value="100K"/>
<element name="R3" library="gm-resistors" package="R0207/3" value="1M"/>
<element name="R4" library="gm-resistors" package="R0207/3" value="1K"/>
<element name="R5" library="gm-resistors" package="R0207/3" value="1M"/>
<element name="VOLUME" library="gm-pots" package="POT" value="10K-A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="U$1" library="logos" package="LOGO-3" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="GAIN" pad="2"/>
<contactref element="GAIN" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="GAIN" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="2"/>
<contactref element="C5" pad="+"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C5" pad="-"/>
<contactref element="VOLUME" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="1"/>
<contactref element="C6" pad="+"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="A"/>
<contactref element="C6" pad="-"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="14"/>
<contactref element="VOLUME" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="GND1" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="VOLUME" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="OUT1" pad="1"/>
</signal>
<signal name="IN">
<contactref element="IN1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="+9V">
<contactref element="+9V1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
