<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.16" y2="0" width="0" layer="20"/>
<wire x1="10.16" y1="0" x2="10.16" y2="13.97" width="0" layer="20"/>
<wire x1="10.16" y1="13.97" x2="0" y2="13.97" width="0" layer="20"/>
<wire x1="0" y1="13.97" x2="0" y2="0" width="0" layer="20"/>
<text>Tiny TeRP Light Board</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="zigbot">
<packages>
<package name="THRU6">
</package>
</packages>
</library>
<library name="gecko">
<description>Keystone
Surface &amp; Thru hole mount compact contacts
http://www.keyelco.com/pdfs/M55p4.pdf</description>
<packages>
<package name="T_4LEAD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0402-CAP" value="0.1 uF"/>
<element name="U$1" library="zigbot" package="THRU6" value="THRU6"/>
<element name="U$2" library="zigbot" package="THRU6" value="THRU6"/>
<element name="U1" library="gecko" package="T_4LEAD" value="TSL237T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="U1" pad="VDD"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="OUT">
<contactref element="U1" pad="OUT"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="GND"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U1" pad="!OE"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
