<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.1275" y1="0.05" x2="100.19" y2="0.05" width="0" layer="20"/>
<wire x1="0.1275" y1="53.39" x2="0.1275" y2="0.05" width="0" layer="20"/>
<wire x1="107.81" y1="45.77" x2="100.19" y2="53.39" width="0" layer="20" curve="89.998496"/>
<wire x1="107.81" y1="7.67" x2="100.19" y2="0.05" width="0" layer="20" curve="-89.998496"/>
<wire x1="0.1275" y1="53.39" x2="100.19" y2="53.39" width="0" layer="20"/>
<wire x1="107.81" y1="45.77" x2="107.81" y2="7.67" width="0" layer="20"/>
<wire x1="0.1275" y1="0.05" x2="100.19" y2="0.05" width="0" layer="46"/>
<wire x1="0.1275" y1="53.39" x2="0.1275" y2="0.05" width="0" layer="46"/>
<wire x1="107.81" y1="45.77" x2="100.19" y2="53.39" width="0" layer="46" curve="89.998496"/>
<wire x1="107.81" y1="7.67" x2="100.19" y2="0.05" width="0" layer="46" curve="-89.998496"/>
<wire x1="0.1275" y1="53.39" x2="100.19" y2="53.39" width="0" layer="46"/>
<wire x1="107.81" y1="45.77" x2="107.81" y2="7.67" width="0" layer="46"/>
<text>Rev.E</text>
<text>JP</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="L2012C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="SOT363_PHILIPS">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt;&lt;p&gt;
Philips Semiconductors, SOT363.pdf</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Hirose-USB">
<packages>
<package name="ZX62-B-5PA-LONG">
</package>
</packages>
</library>
<library name="Hirose-UFL">
<packages>
<package name="U.FL-R-SMT">
</package>
</packages>
</library>
<library name="Murata-TZC3P">
<packages>
<package name="TZC3P">
<description>&lt;b&gt;Trimm capacitor&lt;/b&gt; AVX</description>
</package>
</packages>
</library>
<library name="_ATxmega">
<packages>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
</packages>
</library>
<library name="TLVH431">
<packages>
<package name="SOT23">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="74LVC1G74">
<packages>
<package name="VSSOP8">
</package>
</packages>
</library>
<library name="74xx-little-de">
<packages>
<package name="SC70-5">
<description>&lt;b&gt;SMT SC70-5&lt;/b&gt;&lt;p&gt;
SOT353 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="TXC-Crystal">
<packages>
<package name="5MMX3.2MM">
</package>
</packages>
</library>
<library name="Avago-HSM">
<packages>
<package name="HSMX-C110">
</package>
</packages>
</library>
<library name="Omron-B3U">
<packages>
<package name="B3U-3000P-B">
</package>
</packages>
</library>
<library name="NXP-BZX384">
<packages>
<package name="SOD323">
<description>&lt;b&gt;Small Outline Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="6PAD_ISP">
</package>
</packages>
</library>
<library name="jakob">
<packages>
<package name="SNOWDEN_BACK">
</package>
<package name="FRA_FRONT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C13" library="rcl" package="C1206K" value="10u/6.3V/X5R">
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C1206" value="N.M.">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS138BK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="10R">
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R1206" value="470R">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C1206K" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C1206K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R1206" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0603K" value="22p/NP0">
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603K" value="220p">
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0603" value="47k">
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L2012C" value="33R@100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0603K" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT363_PHILIPS" value="BAS70-07S">
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="SOT363_PHILIPS" value="BAS70-07S">
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="SOT363_PHILIPS" value="BAS70-07S">
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SOT363_PHILIPS" value="BAS70-07S">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-npn" package="SOT23" value="BC846B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603K" value="100n">
<attribute name="VALUE"/>
</element>
<element name="X1" library="Hirose-USB" package="ZX62-B-5PA-LONG" value="ZX62-B-5PA">
<attribute name="VALUE"/>
</element>
<element name="X3" library="Hirose-UFL" package="U.FL-R-SMT" value="U.FL-R-SMT">
<attribute name="VALUE"/>
</element>
<element name="C14" library="Murata-TZC3P" package="TZC3P" value="TZC3P200A110">
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R1206" value="1Meg">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C1206K" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="TLVH431" package="SOT23" value="TLVH431(A)IDBZR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0603" value="200k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="120k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R1206" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="SOT363_PHILIPS" value="BAS70-07S">
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0603" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT363_PHILIPS" value="BAS70-07S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="_ATxmega" package="TQFP44" value="ATxmega32A4U-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0603" value="220R">
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0603K" value="100n">
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0603" value="220R">
<attribute name="VALUE"/>
</element>
<element name="IC3" library="74LVC1G74" package="VSSOP8" value="SN74LVC1G74DCU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="74xx-little-de" package="SC70-5" value="SN74LVC1G08DCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="74xx-little-de" package="SC70-5" value="SN74LVC1G86DCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="TXC-Crystal" package="5MMX3.2MM" value="12MHz">
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603K" value="18p">
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0603K" value="18p">
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="Avago-HSM" package="HSMX-C110" value="HSMS-C110">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="Avago-HSM" package="HSMX-C110" value="HSMG-C110">
<attribute name="VALUE"/>
</element>
<element name="SW2" library="Omron-B3U" package="B3U-3000P-B" value="B3U-3000P-B">
<attribute name="VALUE"/>
</element>
<element name="D7" library="NXP-BZX384" package="SOD323" value="BZX384-C2V7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SparkFun" package="SO08" value="AT45DB081D-SSU">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="avr-7" package="6PAD_ISP" value="AVR-ISP-6-EDGE"/>
<element name="U$2" library="jakob" package="SNOWDEN_BACK" value=""/>
<element name="U$3" library="jakob" package="FRA_FRONT" value=""/>
</elements>
<signals>
<signal name="ANTENNA-A">
<contactref element="D6" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D4" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="D3" pad="3"/>
<contactref element="D6" pad="4"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="D5" pad="4"/>
<contactref element="X3" pad="GND2"/>
</signal>
<signal name="VCC">
<contactref element="R12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="D2" pad="6"/>
<contactref element="R10" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="D1" pad="6"/>
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="39"/>
<contactref element="IC2" pad="31"/>
<contactref element="IC2" pad="19"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="8"/>
<contactref element="C5" pad="1"/>
<contactref element="D1" pad="3"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC4" pad="5"/>
<contactref element="C12" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="6"/>
<contactref element="U$1" pad="RST"/>
</signal>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="D2" pad="4"/>
<contactref element="D4" pad="4"/>
<contactref element="D3" pad="4"/>
<contactref element="R19" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="X1" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="30"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="38"/>
<contactref element="R21" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="IC3" pad="4"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC4" pad="3"/>
<contactref element="C12" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="SW2" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="U$1" pad="MISO"/>
</signal>
<signal name="USB-DM">
<contactref element="IC2" pad="26"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="USB-DP">
<contactref element="IC2" pad="27"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="USB-SENSE">
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="N$10">
<contactref element="R12" pad="1"/>
<contactref element="D4" pad="6"/>
<contactref element="D3" pad="6"/>
</signal>
<signal name="HALFCARRIER">
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="MOD-DEMOD">
<contactref element="R17" pad="2"/>
<contactref element="D6" pad="6"/>
<contactref element="D6" pad="3"/>
</signal>
<signal name="DEMOD/MOSI/ASYNC">
<contactref element="Q2" pad="3"/>
<contactref element="R14" pad="1"/>
<contactref element="IC2" pad="15"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="R17" pad="1"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$56">
<contactref element="C16" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="X1" pad="P$2"/>
<contactref element="C3" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="C1" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="U1" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="DEMOD-PWR">
<contactref element="R11" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$66">
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="D1" pad="4"/>
</signal>
<signal name="MOD-DEMOD1">
<contactref element="C16" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="D5" pad="6"/>
<contactref element="D5" pad="3"/>
</signal>
<signal name="N$12345">
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="PDI-DATA">
<contactref element="IC2" pad="34"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="PDI-CLK">
<contactref element="IC2" pad="35"/>
<contactref element="R5" pad="1"/>
<contactref element="U$1" pad="VCC"/>
</signal>
<signal name="N$1">
<contactref element="R19" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="RSSI">
<contactref element="C19" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="FLASH-CS">
<contactref element="IC2" pad="24"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="FLASH-SCK">
<contactref element="IC2" pad="21"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="FLASH-MISO">
<contactref element="IC2" pad="22"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="FLASH-MOSI">
<contactref element="IC2" pad="23"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$1234">
<contactref element="R15" pad="2"/>
<contactref element="D2" pad="3"/>
<contactref element="D2" pad="1"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="36"/>
<contactref element="Q3" pad="3"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="37"/>
<contactref element="Q3" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="BUTTON">
<contactref element="IC2" pad="2"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="LED-RED">
<contactref element="R7" pad="1"/>
<contactref element="IC2" pad="44"/>
</signal>
<signal name="LED-GREEN">
<contactref element="R6" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R16" pad="2"/>
<contactref element="X3" pad="SIG"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="D7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC5" pad="2"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="SUBCARRIER-PSK">
<contactref element="IC4" pad="2"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="1"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R6" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="BITRATE/SCK">
<contactref element="IC2" pad="17"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="LOADMOD/MISO">
<contactref element="IC4" pad="1"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="SUBCARRIER-OOK">
<contactref element="IC5" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="MODSTART/SS">
<contactref element="IC2" pad="14"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
