<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="82.55" y2="0" width="0" layer="20"/>
<wire x1="82.55" y1="0" x2="82.55" y2="55.88" width="0" layer="20"/>
<wire x1="82.55" y1="55.88" x2="0" y2="55.88" width="0" layer="20"/>
<wire x1="0" y1="55.88" x2="0" y2="0" width="0" layer="20"/>
<text>ASIM
Multiplexer
v1</text>
<text>USB</text>
<text>1 2</text>
<text>8 7</text>
<text>ASIM</text>
<text>Adafruit
FT232H
Breakout</text>
<text>3 4</text>
<text>6 5</text>
<hole x="5.4356" y="51.181" drill="3.2"/>
<hole x="77.1906" y="51.181" drill="3.2"/>
<hole x="77.1906" y="5.4102" drill="3.2"/>
<hole x="5.4356" y="5.4102" drill="3.2"/>
</plain>
<libraries>
<library name="analog-devices">
<description>&lt;b&gt;Analog Devices Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="analog-devices" package="DIL16" value="ADG608N">
<attribute name="OC_NEWARK" value="15P0383"/>
<attribute name="MPN" value="ADG608BNZ"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1438944"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="analog-devices" package="DIL16" value="ADG608N">
<attribute name="OC_NEWARK" value="15P0383"/>
<attribute name="MPN" value="ADG608BNZ"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1438944"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="analog-devices" package="DIL16" value="ADG608N">
<attribute name="OC_NEWARK" value="15P0383"/>
<attribute name="MPN" value="ADG608BNZ"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1438944"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="analog-devices" package="DIL16" value="ADG608N">
<attribute name="OC_NEWARK" value="15P0383"/>
<attribute name="MPN" value="ADG608BNZ"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1438944"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J2" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J3" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J4" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J5" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J6" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J7" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J8" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="J9" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="14"/>
<contactref element="IC3" pad="14"/>
<contactref element="IC4" pad="14"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="485_EN">
<contactref element="JP2" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="485_A2">
<contactref element="JP2" pad="4"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="485_A1">
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="485_A0">
<contactref element="JP2" pad="6"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="232_EN">
<contactref element="JP2" pad="7"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="232_A2">
<contactref element="JP2" pad="8"/>
<contactref element="IC3" pad="15"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="232_A1">
<contactref element="JP2" pad="9"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="232_A0">
<contactref element="JP2" pad="10"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="485A">
<contactref element="J1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="485B">
<contactref element="J1" pad="2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="232TX">
<contactref element="J1" pad="5"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="232RX">
<contactref element="J1" pad="6"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="232_GND">
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="7"/>
<contactref element="J3" pad="7"/>
<contactref element="J4" pad="7"/>
<contactref element="J5" pad="7"/>
<contactref element="J6" pad="7"/>
<contactref element="J7" pad="7"/>
<contactref element="J8" pad="7"/>
<contactref element="J9" pad="7"/>
</signal>
<signal name="485_GND">
<contactref element="J1" pad="8"/>
<contactref element="J2" pad="8"/>
<contactref element="J3" pad="8"/>
<contactref element="J4" pad="8"/>
<contactref element="J5" pad="8"/>
<contactref element="J6" pad="8"/>
<contactref element="J7" pad="8"/>
<contactref element="J8" pad="8"/>
<contactref element="J9" pad="8"/>
</signal>
<signal name="485A_S1">
<contactref element="J2" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="485B_S1">
<contactref element="J2" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="232TX_S1">
<contactref element="J2" pad="5"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="232RX_S1">
<contactref element="J2" pad="6"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="485A_S2">
<contactref element="J3" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="485B_S2">
<contactref element="J3" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="232TX_S2">
<contactref element="J3" pad="5"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="232RX_S2">
<contactref element="J3" pad="6"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="485A_S3">
<contactref element="J4" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="485B_S3">
<contactref element="J4" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="232TX_S3">
<contactref element="J4" pad="5"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="232RX_S3">
<contactref element="J4" pad="6"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="485A_S5">
<contactref element="J6" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="485B_S5">
<contactref element="J6" pad="2"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="232TX_S5">
<contactref element="J6" pad="5"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="232RX_S5">
<contactref element="J6" pad="6"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="485A_S6">
<contactref element="J7" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="485B_S6">
<contactref element="J7" pad="2"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="232TX_S6">
<contactref element="J7" pad="5"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="232RX_S6">
<contactref element="J7" pad="6"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="485A_S4">
<contactref element="J5" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="485B_S4">
<contactref element="J5" pad="2"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="232TX_S4">
<contactref element="J5" pad="5"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="232RX_S4">
<contactref element="J5" pad="6"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="485A_S7">
<contactref element="J8" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="485B_S7">
<contactref element="J8" pad="2"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="232TX_S7">
<contactref element="J8" pad="5"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="232RX_S7">
<contactref element="J8" pad="6"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="485A_S8">
<contactref element="J9" pad="1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="485B_S8">
<contactref element="J9" pad="2"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="232TX_S8">
<contactref element="J9" pad="5"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="232RX_S8">
<contactref element="J9" pad="6"/>
<contactref element="IC4" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
