<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22" y2="0" width="0" layer="20"/>
<wire x1="22" y1="0" x2="22" y2="31" width="0" layer="20"/>
<wire x1="22" y1="31" x2="0" y2="31" width="0" layer="20"/>
<wire x1="0" y1="31" x2="0" y2="0" width="0" layer="20"/>
<text>470Ω</text>
<text>1KΩ</text>
<text>PHOTO</text>
<text>TRIMPOT</text>
</plain>
<libraries>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
 grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-3-2-07">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B25X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP11">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.1 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="transistor-npn" package="TO92-EBC" value="BC548">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-3-2-07" package="AXIAL-0.3" value=""/>
<element name="R2" library="SparkFun-3-2-07" package="AXIAL-0.3" value=""/>
<element name="R3" library="SparkFun-3-2-07" package="AXIAL-0.3" value=""/>
<element name="R4" library="pot" package="B25X" value=""/>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="9V" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="Q1" pad="C"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="B"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="P$2"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="E"/>
</signal>
<signal name="GND">
<contactref element="Q1" pad="E"/>
<contactref element="R3" pad="P$2"/>
<contactref element="GND" pad="MP"/>
</signal>
<signal name="VCC">
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="R4" pad="S"/>
<contactref element="9V" pad="MP"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="P$1"/>
<contactref element="R4" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
