<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="25" y1="19" x2="5.5" y2="19" width="0" layer="20"/>
<wire x1="5.5" y1="19" x2="4.5" y2="18" width="0" layer="20" curve="90"/>
<wire x1="4.5" y1="18" x2="4.5" y2="5.5" width="0" layer="20"/>
<wire x1="4.5" y1="5.5" x2="5.5" y2="4.5" width="0" layer="20" curve="90"/>
<wire x1="5.5" y1="4.5" x2="25" y2="4.5" width="0" layer="20"/>
<wire x1="25" y1="4.5" x2="26" y2="5.5" width="0" layer="20" curve="90"/>
<wire x1="26" y1="5.5" x2="26" y2="18" width="0" layer="20"/>
<wire x1="26" y1="18" x2="25" y2="19" width="0" layer="20" curve="90"/>
<text>RX</text>
<text>TX</text>
<text>JAW 2015-03</text>
<text>V3</text>
<text>GD</text>
<text>RX</text>
<text>TX</text>
<text>V3</text>
<text>GD</text>
<text>RX</text>
<text>TX</text>
<text>www.A791RL.com</text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SSOP-16-FTDI">
<description>SSOP-16, 0.32 x 1.26 mm pad, 0.63mm pitch, 6.82mm Pad length</description>
</package>
<package name="M1X4">
</package>
<package name="CONN_USB_MICRO-B">
<description>USB micro-b connector SMT 0.65 mm pitch,
1.45mm from center to PCB edge,
Based on TE part number 1981568-1</description>
</package>
</packages>
</library>
<library name="jaw">
<packages>
<package name="SMD0603">
</package>
<package name="SMD0603D">
</package>
<package name="SOT-23-5">
</package>
<package name="ROBOTMAN-LOGO">
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U8" library="dp_devices" package="SSOP-16-FTDI" value="IC_FT230X-SSOP-16">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="jaw" package="SMD0603" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0603" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0603" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="jaw" package="SMD0603D" value="ORANGE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="dp_devices" package="M1X4" value="CON_HEADER_1X04">
<attribute name="NAME"/>
</element>
<element name="VR1" library="jaw" package="SOT-23-5" value="MCP1824">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="dp_devices" package="CONN_USB_MICRO-B" value="CON-USB-F-MICRO-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="jaw" package="SMD0603" value="1+u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="jaw" package="ROBOTMAN-LOGO" value="ROBOTMAN-LOGO"/>
<element name="D1" library="jaw" package="SOD-323" value="DIODESOD-323">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U8" pad="5"/>
<contactref element="U8" pad="13"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="CN2" pad="2"/>
<contactref element="USB1" pad="P5"/>
<contactref element="USB1" pad="P4"/>
<contactref element="VR1" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U8" pad="8"/>
<contactref element="USB1" pad="P3"/>
</signal>
<signal name="N$22">
<contactref element="U8" pad="9"/>
<contactref element="USB1" pad="P2"/>
</signal>
<signal name="N$26">
<contactref element="R1" pad="1"/>
<contactref element="U8" pad="14"/>
</signal>
<signal name="N$27">
<contactref element="R2" pad="1"/>
<contactref element="U8" pad="7"/>
</signal>
<signal name="USB3V3">
<contactref element="U8" pad="3"/>
<contactref element="U8" pad="10"/>
<contactref element="U8" pad="11"/>
<contactref element="C1" pad="1"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$24">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="U8" pad="12"/>
<contactref element="C2" pad="1"/>
<contactref element="USB1" pad="P1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="TXD">
<contactref element="U8" pad="4"/>
<contactref element="CN2" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="U8" pad="1"/>
<contactref element="CN2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="CN2" pad="1"/>
<contactref element="VR1" pad="5"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="VR1" pad="3"/>
<contactref element="VR1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
