<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0.889" y1="0.127" x2="25.9842" y2="0.127" width="0" layer="20"/>
<wire x1="26.7462" y1="0.889" x2="26.7462" y2="36.068" width="0" layer="20"/>
<wire x1="25.7302" y1="36.83" x2="0.889" y2="36.83" width="0" layer="20"/>
<wire x1="0.127" y1="36.068" x2="0.127" y2="0.889" width="0" layer="20"/>
<wire x1="0.889" y1="0.127" x2="0.127" y2="0.889" width="0" layer="20" curve="-90"/>
<wire x1="0.127" y1="36.068" x2="0.889" y2="36.83" width="0" layer="20" curve="-90"/>
<wire x1="25.9842" y1="0.127" x2="26.7462" y2="0.889" width="0" layer="20" curve="90"/>
<wire x1="25.7302" y1="36.83" x2="26.7462" y2="36.068" width="0" layer="20" curve="-90"/>
<text>RST</text>
<text>ISP</text>
<text>mBLE LPC11u24/LPC11u35</text>
<text>Debugger
Prototype V1</text>
<text>March 2015
Colin Szechy</text>
</plain>
<libraries>
<library name="mBLE">
<packages>
<package name="USB_MICRO_B-JST-MC5BR3-M404-4S-TB">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="LED-0603">
</package>
<package name="0805">
</package>
<package name="LQFP48">
</package>
<package name="1X06">
</package>
<package name="M50-3600742">
</package>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SC-70">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="mBLE" package="USB_MICRO_B-JST-MC5BR3-M404-4S-TB" value="MICRO_USB_B_JST_MC5BR3-M404-4S">
<attribute name="MOUSER" value="53X3655"/>
<attribute name="DIGIKEY" value="455-2567-2-ND"/>
</element>
<element name="U$6" library="mBLE" package="SOT23-5" value="LDO">
<attribute name="DIGIKEY" value="296-27893-1-ND"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0402-CAP" value="1uF cer">
<attribute name="NAME"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0402-CAP" value="1 uF cer">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="33">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="33">
<attribute name="NAME"/>
</element>
<element name="PWR" library="mBLE" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="mBLE" package="0805" value="56">
<attribute name="NAME"/>
</element>
<element name="DBUG" library="mBLE" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="mBLE" package="0805" value="56">
<attribute name="NAME"/>
</element>
<element name="U3" library="mBLE" package="LQFP48" value="LPC11UXX_4812FBD48">
<attribute name="EEPROM" value="no"/>
<attribute name="FLASH_SIZE" value="16 kB"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="NAME"/>
</element>
<element name="J4" library="mBLE" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="mBLE" package="M50-3600742" value="">
<attribute name="VALUE"/>
</element>
<element name="S3" library="mBLE" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="0805" value="2k">
<attribute name="NAME"/>
</element>
<element name="S4" library="mBLE" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="0805" value="2k">
<attribute name="NAME"/>
</element>
<element name="TR" library="mBLE" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="mBLE" package="0805" value="56">
<attribute name="NAME"/>
</element>
<element name="USB" library="mBLE" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="mBLE" package="0805" value="56">
<attribute name="NAME"/>
</element>
<element name="U$1" library="mBLE" package="SC-70" value="2N7002"/>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="1.5k"/>
<element name="C2" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="U$6" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="U3" pad="41"/>
<contactref element="U3" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="9"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
<contactref element="R12" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="U$6" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U$6" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U$6" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="J4" pad="6"/>
<contactref element="J5" pad="1"/>
<contactref element="PWR" pad="A"/>
<contactref element="U3" pad="44"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="S"/>
</signal>
<signal name="USB_DP">
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="USB_DM">
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="SWDIO">
<contactref element="U3" pad="39"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="DBUG" pad="C"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="U3" pad="19"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="SWDCLK">
<contactref element="U3" pad="29"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="U3" pad="3"/>
<contactref element="J5" pad="10"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="TARGET_SWDIO">
<contactref element="J4" pad="4"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="TARGET_SWDCLK">
<contactref element="J4" pad="3"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="TARGET_NRESET">
<contactref element="J4" pad="1"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="ISP_EN">
<contactref element="U3" pad="4"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="+3V2">
<contactref element="S3" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="BLAH">
<contactref element="S4" pad="1"/>
<contactref element="S4" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="TR" pad="C"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="TRGT_RUN">
<contactref element="TR" pad="A"/>
<contactref element="U3" pad="25"/>
</signal>
<signal name="DBUG_CONND">
<contactref element="DBUG" pad="A"/>
<contactref element="U3" pad="26"/>
</signal>
<signal name="TARGET_NRESET_OE">
<contactref element="U3" pad="35"/>
</signal>
<signal name="TARGET_SWDIO_OE">
<contactref element="U3" pad="36"/>
</signal>
<signal name="TARGET_TDI">
<contactref element="U3" pad="33"/>
</signal>
<signal name="TARGET_TDO">
<contactref element="J4" pad="5"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="USB" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="USB_CONNECT">
<contactref element="USB" pad="A"/>
<contactref element="U3" pad="22"/>
<contactref element="U$1" pad="G"/>
</signal>
<signal name="N$3">
<contactref element="PWR" pad="C"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="D"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
