<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="-19.5" y1="65.77" x2="75.5" y2="65.77" width="0.2032" layer="20"/>
<wire x1="75.5" y1="65.77" x2="78" y2="63.27" width="0.2032" layer="20" curve="-90"/>
<wire x1="-22" y1="63.27" x2="-22" y2="-31.5" width="0.2032" layer="20"/>
<wire x1="-22" y1="-31.5" x2="-19.5" y2="-34" width="0.2032" layer="20" curve="90"/>
<wire x1="-19.5" y1="-34" x2="75.5" y2="-34" width="0.2032" layer="20"/>
<wire x1="75.5" y1="-34" x2="78" y2="-31.5" width="0.2032" layer="20" curve="90"/>
<wire x1="78" y1="-31.5" x2="78" y2="63.27" width="0.2032" layer="20"/>
<wire x1="-19.5" y1="65.77" x2="-22" y2="63.27" width="0.2032" layer="20" curve="90"/>
<text>GND</text>
<text>3V3</text>
<text>5V</text>
<text>12V</text>
<text>ADJ</text>
<text>PWR GOOD</text>
<text>MAINS
ON</text>
<text>5V</text>
<text>GND</text>
<text>OUT</text>
<text>ATX
Breakout 
Board
v1.0</text>
<text>GND</text>
<text>3V3</text>
<text>5V</text>
<text>12V</text>
<text>ADJ</text>
<text>PWR ON</text>
<text>Francesco Truzzi - www.truzzi.me</text>
<text>C:/Users/Fra/Desktop/Untitled-2.bmp</text>
<text>C:/Users/Fra/Desktop/Untitled-3.bmp</text>
<text>Francesco Truzzi - www.truzzi.me</text>
<text>C:/Users/Fra/Desktop/Untitled-2.bmp</text>
<text>C:/Users/Fra/Desktop/Untitled-2.bmp</text>
<text>12V  5V</text>
<text>-12V</text>
<text>-12V</text>
<text>ADJ</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ATX24_RIGHT_ANGLE">
</package>
<package name="1X03">
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="con-berg">
<description>&lt;b&gt;Berg Connectors&lt;/b&gt;&lt;p&gt;
Based on  the following source:
&lt;ul&gt;
&lt;li&gt;http://catalog.fciconnect.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PN87520-S">
<description>&lt;b&gt;USB connector&lt;/b&gt; with shield&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1812">
<description>Multilayer SMD</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220-ADJ">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="PAD_ROUND_4.1MM">
<description>Round pad 4.1mm hole 8mm pad diameter</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="dp_devices.v6">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SW_PUSH_BUTTON_MINI">
</package>
</packages>
</library>
<library name="resistor-power">
<description>&lt;b&gt;Vitrohm Power Resistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="KH214-8">
<description>&lt;b&gt;POWER RESISTOR&lt;/b&gt;&lt;p&gt;
9W, grid 43,18 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_3">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="Fra">
<packages>
<package name="ALPHA_9MM_PCB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="ATX24_RIGHT_ANGLE" value="ATX24RH"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="GREEN">
<attribute name="NAME"/>
</element>
<element name="X1" library="con-berg" package="PN87520-S" value="PN87520-S">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="TO220-ADJ" value="V_REG_317SINK"/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="T1" library="dp_devices" package="PAD_ROUND_4.1MM" value="5V"/>
<element name="T2" library="dp_devices" package="PAD_ROUND_4.1MM" value="3V3"/>
<element name="T3" library="dp_devices" package="PAD_ROUND_4.1MM" value="12V"/>
<element name="T4" library="dp_devices" package="PAD_ROUND_4.1MM" value="GND"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="1.0uF"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T5" library="dp_devices" package="PAD_ROUND_4.1MM" value="ADJ"/>
<element name="F2" library="adafruit" package="1812" value="3A">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="F1" library="adafruit" package="1812" value="3A">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="F4" library="adafruit" package="1812" value="3A">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SW1" library="dp_devices.v6" package="SW_PUSH_BUTTON_MINI" value="SW_PUSH_DPDT">
<attribute name="NAME"/>
</element>
<element name="X2" library="con-berg" package="PN87520-S" value="PN87520-S">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="F3" library="adafruit" package="1812" value="3A">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R9" library="resistor-power" package="KH214-8" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="U$1" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$2" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$3" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$4" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="SJ1" library="SparkFun-Retired" package="SJ_3" value=""/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T6" library="dp_devices" package="PAD_ROUND_4.1MM" value="-12V"/>
<element name="U2" library="SparkFun-DigitalIC" package="SOT23-6" value="TPS2513"/>
<element name="VR1" library="Fra" package="ALPHA_9MM_PCB" value="ALPHA_9MM_PCB"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="X1" pad="4"/>
<contactref element="J1" pad="18"/>
<contactref element="J1" pad="15"/>
<contactref element="J1" pad="19"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="17"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="5"/>
<contactref element="JP2" pad="1"/>
<contactref element="T4" pad="P"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="X2" pad="4"/>
<contactref element="LED7" pad="C"/>
<contactref element="R9" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="U2" pad="2"/>
<contactref element="VR1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="5V_STDBY">
<contactref element="J1" pad="9"/>
<contactref element="R8" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="X1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="12V">
<contactref element="J1" pad="11"/>
<contactref element="J1" pad="10"/>
<contactref element="U1" pad="IN"/>
<contactref element="C1" pad="1"/>
<contactref element="F4" pad="2"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="8"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="23"/>
<contactref element="J1" pad="21"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="22"/>
<contactref element="J1" pad="4"/>
<contactref element="F1" pad="2"/>
<contactref element="F3" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="ADJ"/>
<contactref element="R2" pad="1"/>
<contactref element="VR1" pad="2"/>
</signal>
<signal name="VOUT">
<contactref element="U1" pad="OUT"/>
<contactref element="R2" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="T5" pad="P"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="3V3">
<contactref element="J1" pad="13"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="F2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="16"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R8" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="USB_P4">
<contactref element="X2" pad="1"/>
<contactref element="F3" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="3V3OUT">
<contactref element="T2" pad="P"/>
<contactref element="F2" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="5VOUT">
<contactref element="T1" pad="P"/>
<contactref element="F1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="12VOUT">
<contactref element="T3" pad="P"/>
<contactref element="F4" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$7">
<contactref element="R9" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R5" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="R6" pad="2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="R7" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="DP1">
<contactref element="X1" pad="3"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="DM1">
<contactref element="X1" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="R4" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="-12V">
<contactref element="J1" pad="14"/>
<contactref element="JP1" pad="5"/>
<contactref element="T6" pad="P"/>
</signal>
<signal name="DM2">
<contactref element="U2" pad="4"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="DP2">
<contactref element="U2" pad="3"/>
<contactref element="X2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
