<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="50" width="0" layer="20"/>
<wire x1="50" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<hole x="2" y="47" drill="2"/>
<hole x="48" y="47" drill="2"/>
<hole x="47" y="3" drill="2"/>
<hole x="2" y="2" drill="2"/>
<text>DMJ 2015</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>CH1</text>
<text>CH2</text>
<text>CH3</text>
<text>CH4</text>
<text>PE0</text>
<text>PE1</text>
<text>PE10</text>
<text>PC5</text>
<text>PA10</text>
<text>PB5</text>
<text>PB2</text>
<text>PA5</text>
<text>PC4</text>
<text>PE9</text>
<text>INT1</text>
<text>INT2</text>
<text>INT2</text>
<text>INT1</text>
<text>INT2</text>
<text>INT1</text>
<text>INT1</text>
<text>INT2</text>
<text>RX</text>
<text>RX</text>
<text>RX</text>
<text>RX</text>
<text>TX</text>
<text>TX</text>
<text>TX</text>
<text>TX</text>
<text>SCL</text>
<text>CLK</text>
<text>CLK</text>
<text>CLK</text>
<text>SCL</text>
<text>SDA</text>
<text>SDA</text>
<text>MOSI</text>
<text>MOSI</text>
<text>MISO</text>
<text>MISO</text>
<text>CSS</text>
<text>CSS</text>
<text>TIM14 CH1</text>
<text>R3</text>
<text>R4</text>
<text>R6</text>
<text>G2</text>
<text>R7</text>
<text>R5</text>
<text>G3</text>
<text>G4</text>
<text>G5</text>
<text>G6</text>
<text>G7</text>
<text>B3</text>
<text>B4</text>
<text>B5</text>
<text>B6</text>
<text>B7</text>
<text>DE</text>
<text>VSYNC</text>
<text>HSYNC</text>
<text>CLK</text>
<text>PC0</text>
<text>PC1</text>
<text>PC2</text>
<text>PC3</text>
<text>PD0</text>
<text>PD1</text>
<text>PD4</text>
<text>PD5</text>
<text>PB6</text>
<text>PB7</text>
<text>PC9</text>
<text>PA8</text>
<text>PE4</text>
<text>PA9</text>
<text>PC11</text>
<text>PD6</text>
<text>PC10</text>
<text>PE5</text>
<text>PE6</text>
<text>PE2</text>
<text>PA0</text>
<text>PA1</text>
<text>PD2</text>
<text>PC12</text>
<text>PE9</text>
<text>PE8</text>
<text>GND</text>
<text>PD13</text>
<text>PD14</text>
<text>PD15</text>
<text>PD12</text>
<text>PD8</text>
<text>PD9</text>
<text>PB12</text>
<text>PA7</text>
<text>PE13</text>
<text>PE14</text>
<text>PA4</text>
<text>PC6</text>
<text>B0</text>
<text>A11</text>
<text>A12</text>
<text>B1</text>
<text>E15</text>
<text>A6</text>
<text>E11</text>
<text>B10</text>
<text>B11</text>
<text>C7</text>
<text>D3</text>
<text>D10</text>
<text>E12</text>
<text>A3</text>
<text>B8</text>
<text>B9</text>
</plain>
<libraries>
<library name="STM32F429VI">
<packages>
<package name="LQFP100_PACKAGE">
<description>&lt;b&gt;LQFP100&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08_ROUND">
</package>
<package name="USB-B-MICRO-SMD_V03">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="0-svo">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_TALL">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DMJ">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="06X1-PTH">
<description>6x 0.1in Pin Header Octagon Shape</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="STM32F429VI" package="LQFP100_PACKAGE" value="STM32F42X_43X_LQFP100STM32F429">
<attribute name="NAME"/>
</element>
<element name="JTAG" library="SparkFun-Connectors" package="AVR_ICSP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="adafruit" package="DCJACK_2MM_SMT" value="2.1MMJACKSMT"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K"/>
<element name="U7" library="v-reg" package="SOT223" value="3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Retired" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C15" library="SparkFun-Passives" package="PANASONIC_C" value="10uF"/>
<element name="PWR" library="0-svo" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STS" library="0-svo" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="250"/>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="250"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_TALL" value="RST">
<attribute name="PROD_ID" value="SWCH-11966"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="9.0pF">
<attribute name="PROD_ID" value="CAP-09341"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603-CAP" value="9.0pF">
<attribute name="PROD_ID" value="CAP-09341"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603-CAP" value="15pF">
<attribute name="PROD_ID" value="CAP-07881"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0603-CAP" value="15pF">
<attribute name="PROD_ID" value="CAP-07881"/>
</element>
<element name="C22" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
</element>
<element name="C27" library="SparkFun-Capacitors" package="0603-CAP" value="4.7nF">
<attribute name="PROD_ID" value="CAP-11378"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0603-CAP" value="2.2uF">
<attribute name="PROD_ID" value="CAP-11378"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="DMJ" value="DMJ2"/>
<element name="Y2" library="SparkFun-FreqCtrl" package="DMJ" value="DMJ2"/>
<element name="C16" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C18" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C19" library="SparkFun-Capacitors" package="0603-CAP" value="2.2uF">
<attribute name="PROD_ID" value="CAP-11378"/>
</element>
<element name="LCD" library="SparkFun-Connectors" package="2X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C1" library="GeekAmmo" package="06X1-PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C3" library="GeekAmmo" package="06X1-PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPI3" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPI4" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB" library="SparkFun-Connectors" package="USB-B-MICRO-SMD_V03" value="">
<attribute name="PROD_ID" value="CONN-11752"/>
</element>
<element name="UART4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UART5" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UART7" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TIM4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GIO" library="SparkFun-Connectors" package="AVR_ICSP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USART" library="GeekAmmo" package="06X1-PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="JTAG" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U7" pad="4"/>
<contactref element="C14" pad="A"/>
<contactref element="PWR" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="6"/>
<contactref element="C18" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="50"/>
<contactref element="IC1" pad="75"/>
<contactref element="IC1" pad="100"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="21"/>
<contactref element="I2C1" pad="1"/>
<contactref element="I2C3" pad="1"/>
<contactref element="SPI4" pad="1"/>
<contactref element="SPI3" pad="1"/>
<contactref element="UART4" pad="1"/>
<contactref element="UART7" pad="1"/>
<contactref element="UART5" pad="1"/>
<contactref element="USART" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C15" pad="-"/>
<contactref element="U7" pad="1"/>
<contactref element="C14" pad="C"/>
<contactref element="JTAG" pad="3"/>
<contactref element="JTAG" pad="5"/>
<contactref element="JTAG" pad="9"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="S1" pad="A2"/>
<contactref element="C8" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="IC1" pad="94"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="27"/>
<contactref element="IC1" pad="74"/>
<contactref element="IC1" pad="99"/>
<contactref element="IC1" pad="20"/>
<contactref element="I2C1" pad="2"/>
<contactref element="SPI3" pad="2"/>
<contactref element="SPI4" pad="2"/>
<contactref element="UART5" pad="2"/>
<contactref element="UART7" pad="2"/>
<contactref element="UART4" pad="2"/>
<contactref element="USB" pad="ID1"/>
<contactref element="USB" pad="GND1"/>
<contactref element="USB" pad="SHIELD1"/>
<contactref element="USB" pad="SHIELD2"/>
<contactref element="USB" pad="SHIELD3"/>
<contactref element="I2C3" pad="2"/>
<contactref element="USART" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="PWR2"/>
<contactref element="U7" pad="3"/>
<contactref element="C15" pad="+"/>
</signal>
<signal name="JTCK">
<contactref element="JTAG" pad="4"/>
<contactref element="IC1" pad="76"/>
</signal>
<signal name="JTDI">
<contactref element="JTAG" pad="8"/>
<contactref element="IC1" pad="77"/>
</signal>
<signal name="JTMS">
<contactref element="JTAG" pad="2"/>
<contactref element="IC1" pad="72"/>
</signal>
<signal name="JTRST">
<contactref element="JTAG" pad="7"/>
<contactref element="IC1" pad="90"/>
</signal>
<signal name="JTDO">
<contactref element="JTAG" pad="6"/>
<contactref element="IC1" pad="89"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$11">
<contactref element="C10" pad="1"/>
<contactref element="Y1" pad="P$2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$12">
<contactref element="C12" pad="1"/>
<contactref element="Y1" pad="P$1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$14">
<contactref element="C2" pad="1"/>
<contactref element="Y2" pad="P$2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="C8" pad="1"/>
<contactref element="Y2" pad="P$1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="PWR" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="STS" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="LED_STATUS">
<contactref element="STS" pad="A"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="B2"/>
<contactref element="JTAG" pad="10"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C11" pad="1"/>
<contactref element="IC1" pad="73"/>
</signal>
<signal name="N$6">
<contactref element="C19" pad="1"/>
<contactref element="IC1" pad="49"/>
</signal>
<signal name="LCD_R3">
<contactref element="IC1" pad="35"/>
<contactref element="LCD" pad="1"/>
</signal>
<signal name="LCD_R4">
<contactref element="IC1" pad="70"/>
<contactref element="LCD" pad="2"/>
</signal>
<signal name="LCD_R5">
<contactref element="IC1" pad="71"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="LCD_R6">
<contactref element="IC1" pad="36"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="LCD_R7">
<contactref element="IC1" pad="46"/>
<contactref element="LCD" pad="5"/>
</signal>
<signal name="LCD_G3">
<contactref element="IC1" pad="42"/>
<contactref element="LCD" pad="7"/>
</signal>
<signal name="LCD_G4">
<contactref element="IC1" pad="47"/>
<contactref element="LCD" pad="8"/>
</signal>
<signal name="LCD_G5">
<contactref element="IC1" pad="48"/>
<contactref element="LCD" pad="9"/>
</signal>
<signal name="LCD_G6">
<contactref element="IC1" pad="64"/>
<contactref element="LCD" pad="10"/>
</signal>
<signal name="LCD_G7">
<contactref element="IC1" pad="84"/>
<contactref element="LCD" pad="11"/>
</signal>
<signal name="LCD_B3">
<contactref element="IC1" pad="57"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="LCD_B4">
<contactref element="IC1" pad="43"/>
<contactref element="LCD" pad="13"/>
</signal>
<signal name="LCD_B5">
<contactref element="IC1" pad="26"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="LCD_HSYNC">
<contactref element="IC1" pad="63"/>
<contactref element="LCD" pad="17"/>
</signal>
<signal name="LCD_VSYNC">
<contactref element="IC1" pad="29"/>
<contactref element="LCD" pad="18"/>
</signal>
<signal name="LCD_CLK">
<contactref element="IC1" pad="45"/>
<contactref element="LCD" pad="19"/>
</signal>
<signal name="LCD_DE">
<contactref element="IC1" pad="44"/>
<contactref element="LCD" pad="20"/>
</signal>
<signal name="LCD_G2">
<contactref element="IC1" pad="31"/>
<contactref element="LCD" pad="6"/>
</signal>
<signal name="LCD_B6">
<contactref element="IC1" pad="95"/>
<contactref element="LCD" pad="15"/>
</signal>
<signal name="LCD_B7">
<contactref element="IC1" pad="96"/>
<contactref element="LCD" pad="16"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="IC1" pad="92"/>
<contactref element="I2C1" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="IC1" pad="93"/>
<contactref element="I2C1" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="I2C3_SCL">
<contactref element="IC1" pad="67"/>
<contactref element="I2C3" pad="5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="I2C3_SDA">
<contactref element="IC1" pad="66"/>
<contactref element="I2C3" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="SPI3_MISO">
<contactref element="IC1" pad="79"/>
<contactref element="SPI3" pad="8"/>
</signal>
<signal name="SPI3_MOSI">
<contactref element="IC1" pad="87"/>
<contactref element="SPI3" pad="7"/>
</signal>
<signal name="SPI3_CLK">
<contactref element="IC1" pad="78"/>
<contactref element="SPI3" pad="6"/>
</signal>
<signal name="SPI4_MISO">
<contactref element="IC1" pad="4"/>
<contactref element="SPI4" pad="8"/>
</signal>
<signal name="SPI4_MOSI">
<contactref element="IC1" pad="5"/>
<contactref element="SPI4" pad="7"/>
</signal>
<signal name="SPI4_CLK">
<contactref element="IC1" pad="1"/>
<contactref element="SPI4" pad="6"/>
</signal>
<signal name="SPI4_NSS">
<contactref element="IC1" pad="3"/>
<contactref element="SPI4" pad="5"/>
</signal>
<signal name="TIM4_CH1">
<contactref element="IC1" pad="59"/>
<contactref element="TIM4" pad="1"/>
</signal>
<signal name="TIM4_CH2">
<contactref element="IC1" pad="60"/>
<contactref element="TIM4" pad="2"/>
</signal>
<signal name="TIM4_CH3">
<contactref element="IC1" pad="61"/>
<contactref element="TIM4" pad="3"/>
</signal>
<signal name="TIM4_CH4">
<contactref element="IC1" pad="62"/>
<contactref element="TIM4" pad="4"/>
</signal>
<signal name="TIM14_CH1">
<contactref element="IC1" pad="32"/>
<contactref element="USART" pad="3"/>
</signal>
<signal name="UART4_TX">
<contactref element="IC1" pad="23"/>
<contactref element="UART4" pad="3"/>
</signal>
<signal name="UART4_RX">
<contactref element="IC1" pad="24"/>
<contactref element="UART4" pad="4"/>
</signal>
<signal name="UART5_RX">
<contactref element="IC1" pad="83"/>
<contactref element="UART5" pad="4"/>
</signal>
<signal name="UART5_TX">
<contactref element="IC1" pad="80"/>
<contactref element="UART5" pad="3"/>
</signal>
<signal name="UART7_RX">
<contactref element="IC1" pad="38"/>
<contactref element="UART7" pad="4"/>
</signal>
<signal name="UART7_TX">
<contactref element="IC1" pad="39"/>
<contactref element="UART7" pad="3"/>
</signal>
<signal name="USART3_CK">
<contactref element="IC1" pad="51"/>
<contactref element="USART" pad="4"/>
</signal>
<signal name="USART3_TX">
<contactref element="IC1" pad="55"/>
<contactref element="USART" pad="6"/>
</signal>
<signal name="USART3_RX">
<contactref element="IC1" pad="56"/>
<contactref element="USART" pad="5"/>
</signal>
<signal name="USB_DM">
<contactref element="IC1" pad="53"/>
<contactref element="USB" pad="D-1"/>
</signal>
<signal name="USB_DP">
<contactref element="IC1" pad="54"/>
<contactref element="USB" pad="D+1"/>
</signal>
<signal name="USB_VBUS">
<contactref element="IC1" pad="52"/>
<contactref element="USB" pad="VBUS1"/>
</signal>
<signal name="SPI4_INT1">
<contactref element="SPI4" pad="4"/>
<contactref element="IC1" pad="85"/>
</signal>
<signal name="SPI4_INT2">
<contactref element="SPI4" pad="3"/>
<contactref element="IC1" pad="86"/>
</signal>
<signal name="SPI3_INT2">
<contactref element="SPI3" pad="3"/>
<contactref element="IC1" pad="82"/>
</signal>
<signal name="SPI3_INT1">
<contactref element="SPI3" pad="4"/>
<contactref element="IC1" pad="81"/>
</signal>
<signal name="SPI3_CSS">
<contactref element="SPI3" pad="5"/>
<contactref element="IC1" pad="68"/>
</signal>
<signal name="I2C1_INT1">
<contactref element="I2C1" pad="4"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="I2C1_INT2">
<contactref element="I2C1" pad="3"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="I2C3_INT1">
<contactref element="I2C3" pad="4"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="I2C3_INT2">
<contactref element="I2C3" pad="3"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="IO1">
<contactref element="IC1" pad="97"/>
<contactref element="GIO" pad="1"/>
</signal>
<signal name="IO2">
<contactref element="IC1" pad="98"/>
<contactref element="GIO" pad="2"/>
</signal>
<signal name="IO3">
<contactref element="IC1" pad="40"/>
<contactref element="GIO" pad="3"/>
</signal>
<signal name="IO4">
<contactref element="IC1" pad="41"/>
<contactref element="GIO" pad="4"/>
</signal>
<signal name="IO5">
<contactref element="IC1" pad="33"/>
<contactref element="GIO" pad="5"/>
</signal>
<signal name="IO6">
<contactref element="IC1" pad="34"/>
<contactref element="GIO" pad="6"/>
</signal>
<signal name="IO7">
<contactref element="GIO" pad="7"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="IO8">
<contactref element="IC1" pad="69"/>
<contactref element="GIO" pad="8"/>
</signal>
<signal name="IO9">
<contactref element="IC1" pad="37"/>
<contactref element="GIO" pad="9"/>
</signal>
<signal name="IO10">
<contactref element="IC1" pad="91"/>
<contactref element="GIO" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
