<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.75" x2="0" y2="33.25" width="0.25" layer="20"/>
<wire x1="0" y1="33.25" x2="2.75" y2="36" width="0.25" layer="20" curve="-90"/>
<wire x1="2.75" y1="36" x2="33.25" y2="36" width="0.25" layer="20"/>
<wire x1="33.25" y1="36" x2="36" y2="33.25" width="0.25" layer="20" curve="-90"/>
<wire x1="36" y1="33.25" x2="36" y2="2.75" width="0.25" layer="20"/>
<wire x1="36" y1="2.75" x2="33.25" y2="0" width="0.25" layer="20" curve="-90"/>
<wire x1="33.25" y1="0" x2="2.75" y2="0" width="0.25" layer="20"/>
<wire x1="2.75" y1="0" x2="0" y2="2.75" width="0.25" layer="20" curve="-90"/>
<text>OSD36 RV1
2014-DEC-27
TIM KOSTKA</text>
<text>GND</text>
<text>VCC</text>
<text>VID</text>
<text>AUD</text>
<text>AUD</text>
<text>VID</text>
<text>VCC</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>GRN</text>
<text>+5V</text>
<text>GND</text>
<text>BLK</text>
<text>GND</text>
<text>+5V</text>
<text>CAM</text>
<text>BAT</text>
<text>+5V</text>
<text>TX</text>
<text>TX</text>
<text>RX</text>
<text>VTX</text>
<text>12V</text>
</plain>
<libraries>
<library name="kcl_ics">
<packages>
<package name="SOT23-5">
</package>
<package name="TSSOP28EP">
</package>
<package name="TQFP32">
</package>
<package name="TSSOT-23-6">
</package>
</packages>
</library>
<library name="kcl_passives">
<packages>
<package name="HDR1X04">
</package>
<package name="HDR1X03">
</package>
<package name="HDR1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="HDR1X02">
</package>
<package name="ISP">
</package>
<package name="HDR1X06">
</package>
<package name="C0603R">
<description>Chip capacitor land pattern, reflow soldering, size 0603.</description>
</package>
<package name="C0402R">
<description>Chip capacitor land pattern, reflow soldering, size 0402.</description>
</package>
<package name="AVAGO_LED_0603_C190">
<description>Avago C190/C191 0603 LED</description>
</package>
<package name="MCS0402R">
<description>Vishay MCS 0402 resistor footprint for reflow soldering.</description>
</package>
<package name="MCT0603R">
<description>Vishay MCT 0603 resistor footprint for reflow soldering.</description>
</package>
<package name="BRIDGE">
</package>
<package name="C0805R">
<description>Chip capacitor land pattern, reflow soldering, size 0805.</description>
</package>
<package name="C1210AR">
<description>Chip capacitor land pattern, reflow soldering, size 1210, under 22uF.</description>
</package>
<package name="D0603">
<description>0603 diode package (AVX SOD-523).</description>
</package>
<package name="XRCGB">
<description>Murata crystal.</description>
</package>
<package name="CSTCE*V*C">
<description>Murata Ceralock resonator.</description>
</package>
</packages>
</library>
<library name="kcl_pdb360">
<packages>
<package name="HOLE3MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="kcl_ics" package="SOT23-5" value="TI-INA195">
<attribute name="PN" value="INA195AIDBVR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="kcl_passives" package="HDR1X03" value="HDR1X3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J3" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J4" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J5" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="CUR" library="kcl_passives" package="HDR1X01" value="HDR1X1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VBAT" library="kcl_passives" package="HDR1X02" value="HDR1X2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="kcl_passives" package="HDR1X02" value="HDR1X2">
<attribute name="VALUE"/>
</element>
<element name="U2" library="kcl_ics" package="TSSOP28EP" value="MAX7456">
<attribute name="PN" value="MAX7456EUI+"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CAM" library="kcl_passives" package="HDR1X04" value="HDR1X4HDR1X4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VTX" library="kcl_passives" package="HDR1X04" value="HDR1X4HDR1X4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="kcl_ics" package="TQFP32" value="ATMEGA328P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP" library="kcl_passives" package="ISP" value="ISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI" library="kcl_passives" package="HDR1X06" value="HDR1X6HDR1X6">
<attribute name="VALUE"/>
</element>
<element name="C1" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="kcl_passives" package="AVAGO_LED_0603_C190" value="RED">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="kcl_passives" package="AVAGO_LED_0603_C190" value="BLU">
<attribute name="VALUE"/>
</element>
<element name="R1" library="kcl_passives" package="MCT0603R" value="5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="kcl_passives" package="MCT0603R" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B4" library="kcl_passives" package="BRIDGE" value="+5V">
<attribute name="VALUE"/>
</element>
<element name="B6" library="kcl_passives" package="BRIDGE" value="BAT">
<attribute name="VALUE"/>
</element>
<element name="B7" library="kcl_passives" package="BRIDGE" value="+5V">
<attribute name="VALUE"/>
</element>
<element name="B9" library="kcl_passives" package="BRIDGE" value="BAT">
<attribute name="VALUE"/>
</element>
<element name="U4" library="kcl_ics" package="TSSOT-23-6" value="LM2842">
<attribute name="PN" value="LM2842YMK-ADJL/NOPB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="TMK107ABJ225KA-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="kcl_passives" package="C0603R" value="0.15uF">
<attribute name="PN" value="C0603C154J4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="kcl_passives" package="C0805R" value="47uF">
<attribute name="PN" value="C2012JB1A476M125AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="kcl_passives" package="MCT0603R" value="1.02K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="kcl_passives" package="MCT0603R" value="5.62K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="kcl_passives" package="C1210AR" value="15uH">
<attribute name="PN" value="CBC3225T150KR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="kcl_passives" package="D0603" value="SCHOTTKY0603">
<attribute name="PN" value="SD0603S040S0R2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="kcl_passives" package="AVAGO_LED_0603_C190" value="GREEN">
<attribute name="VALUE"/>
</element>
<element name="R5" library="kcl_passives" package="MCT0603R" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="kcl_passives" package="MCS0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="kcl_passives" package="C0603R" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="kcl_passives" package="C0603R" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="kcl_passives" package="MCS0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="kcl_passives" package="MCS0402R" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="kcl_passives" package="MCS0402R" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="kcl_passives" package="MCS0402R" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TXRX" library="kcl_passives" package="HDR1X02" value="HDR1X2">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="kcl_passives" package="XRCGB" value="27MHz">
<attribute name="PN" value="XRCGB27M000F2P00R0"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="kcl_passives" package="MCS0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y2" library="kcl_passives" package="CSTCE*V*C" value="16MHz">
<attribute name="PN" value="CSTCE16M0V53-R0"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="kcl_passives" package="BRIDGE" value="PAL">
<attribute name="VALUE"/>
</element>
<element name="U5" library="kcl_ics" package="TSSOT-23-6" value="LM2842">
<attribute name="PN" value="LM2842YMK-ADJL/NOPB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="TMK107ABJ225KA-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="kcl_passives" package="C0603R" value="0.15uF">
<attribute name="PN" value="C0603C154J4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="kcl_passives" package="C0805R" value="47uF">
<attribute name="PN" value="C2012JB1A476M125AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="kcl_passives" package="MCT0603R" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="kcl_passives" package="MCT0603R" value="14.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="kcl_passives" package="C1210AR" value="15uH">
<attribute name="PN" value="CBC3225T150KR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="kcl_passives" package="D0603" value="SCHOTTKY0603">
<attribute name="PN" value="SD0603S040S0R2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="kcl_passives" package="AVAGO_LED_0603_C190" value="GREEN">
<attribute name="VALUE"/>
</element>
<element name="R14" library="kcl_passives" package="MCT0603R" value="5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B2" library="kcl_passives" package="BRIDGE" value="12V">
<attribute name="VALUE"/>
</element>
<element name="B3" library="kcl_passives" package="BRIDGE" value="12V">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="VBAT" pad="1"/>
<contactref element="+5V" pad="1"/>
<contactref element="CAM" pad="1"/>
<contactref element="VTX" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="21"/>
<contactref element="ISP" pad="GND"/>
<contactref element="FTDI" pad="6"/>
<contactref element="FTDI" pad="5"/>
<contactref element="U2" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="20"/>
<contactref element="U2" pad="23"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="U2" pad="PAD"/>
<contactref element="C3" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="LED3" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="Y2" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="5"/>
<contactref element="+5V" pad="2"/>
<contactref element="ISP" pad="VCC"/>
<contactref element="FTDI" pad="4"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="24"/>
<contactref element="U2" pad="21"/>
<contactref element="C2" pad="1"/>
<contactref element="B4" pad="1"/>
<contactref element="B7" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="18"/>
<contactref element="R11" pad="2"/>
<contactref element="B1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="1"/>
<contactref element="CUR" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="VBAT" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="3"/>
<contactref element="B6" pad="1"/>
<contactref element="B9" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="U4" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="5"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="VID_IN">
<contactref element="CAM" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="CAM_VCC">
<contactref element="CAM" pad="2"/>
<contactref element="B7" pad="2"/>
<contactref element="B9" pad="2"/>
<contactref element="B2" pad="2"/>
</signal>
<signal name="VID_OUT">
<contactref element="VTX" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="VTX_VCC">
<contactref element="VTX" pad="2"/>
<contactref element="B4" pad="2"/>
<contactref element="B6" pad="2"/>
<contactref element="B3" pad="2"/>
</signal>
<signal name="AUDIO">
<contactref element="CAM" pad="4"/>
<contactref element="VTX" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U3" pad="15"/>
<contactref element="ISP" pad="MOSI"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="U3" pad="16"/>
<contactref element="ISP" pad="MISO"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="SCK">
<contactref element="U3" pad="17"/>
<contactref element="ISP" pad="SCK"/>
<contactref element="U2" pad="10"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="ISP" pad="!RESET!"/>
<contactref element="U3" pad="29"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="19"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="FTDI" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="RXI">
<contactref element="FTDI" pad="3"/>
<contactref element="U3" pad="30"/>
<contactref element="TXRX" pad="2"/>
</signal>
<signal name="TXO">
<contactref element="FTDI" pad="2"/>
<contactref element="U3" pad="31"/>
<contactref element="TXRX" pad="1"/>
</signal>
<signal name="VSYNC">
<contactref element="U3" pad="32"/>
<contactref element="U2" pad="17"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="HSYNC">
<contactref element="U2" pad="18"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="LOS">
<contactref element="U2" pad="12"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SSOSD-IN">
<contactref element="U2" pad="8"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="CLKOUT">
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U4" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C4" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="U4" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="U4" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="22"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="26"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="25"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="6"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="5"/>
<contactref element="Y1" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="20"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="B1" pad="1"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="Y2" pad="3"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="8"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U5" pad="1"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="C12" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="U5" pad="6"/>
<contactref element="R13" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$21">
<contactref element="U5" pad="3"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="L2" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="B3" pad="1"/>
<contactref element="B2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R14" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
