<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.42" y2="0" width="0" layer="20"/>
<wire x1="58.42" y1="0" x2="58.42" y2="46.355" width="0" layer="20"/>
<wire x1="36.83" y1="48.26" x2="38.735" y2="46.355" width="0" layer="20" curve="90"/>
<wire x1="38.735" y1="46.355" x2="58.42" y2="46.355" width="0" layer="20"/>
<wire x1="0" y1="46.355" x2="19.685" y2="46.355" width="0" layer="20"/>
<wire x1="19.685" y1="46.355" x2="21.59" y2="48.26" width="0" layer="20" curve="90"/>
<wire x1="0" y1="46.355" x2="0" y2="0" width="0" layer="20"/>
<wire x1="21.59" y1="48.26" x2="21.59" y2="52.07" width="0" layer="20"/>
<wire x1="21.59" y1="52.07" x2="36.83" y2="52.07" width="0" layer="20"/>
<wire x1="36.83" y1="52.07" x2="36.83" y2="48.26" width="0" layer="20"/>
<hole x="19.05" y="43.18" drill="3.302"/>
<text>(C) 2014</text>
<text>(512)æ</text>
<text>Inamorata</text>
</plain>
<libraries>
<library name="mm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mm-trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="mm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/4">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 4 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="mm-caps-ceramic">
<description>&lt;b&gt;Capacitors, Ceramic&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;very small capacitances: 1 - 1000pF
&lt;/ul&gt;</description>
<packages>
<package name="050X030_025_2">
<description>&lt;b&gt;5mm x 3mm, 0.2" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mm_pots">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;chassis-mount (e.g., Alpha 16mm) pots&lt;/li&gt;
&lt;li&gt;board-mount trim pots (1/4" and 3/8")&lt;/li&gt;
&lt;li&gt; all pot values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="16MM_PCB_PADS">
</package>
</packages>
</library>
<library name="mm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO35-4">
<description>&lt;B&gt;DO-35 0.4" spacing&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="mm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="ROUND">
<description>&lt;b&gt;Round Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="mm_jacks_alt">
<description>PCB MOUNTED JACK</description>
<packages>
<package name="BATTERY">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="mm-ics" package="DIL08" value="TL072">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="mm-trans" package="TO92-" value="2N5089">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="mm-trans" package="TO92-" value="2N5089">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="mm-resistors" package="R0207/4" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="mm-resistors" package="R0207/4" value="470k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="mm-resistors" package="R0207/4" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="mm-resistors" package="R0207/4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GAIN" library="mm_pots" package="16MM_PCB_PADS" value="100kA">
<attribute name="NAME"/>
</element>
<element name="TONE" library="mm_pots" package="16MM_PCB_PADS" value="100kB">
<attribute name="NAME"/>
</element>
<element name="MIDS" library="mm_pots" package="16MM_PCB_PADS" value="100kC">
<attribute name="NAME"/>
</element>
<element name="C2" library="mm-caps-ceramic" package="050X030_025_2" value="15n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="mm-caps-ceramic" package="050X030_025_2" value="2µ2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TIGHT" library="mm_pots" package="16MM_PCB_PADS" value="50kC">
<attribute name="NAME"/>
</element>
<element name="C5" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="mm-resistors" package="R0207/4" value="330Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="mm-resistors" package="R0207/4" value="470k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="mm-caps-ceramic" package="050X030_025_2" value="470p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="mm-diodes" package="DO35-4" value="1N914">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="mm-diodes" package="DO35-4" value="1N914">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="mm-resistors" package="R0207/4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="mm-resistors" package="R0207/4" value="330Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="mm-resistors" package="R0207/4" value="470k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="mm-caps-ceramic" package="050X030_025_2" value="470p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="mm-diodes" package="DO35-4" value="1N914">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="mm-diodes" package="DO35-4" value="1N914">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="mm-resistors" package="R0207/4" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VOL" library="mm_pots" package="16MM_PCB_PADS" value="1MA">
<attribute name="NAME"/>
</element>
<element name="C13" library="mm-caps-ceramic" package="050X030_025_2" value="4n7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="mm-caps-ceramic" package="050X030_025_2" value="47n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="mm-caps-ceramic" package="050X030_025_2" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="mm-resistors" package="R0207/4" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="mm-resistors" package="R0207/4" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="mm-resistors" package="R0207/4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="mm-caps-ceramic" package="050X030_025_2" value="2µ2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="mm-resistors" package="R0207/4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="mm-resistors" package="R0207/4" value="560Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="mm-diodes" package="DO35-4" value="BAT46">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="mm-resistors" package="R0207/4" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="mm-caps-electro-pol" package="063_025" value="47µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="mm-caps-electro-pol" package="063_025" value="47µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="2" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="4" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="5" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="6" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="3" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="U$1" library="mm_jacks_alt" package="BATTERY" value="BATTERY"/>
<element name="IT" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="IR" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="IS" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="VS" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="VR" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="VT" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="OT" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="OS" library="mm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="R5" library="mm-resistors" package="R0207/4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="mm-caps-ceramic" package="050X030_025_2" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="mm-caps-ceramic" package="050X030_025_2" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="mm-resistors" package="R0207/4" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VR">
<contactref element="IC1" pad="5"/>
<contactref element="R3" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="C19" pad="+"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="GD">
<contactref element="R9" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="D2">
<contactref element="R10" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
<contactref element="R11" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="D1" pad="A"/>
<contactref element="C9" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$15">
<contactref element="C10" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R13" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R14" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="R15" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="R16" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="D3" pad="A"/>
<contactref element="C11" pad="2"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$24">
<contactref element="R17" pad="2"/>
<contactref element="TONE" pad="1"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="C16" pad="1"/>
<contactref element="TONE" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="C16" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="VOL" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$28">
<contactref element="VOL" pad="3"/>
<contactref element="IC1" pad="7"/>
<contactref element="VOL" pad="2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="C17" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="D5" pad="A"/>
<contactref element="VS" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R21" pad="2"/>
<contactref element="4" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="1" pad="1"/>
<contactref element="IT" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="U$1" pad="P$1"/>
<contactref element="VR" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="C18" pad="-"/>
<contactref element="R24" pad="1"/>
<contactref element="C19" pad="-"/>
<contactref element="3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="IS" pad="1"/>
<contactref element="VT" pad="1"/>
<contactref element="OS" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D5" pad="C"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="P$2"/>
<contactref element="IR" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="5" pad="1"/>
<contactref element="OT" pad="1"/>
</signal>
<signal name="R11">
<contactref element="C18" pad="+"/>
<contactref element="IC1" pad="8"/>
<contactref element="R23" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="6" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="C13" pad="2"/>
<contactref element="TONE" pad="3"/>
<contactref element="MIDS" pad="2"/>
<contactref element="MIDS" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="MIDS" pad="3"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C3" pad="1"/>
<contactref element="TIGHT" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="TIGHT" pad="2"/>
<contactref element="TIGHT" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="ADAS">
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="GAIN" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="GAIN" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R6" pad="2"/>
<contactref element="GAIN" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R7" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
