<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="82.22" y2="0" width="0" layer="20"/>
<wire x1="82.22" y1="0" x2="82.22" y2="50.79" width="0" layer="20"/>
<wire x1="82.22" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<text>POS</text>
<text>NEG</text>
<text>REV REL</text>
<text>11-8-14</text>
<text>VAWT</text>
<text>CONTROLLER</text>
<text>LM2596</text>
<text>BASED</text>
<text>Q1</text>
</plain>
<libraries>
<library name="caleb-ic">
<packages>
<package name="TO92">
</package>
<package name="TO225">
</package>
<package name="SOT23">
</package>
<package name="D2PAK5">
</package>
<package name="DO-41">
</package>
<package name="SOIC-8">
</package>
<package name="DO35-250">
</package>
<package name="DO-214AB">
</package>
<package name="SOT223-NXP">
</package>
<package name="DO35-5">
</package>
<package name="SOT25">
</package>
</packages>
</library>
<library name="caleb-ic-attiny85-ucontroller">
<packages>
<package name="ATTINY85-UCONTROLLER-DIP8">
</package>
</packages>
</library>
<library name="caleb-passive">
<packages>
<package name="R1206">
</package>
<package name="PJ125">
</package>
<package name="KY10X5">
</package>
<package name="R0805">
</package>
<package name="L1210">
</package>
</packages>
</library>
<library name="caleb-con-OST-termblock">
<packages>
<package name="3POS200">
</package>
<package name="EDZ350-2POS">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_8X150_NOTEXT">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="caleb-ic" package="TO92" value="78L05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="caleb-ic" package="TO225" value="MCR106">
<attribute name="VALUE"/>
</element>
<element name="U5" library="caleb-ic-attiny85-ucontroller" package="ATTINY85-UCONTROLLER-DIP8" value="ATTINY85-UCONTROLLER-DIP8">
<attribute name="NAME"/>
</element>
<element name="J1" library="caleb-con-OST-termblock" package="3POS200" value="CON-OST-3POS-0200SPACING"/>
<element name="J2" library="caleb-con-OST-termblock" package="EDZ350-2POS" value="CON-EDZ350-2"/>
<element name="U4" library="caleb-ic" package="SOT23" value="APX809">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="caleb-passive" package="R1206" value="7A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="ohw-logo" package="OSHW_8X150_NOTEXT" value="OSHW_LOGO_8MILX0150-NT"/>
<element name="U2" library="caleb-ic" package="D2PAK5" value="LM2596">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="caleb-passive" package="R1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="caleb-passive" package="R1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="caleb-passive" package="R1206" value="0.04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor" package="TO92" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="caleb-passive" package="PJ125" value="560uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="caleb-passive" package="KY10X5" value="220uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="caleb-passive" package="KY10X5" value="220uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="caleb-ic" package="SOIC-8" value="LM358">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="caleb-passive" package="R0805" value="2200pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="caleb-passive" package="R0805" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="caleb-passive" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="caleb-passive" package="R0805" value="523">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="caleb-ic" package="DO35-250" value="36V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="caleb-passive" package="R0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="caleb-passive" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="caleb-passive" package="R0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="caleb-passive" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="caleb-passive" package="L1210" value="68uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="caleb-passive" package="R0805" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="caleb-passive" package="R0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="caleb-passive" package="R0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="caleb-passive" package="R0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="caleb-passive" package="R0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="caleb-passive" package="R0805" value="3.32k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="caleb-passive" package="R0805" value="34.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="caleb-ic" package="DO-214AB" value="STPS5L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="caleb-ic" package="DO-41" value="STPS2L60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="caleb-ic" package="SOT223-NXP" value="PMT21EN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="caleb-passive" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="caleb-ic" package="DO35-5" value="10V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="caleb-passive" package="R0805" value="2200pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="caleb-passive" package="R0805" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="caleb-ic" package="SOT25" value="ZXCT1084">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="caleb-passive" package="R0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U5" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="Q1" pad="C"/>
<contactref element="U4" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="C5" pad="NEG"/>
<contactref element="C1" pad="NEG"/>
<contactref element="C2" pad="NEG"/>
<contactref element="D5" pad="A"/>
<contactref element="U6" pad="4"/>
<contactref element="R15" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="C10" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="D12" pad="A"/>
<contactref element="C6" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="J2" pad="P$2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="L1">
<contactref element="J1" pad="P$1"/>
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="P$2"/>
<contactref element="D3" pad="K"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="P$3"/>
<contactref element="D5" pad="K"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="VRECT">
<contactref element="D2" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="D6" pad="K"/>
<contactref element="D11" pad="C"/>
<contactref element="Q1" pad="A"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="5V">
<contactref element="U5" pad="8"/>
<contactref element="U1" pad="1"/>
<contactref element="U4" pad="3"/>
<contactref element="U6" pad="8"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="SWE">
<contactref element="U2" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="D12" pad="C"/>
</signal>
<signal name="FB">
<contactref element="U2" pad="4"/>
<contactref element="C18" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="D7" pad="K"/>
</signal>
<signal name="VLO">
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="POS"/>
<contactref element="L1" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="D10" pad="A"/>
<contactref element="U1" pad="3"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U5" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="VOUT">
<contactref element="F1" pad="1"/>
<contactref element="Q3" pad="P$1"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="F1" pad="2"/>
<contactref element="J2" pad="P$1"/>
</signal>
<signal name="PWM">
<contactref element="U5" pad="6"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$10">
</signal>
<signal name="N$9">
<contactref element="Q2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="NSNS">
<contactref element="Q2" pad="1"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R4" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="EN">
<contactref element="U5" pad="5"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="G"/>
<contactref element="D11" pad="A"/>
<contactref element="C10" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="VHI">
<contactref element="U2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="D10" pad="C"/>
<contactref element="R12" pad="1"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="REF">
<contactref element="U6" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R2" pad="1"/>
<contactref element="U6" pad="6"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U6" pad="7"/>
<contactref element="D7" pad="A"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U6" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="ISNS">
<contactref element="R1" pad="1"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="R10" pad="1"/>
<contactref element="D8" pad="K"/>
<contactref element="C1" pad="POS"/>
<contactref element="C2" pad="POS"/>
<contactref element="U3" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
